# ZX-Spectrum-BDI-TR-DOS-interface
Open-source Beta Disk Interface (TR-DOS) for ZX Spectrum 48K/128K. Powered strictly by +5V using Fujitsu MB8877A FDC. No +12V required! Available in classic sandwich and compact single-board versions.
