<!--This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International License (CC BY-SA) with Design Exception 1.0-->
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="MODULE_ABX00028">
</package>
</packages>
<symbols>
<symbol name="ABX00028">
<pin name="D13"/>
<pin name="+3V3" direction="pwr"/>
<pin name="AREF"/>
<pin name="A0/DAC0"/>
<pin name="+5V" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4/SDA"/>
<pin name="A5/SCL"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="D2"/>
<pin name="D3/PWM"/>
<pin name="D4"/>
<pin name="D5/PWM"/>
<pin name="D6/PWM"/>
<pin name="D8"/>
<pin name="D7"/>
<pin name="D9/PWM"/>
<pin name="D10/PWM"/>
<pin name="D11/MOSI"/>
<pin name="D12/MISO"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ABX00028" prefix="U">
<description>ATmega4809 Arduino Nano Every AVR AVR MCU 8-Bit Embedded Evaluation Board   &lt;a href="https://pricing.snapeda.com/parts/Arduino%20Nano%20Every/Arduino/view-part?ref=eda"&gt;Check availability&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ABX00028"/>
</gates>
<devices>
<device name="" package="MODULE_ABX00028">
<connects>
<connect gate="G$1" pin="!RESET" pad="13 18"/>
<connect gate="G$1" pin="+3V3" pad="2"/>
<connect gate="G$1" pin="+5V" pad="12"/>
<connect gate="G$1" pin="A0/DAC0" pad="4"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4/SDA" pad="8"/>
<connect gate="G$1" pin="A5/SCL" pad="9"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="11"/>
<connect gate="G$1" pin="AREF" pad="3"/>
<connect gate="G$1" pin="D10/PWM" pad="28"/>
<connect gate="G$1" pin="D11/MOSI" pad="29"/>
<connect gate="G$1" pin="D12/MISO" pad="30"/>
<connect gate="G$1" pin="D13" pad="1"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3/PWM" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5/PWM" pad="23"/>
<connect gate="G$1" pin="D6/PWM" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="D8" pad="26"/>
<connect gate="G$1" pin="D9/PWM" pad="27"/>
<connect gate="G$1" pin="GND" pad="14 19"/>
<connect gate="G$1" pin="RX" pad="17"/>
<connect gate="G$1" pin="TX" pad="16"/>
<connect gate="G$1" pin="VIN" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="Availability" value="In Stock"/>
<attribute name="Price" value="None"/>
<attribute name="MP" value="Arduino Nano Every"/>
<attribute name="Package" value="None"/>
<attribute name="Description" value="
Arduino’s 5V compatible board in the smallest available form factor: 45x18mm!
"/>
<attribute name="Purchase-URL" value="https://pricing.snapeda.com/search/part/Arduino Nano Every/?ref=eda"/>
<attribute name="MF" value="Arduino"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
