<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.96" y2="0" width="0.1524" layer="20"/>
<wire x1="60.96" y1="0" x2="60.96" y2="38.1" width="0.1524" layer="20"/>
<wire x1="60.96" y1="38.1" x2="99.06" y2="38.1" width="0.1524" layer="20"/>
<wire x1="99.06" y1="38.1" x2="99.06" y2="63.5" width="0.1524" layer="20"/>
<wire x1="99.06" y1="63.5" x2="27.94" y2="63.5" width="0.1524" layer="20"/>
<text>Gigatron Video Repeater Rev.3</text>
<wire x1="0" y1="43.18" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="43.18" x2="27.94" y2="43.18" width="0.1524" layer="20"/>
<wire x1="27.94" y1="43.18" x2="27.94" y2="63.5" width="0.1524" layer="20"/>
<text>all</text>
<text>3 from 4</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B2.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 2.5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74ttl-din">
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="memory-idt">
<description>&lt;b&gt;IDT Memories&lt;/b&gt;&lt;p&gt;
Integrated Device Technology, Inc.&lt;p&gt;
http://www.idt.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="C2" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="C3" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="C4" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="C5" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="C6" library="capacitor-wima" package="C5B2.5" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="10"/>
</element>
<element name="U6" library="memory-idt" package="DIL28-3" value="IDT7204L-15">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X03" value="videolines">
<attribute name="POPULARITY" value="92"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="74ttl-din" package="DIL14" value="74113N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="74ttl-din" package="DIL14" value="74113N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="ADAPTER" library="74ttl-din" package="DIL20" value="Adapter74377N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="74ttl-din" package="DIL20" value="74574N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="74ttl-din" package="DIL14" value="74LS00N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="74ttl-din" package="DIL20" value="74377N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U5" pad="14"/>
<contactref element="U4" pad="14"/>
<contactref element="ADAPTER" pad="20"/>
<contactref element="U2" pad="20"/>
<contactref element="U6" pad="28"/>
<contactref element="U3" pad="14"/>
<contactref element="U1" pad="20"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U5" pad="12"/>
</signal>
<signal name="GND">
<contactref element="U5" pad="7"/>
<contactref element="U4" pad="7"/>
<contactref element="ADAPTER" pad="10"/>
<contactref element="U2" pad="10"/>
<contactref element="U6" pad="14"/>
<contactref element="U3" pad="7"/>
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="9"/>
<contactref element="JP1" pad="3"/>
<contactref element="U5" pad="3"/>
<contactref element="U6" pad="25"/>
<contactref element="U6" pad="24"/>
<contactref element="U6" pad="2"/>
<contactref element="U6" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U5" pad="11"/>
</signal>
<signal name="D7">
<contactref element="ADAPTER" pad="18"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="D6">
<contactref element="ADAPTER" pad="17"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="D5">
<contactref element="ADAPTER" pad="14"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="D0">
<contactref element="ADAPTER" pad="3"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D1">
<contactref element="ADAPTER" pad="4"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="D2">
<contactref element="ADAPTER" pad="7"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="D3">
<contactref element="ADAPTER" pad="8"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="D4">
<contactref element="ADAPTER" pad="13"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="RL">
<contactref element="U1" pad="2"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="RH">
<contactref element="U1" pad="5"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="GL">
<contactref element="U1" pad="6"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="GH">
<contactref element="U1" pad="9"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="BL">
<contactref element="U1" pad="12"/>
<contactref element="U6" pad="27"/>
</signal>
<signal name="BH">
<contactref element="U1" pad="15"/>
<contactref element="U6" pad="26"/>
</signal>
<signal name="F0">
<contactref element="U6" pad="9"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="F1">
<contactref element="U6" pad="10"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="F2">
<contactref element="U6" pad="11"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="F3">
<contactref element="U6" pad="12"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="F4">
<contactref element="U6" pad="16"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="F5">
<contactref element="U6" pad="17"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="/HSYNC">
<contactref element="U1" pad="16"/>
<contactref element="U6" pad="23"/>
<contactref element="ADAPTER" pad="16"/>
<contactref element="U4" pad="13"/>
<contactref element="U4" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="13"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="U3" pad="3"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="CLK377">
<contactref element="U1" pad="11"/>
<contactref element="ADAPTER" pad="11"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U6" pad="15"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="/E377">
<contactref element="ADAPTER" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="Q0">
<contactref element="ADAPTER" pad="2"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="Q1">
<contactref element="ADAPTER" pad="5"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="Q2">
<contactref element="ADAPTER" pad="6"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="Q3">
<contactref element="ADAPTER" pad="9"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="Q4">
<contactref element="ADAPTER" pad="12"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="Q5">
<contactref element="ADAPTER" pad="15"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="/VSYNC">
<contactref element="ADAPTER" pad="19"/>
<contactref element="U1" pad="19"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="5"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="U4" pad="6"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="U4" pad="9"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="N$6">
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="6"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="11"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="U5" pad="6"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="1"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U6" pad="22"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
