(module SOIC-8_3.9x4.9mm_Pitch1.27mm_Handsoldering (layer F.Cu) (tedit 56951424)
  (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "SOIC 1.27")
  (attr smd)
  (fp_text reference REF** (at 0 -3.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SOIC-8_3.9x4.9mm_Pitch1.27mm (at 0 3.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -1.2319 -1.86944) (end -0.94234 -1.6256) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.75 -2.75) (end -3.75 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.75 -2.75) (end 3.75 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 -2.75) (end 3.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.75 2.75) (end 3.75 2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.075 -2.575) (end -2.075 -2.43) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.075 -2.575) (end 2.075 -2.43) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.075 2.575) (end 2.075 2.43) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.075 2.575) (end -2.075 2.43) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.075 -2.575) (end 2.075 -2.575) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.075 2.575) (end 2.075 2.575) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.075 -2.43) (end -3.475 -2.43) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -3.1 -1.905) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.1 -0.635) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.1 0.635) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -3.1 1.905) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.1 1.905) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.1 0.635) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 3.1 -0.635) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 3.1 -1.905) (size 2.35 0.6) (layers F.Cu F.Paste F.Mask))
  (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
