(module SW_PUSH-SKHCBFA010 (layer F.Cu) (tedit 56950D65)
  (fp_text reference REF** (at 0 -0.762) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SW_PUSH-12mm (at 0 1.016) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 3.81 2.54) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -6) (end 6 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 -6) (end 6 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 6) (end -6 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 6) (end -6 -6) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 6.25 -2.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 6.25 2.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -6.25 -2.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -6.25 2.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad "" thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad "" thru_hole circle (at 0 -4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH-12mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 4 4 4))
    (rotate (xyz 0 0 0))
  )
)
