(module LED-0603 (layer F.Cu) (tedit 5FEA3C9B)
  (descr "LED 0603 smd package")
  (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
  (attr smd)
  (fp_text reference REF** (at 0 -1.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value LED-0603 (at 0 1.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.4 -0.75) (end 1.4 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.4 0.75) (end -1.4 -0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.4 0.75) (end -1.4 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.4 -0.75) (end 1.4 0.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.1 -0.6262) (end 0.8 -0.6262) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.1 0.6262) (end 0.8 0.6262) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.0955 -0.00762) (end -1.36398 -0.00762) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.3589 -0.00762) (end 2.09042 -0.00762) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.72212 0.36322) (end 1.72212 -0.3683) (layer F.SilkS) (width 0.15))
  (pad 2 smd rect (at 0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.7493 0 180) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask))
)
