(module SOD-323_Handsoldering (layer F.Cu) (tedit 55F1B69A)
  (descr SOD-323)
  (tags SOD-323)
  (attr smd)
  (fp_text reference REF** (at 0 -1.85) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SOD-323_Handsoldering (at 0.1 1.9) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.25 0) (end 0.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0) (end -0.5 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 0) (end 0.25 -0.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 -0.35) (end 0.25 0.35) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.25 0.35) (end -0.25 0) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.25 -0.35) (end -0.25 0.35) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -0.95) (end 1.5 -0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.5 -0.95) (end 1.5 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 0.95) (end 1.5 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -0.95) (end -1.5 0.95) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.3 0.8) (end 1.1 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3 -0.8) (end 1.1 -0.8) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.4 0) (size 1.4 0.45) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.4 0) (size 1.4 0.45) (layers F.Cu F.Paste F.Mask))
)
