(module PCIexpress_x16 (layer F.Cu) (tedit 5D338A18)
  (descr "PCIexpress x16 footprint")
  (tags PCIexpress)
  (attr virtual)
  (fp_text reference REF** (at 0 -19.75) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BUS_PCIexpress_x16 (at 0 -23) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 261.77 -106.13) (end 263.37 -106.13) (layer Dwgs.User) (width 0.12))
  (fp_circle (center 261.77 -16.6) (end 263.37 -16.6) (layer Dwgs.User) (width 0.12))
  (fp_line (start 261.77 -99.7) (end 261.77 -22.9) (layer Dwgs.User) (width 0.12))
  (fp_line (start 256.65 -99.7) (end 261.77 -99.7) (layer Dwgs.User) (width 0.12))
  (fp_line (start 256.65 -22.9) (end 261.77 -22.9) (layer Dwgs.User) (width 0.12))
  (fp_line (start 256.65 -13.75) (end 256.65 -22.9) (layer Dwgs.User) (width 0.12))
  (fp_line (start 122.5 -13.75) (end 256.65 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start 256.65 -108.15) (end 256.65 -99.7) (layer Dwgs.User) (width 0.12))
  (fp_line (start 122.5 -108.15) (end 256.65 -108.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start 107.5 -15) (end 108 -14.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 107.5 -15) (end 107 -14.5) (layer Cmts.User) (width 0.12))
  (fp_line (start 107.5 -10) (end 107.5 -15) (layer Cmts.User) (width 0.12))
  (fp_text user "Keep out components and traces component side" (at 126 -9 180) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 110.3 -16.1) (end 110.3 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start 105.05 -16.1) (end 110.3 -16.1) (layer Dwgs.User) (width 0.12))
  (fp_line (start 105.05 -14.1) (end 105.05 -16.1) (layer Dwgs.User) (width 0.12))
  (fp_line (start 96.9 -14.1) (end 105.05 -14.1) (layer Dwgs.User) (width 0.12))
  (fp_line (start 96.9 -14.1) (end 96.9 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_text user "Max component height: solder side 2,67mm component side 14,49mm" (at 40 -44.25) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_text user "Keep out components and traces solder side" (at -42.25 -77.5 180) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -40.07 -13.75) (end -40.07 -89.7) (layer Dwgs.User) (width 0.12))
  (fp_text user "Keep out components and traces both sides" (at 120 -87.75 90) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 117.42 -108.15) (end 117.42 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -32.45 -110.15) (end -32.45 -89.7) (layer Dwgs.User) (width 0.12))
  (fp_line (start -45.15 -89.7) (end -32.45 -89.7) (layer Dwgs.User) (width 0.12))
  (fp_line (start -32.45 -67.9) (end 121.5 -67.9) (layer Dwgs.User) (width 0.12))
  (fp_text user "Keep out components and traces both sides" (at 121.893243 -40.134926 90) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Keep out components and traces solder side" (at -44.75 -36 90) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -44.15 -58.5) (end -44.15 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start 121.5 -67.9) (end 121.5 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start 92 -108.15) (end 117.42 -108.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start 92 -110.15) (end 92 -108.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start 84.15 -13.75) (end 121.5 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -32.45 -110.15) (end 92 -110.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start -32.45 -58.5) (end -32.45 -67.9) (layer Dwgs.User) (width 0.12))
  (fp_line (start -45.15 -58.5) (end -32.45 -58.5) (layer Dwgs.User) (width 0.12))
  (fp_text user "Keep out components and traces both sides" (at -21.75 -12) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 84.15 -12.75) (end 84.15 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.15 -13.75) (end -45.15 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.15 -10.925) (end -0.15 -13.75) (layer Dwgs.User) (width 0.12))
  (fp_text user "Full length max" (at 269 -74 90) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_line (start 266.85 -111.15) (end 266.8527 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start 122.5 -111.15) (end 266.85 -111.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start 122.5027 -12.75) (end 266.8527 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_circle (center -37.65 -94.75) (end -36.05 -94.75) (layer Dwgs.User) (width 0.12))
  (fp_circle (center -37.65 -63.25) (end -36.05 -63.25) (layer Dwgs.User) (width 0.12))
  (fp_poly (pts (xy -11.8 -4.5) (xy -11.8 -8) (xy -3.8 -8) (xy -3.8 -4.5)) (layer B.Mask) (width 0))
  (fp_poly (pts (xy -11.8 -4.5) (xy -11.8 -8) (xy -3.8 -8) (xy -3.8 -4.5)) (layer F.Mask) (width 0))
  (fp_text user "Keep Out Cu" (at -7.75 -3.5) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -11.8 -8) (end -3.8 -8) (layer Dwgs.User) (width 0.12))
  (fp_circle (center -37.65 -9.35) (end -36.05 -9.35) (layer Dwgs.User) (width 0.12))
  (fp_text user "Half length max" (at 124.5 -72.25 90) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_text user "Full height max" (at 36.75 -108.25) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_text user "Low profile max height" (at 39.25 -71) (layer Cmts.User)
    (effects (font (size 2 2) (thickness 0.25)))
  )
  (fp_line (start -45.15 -68.9) (end 122.5 -68.9) (layer Dwgs.User) (width 0.12))
  (fp_line (start -45.15 -111.15) (end -45.15 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 122.5 -111.15) (end 122.5 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -45.15 -111.15) (end 122.5 -111.15) (layer Dwgs.User) (width 0.12))
  (fp_line (start 84.15 -12.75) (end 122.5027 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -30.15 -4.5) (end -45.15 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start -30.15 -4.5) (end -30.15 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -30.15 -12.75) (end -11.8 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -11.8 -4.5) (end -11.8 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -3.8 -4.5) (end -3.8 -10.925) (layer Dwgs.User) (width 0.12))
  (fp_line (start -11.8 -4.5) (end -3.8 -4.5) (layer Dwgs.User) (width 0.12))
  (fp_arc (start -1.975 -10.925) (end -0.15 -10.925) (angle -180) (layer Dwgs.User) (width 0.12))
  (fp_poly (pts (xy -0.25 -5.5) (xy 84.25 -5.5) (xy 84.25 0) (xy -0.25 0)) (layer B.Mask) (width 0.2))
  (fp_poly (pts (xy -0.25 -5.5) (xy 84.25 -5.5) (xy 84.25 0) (xy -0.25 0)) (layer F.Mask) (width 0.2))
  (fp_line (start 84.15 -0.5) (end 83.65 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.15 -0.5) (end 0.35 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start 84.15 -0.5) (end 84.15 -12.75) (layer Dwgs.User) (width 0.12))
  (fp_line (start -0.15 -0.5) (end -0.15 -10.925) (layer Dwgs.User) (width 0.12))
  (fp_line (start 13.45 0) (end 83.65 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start 12.95 -0.5) (end 13.45 0) (layer Dwgs.User) (width 0.12))
  (fp_line (start 11.05 -0.5) (end 10.55 0) (layer Dwgs.User) (width 0.12))
  (fp_arc (start 12 -7.45) (end 11.05 -7.45) (angle 180) (layer Dwgs.User) (width 0.12))
  (fp_line (start 12.95 -7.45) (end 12.95 -0.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 11.05 -7.45) (end 11.05 -0.5) (layer Dwgs.User) (width 0.12))
  (fp_line (start 0.35 0) (end 10.55 0) (layer Dwgs.User) (width 0.12))
  (fp_text user %R (at 0 -17.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Keep out components and traces both sides" (at 264.25 -65.25 90) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 87.4 -2.95) (end 98.2 -2.95) (layer Dwgs.User) (width 0.12))
  (fp_line (start 86.9 -3.45) (end 86.9 -7.95) (layer Dwgs.User) (width 0.12))
  (fp_arc (start 85.525 -7.95) (end 86.9 -7.95) (angle -180) (layer Dwgs.User) (width 0.12))
  (fp_line (start 86.9 -3.45) (end 87.4 -2.95) (layer Dwgs.User) (width 0.12))
  (fp_line (start 99.6 -5.5) (end 99.6 -7.95) (layer Dwgs.User) (width 0.12))
  (fp_line (start 95.9 -7.95) (end 86.9 -7.95) (layer Dwgs.User) (width 0.12))
  (fp_arc (start 95.9 -9.7) (end 94.15 -9.7) (angle -90) (layer Dwgs.User) (width 0.12))
  (fp_line (start 95.9 -7.95) (end 99.6 -7.95) (layer Dwgs.User) (width 0.12))
  (fp_arc (start 95.9 -11) (end 95.9 -12.75) (angle -90) (layer Dwgs.User) (width 0.12))
  (fp_line (start 94.15 -11) (end 94.15 -9.7) (layer Dwgs.User) (width 0.12))
  (fp_line (start 98.2 -2.95) (end 99.6 -5.5) (layer Dwgs.User) (width 0.12))
  (fp_poly (pts (xy 86.9 -7.95) (xy 99.6 -7.95) (xy 99.6 -5.5) (xy 98.2 -2.95)
    (xy 87.4 -2.95) (xy 86.9 -3.45)) (layer F.Mask) (width 0))
  (fp_poly (pts (xy 86.9 -7.95) (xy 99.6 -7.95) (xy 99.6 -5.5) (xy 98.2 -2.95)
    (xy 87.4 -2.95) (xy 86.9 -3.45)) (layer B.Mask) (width 0))
  (fp_text user "Keep Out Cu" (at 93 -1.75) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad A13 connect rect (at 14.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A12 connect rect (at 13.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A18 connect rect (at 19.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A17 connect rect (at 18.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A16 connect rect (at 17.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A15 connect rect (at 16.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A14 connect rect (at 15.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A11 connect rect (at 10.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A10 connect rect (at 9.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A9 connect rect (at 8.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A8 connect rect (at 7.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A7 connect rect (at 6.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A6 connect rect (at 5.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A5 connect rect (at 4.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A4 connect rect (at 3.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A3 connect rect (at 2.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A2 connect rect (at 1.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A1 connect rect (at 0.5 -4) (size 0.7 3.2) (layers B.Cu))
  (pad B13 connect rect (at 14.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B12 connect rect (at 13.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B18 connect rect (at 19.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B17 connect rect (at 18.5 -4) (size 0.7 3.2) (layers F.Cu))
  (pad B16 connect rect (at 17.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B15 connect rect (at 16.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B14 connect rect (at 15.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B11 connect rect (at 10.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B10 connect rect (at 9.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B9 connect rect (at 8.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B8 connect rect (at 7.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B7 connect rect (at 6.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B6 connect rect (at 5.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B5 connect rect (at 4.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B4 connect rect (at 3.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B3 connect rect (at 2.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B2 connect rect (at 1.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B1 connect rect (at 0.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B19 connect rect (at 20.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad A19 connect rect (at 20.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad B20 connect rect (at 21.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B21 connect rect (at 22.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B22 connect rect (at 23.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B23 connect rect (at 24.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B24 connect rect (at 25.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B25 connect rect (at 26.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B26 connect rect (at 27.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B27 connect rect (at 28.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B28 connect rect (at 29.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B29 connect rect (at 30.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B30 connect rect (at 31.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B31 connect rect (at 32.5 -4) (size 0.7 3.2) (layers F.Cu))
  (pad B32 connect rect (at 33.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad A20 connect rect (at 21.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A21 connect rect (at 22.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A22 connect rect (at 23.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A23 connect rect (at 24.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A24 connect rect (at 25.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A25 connect rect (at 26.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A26 connect rect (at 27.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A27 connect rect (at 28.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A28 connect rect (at 29.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A29 connect rect (at 30.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A30 connect rect (at 31.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A31 connect rect (at 32.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A32 connect rect (at 33.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A33 connect rect (at 34.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A34 connect rect (at 35.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A35 connect rect (at 36.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A36 connect rect (at 37.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A37 connect rect (at 38.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A38 connect rect (at 39.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A39 connect rect (at 40.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A40 connect rect (at 41.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A41 connect rect (at 42.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A42 connect rect (at 43.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A43 connect rect (at 44.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A44 connect rect (at 45.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A45 connect rect (at 46.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A46 connect rect (at 47.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A47 connect rect (at 48.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A48 connect rect (at 49.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A49 connect rect (at 50.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad B33 connect rect (at 34.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B34 connect rect (at 35.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B35 connect rect (at 36.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B36 connect rect (at 37.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B37 connect rect (at 38.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B38 connect rect (at 39.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B39 connect rect (at 40.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B40 connect rect (at 41.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B41 connect rect (at 42.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B42 connect rect (at 43.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B43 connect rect (at 44.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B44 connect rect (at 45.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B45 connect rect (at 46.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B46 connect rect (at 47.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B47 connect rect (at 48.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B48 connect rect (at 49.5 -4) (size 0.7 3.2) (layers F.Cu))
  (pad B49 connect rect (at 50.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B50 connect rect (at 51.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B51 connect rect (at 52.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B52 connect rect (at 53.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B53 connect rect (at 54.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B54 connect rect (at 55.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B55 connect rect (at 56.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B56 connect rect (at 57.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B57 connect rect (at 58.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B58 connect rect (at 59.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B59 connect rect (at 60.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B60 connect rect (at 61.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B61 connect rect (at 62.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B62 connect rect (at 63.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B63 connect rect (at 64.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B64 connect rect (at 65.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B65 connect rect (at 66.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B66 connect rect (at 67.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B67 connect rect (at 68.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B68 connect rect (at 69.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B69 connect rect (at 70.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B70 connect rect (at 71.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B71 connect rect (at 72.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B72 connect rect (at 73.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B73 connect rect (at 74.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B74 connect rect (at 75.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B75 connect rect (at 76.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B76 connect rect (at 77.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B77 connect rect (at 78.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B78 connect rect (at 79.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B79 connect rect (at 80.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B80 connect rect (at 81.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad B81 connect rect (at 82.5 -4) (size 0.7 3.2) (layers F.Cu))
  (pad B82 connect rect (at 83.5 -3.5) (size 0.7 4.2) (layers F.Cu))
  (pad A50 connect rect (at 51.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A51 connect rect (at 52.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A52 connect rect (at 53.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A53 connect rect (at 54.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A54 connect rect (at 55.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A55 connect rect (at 56.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A56 connect rect (at 57.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A57 connect rect (at 58.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A58 connect rect (at 59.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A59 connect rect (at 60.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A60 connect rect (at 61.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A61 connect rect (at 62.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A62 connect rect (at 63.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A63 connect rect (at 64.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A64 connect rect (at 65.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A65 connect rect (at 66.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A66 connect rect (at 67.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A67 connect rect (at 68.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A68 connect rect (at 69.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A69 connect rect (at 70.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A70 connect rect (at 71.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A71 connect rect (at 72.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A72 connect rect (at 73.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A73 connect rect (at 74.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A74 connect rect (at 75.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A75 connect rect (at 76.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A76 connect rect (at 77.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A77 connect rect (at 78.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A78 connect rect (at 79.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A79 connect rect (at 80.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A80 connect rect (at 81.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A81 connect rect (at 82.5 -3.5) (size 0.7 4.2) (layers B.Cu))
  (pad A82 connect rect (at 83.5 -3.5) (size 0.7 4.2) (layers B.Cu))
)
