(footprint "M.2 C Key Connector"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.08 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "192656a4-d1cb-4e09-8d59-5f94769679ab")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "M.2 C Key Connector"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cb04d929-07a4-4ab2-8b46-9700f01a20eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4918a189-9e1a-43bf-a05c-34e4e610d286")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a394491f-1cd1-409c-9f9b-c47da2d0e55c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_rect
		(start -9.925 -0.94)
		(end 9.925 1.11)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "680f2dbd-4201-41ce-b215-c56ea361d055")
	)
	(fp_rect
		(start -9.925 -1.44)
		(end 9.925 1.11)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "B.Mask")
		(uuid "db7a4d36-3f34-4033-b3a0-b9cfdb8675ca")
	)
	(fp_line
		(start -15 -108.89)
		(end 15 -108.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "882919ef-b482-4a81-a30f-3ba12e7099f3")
	)
	(fp_line
		(start -15 -78.89)
		(end 15 -78.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "8cd028dd-0f51-4d86-9668-74a340f03999")
	)
	(fp_line
		(start -15 -58.89)
		(end 15 -58.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "b5e2da54-cee5-4883-8059-0aad10e18d7b")
	)
	(fp_line
		(start -15 -40.89)
		(end 15 -40.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "783a5739-ba44-4b19-a5f8-b6777f8ce734")
	)
	(fp_line
		(start -15 -28.89)
		(end 15 -28.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ce6c26b4-a6ae-43e6-8d71-98bf0607a0ce")
	)
	(fp_line
		(start -15 -2.89)
		(end -15 -108.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "0a636e4d-5cc9-4005-a52f-044a98c1439d")
	)
	(fp_line
		(start -15 -2.89)
		(end -15 -78.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "06ef01d9-0519-43d8-8cd3-bab4bc1d9250")
	)
	(fp_line
		(start -15 -2.89)
		(end -15 -58.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "aa379611-d849-481b-8e9c-da03d22f16a4")
	)
	(fp_line
		(start -15 -2.89)
		(end -15 -40.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "d2350da6-fd38-4119-95a9-572bdd38fee2")
	)
	(fp_line
		(start -15 -2.89)
		(end -15 -28.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "6f8f5c26-d83a-4917-80eb-e6e03255decb")
	)
	(fp_line
		(start -11 -108.89)
		(end 11 -108.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "125cc4f5-cdc3-44f4-ab43-ba9766e33c30")
	)
	(fp_line
		(start -11 -78.89)
		(end 11 -78.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f3889784-7c5e-48bd-bda7-9d35a2dbe20c")
	)
	(fp_line
		(start -11 -58.89)
		(end 11 -58.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "2ac0af95-1e95-4369-98d2-b4f9052f50cf")
	)
	(fp_line
		(start -11 -40.89)
		(end 11 -40.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3110ccc3-5262-46cc-b8d6-1f539a211342")
	)
	(fp_line
		(start -11 -28.89)
		(end 11 -28.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "53bcdb19-0373-4014-830c-aba8532cdc01")
	)
	(fp_line
		(start -11 -2.89)
		(end -15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "111c631a-3e2c-4a1e-bcaa-c47f3608e031")
	)
	(fp_line
		(start -11 -2.89)
		(end -11 -108.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f28d68b8-fe7f-4646-bff5-3d0ffefe8d82")
	)
	(fp_line
		(start -11 -2.89)
		(end -11 -78.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a7b40686-b853-4880-af47-16d3954ab709")
	)
	(fp_line
		(start -11 -2.89)
		(end -11 -58.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "6e998948-1ac9-417a-9614-fcf71fbd5751")
	)
	(fp_line
		(start -11 -2.89)
		(end -11 -40.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3e9d1a94-1893-45e2-858b-391605409c3d")
	)
	(fp_line
		(start -11 -2.89)
		(end -11 -28.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "2a288a9e-eb09-4fdb-9e10-6a1214d7875e")
	)
	(fp_line
		(start 11 -108.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "135aefc0-0e2b-4030-b0dc-5673f8033443")
	)
	(fp_line
		(start 11 -78.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "cd14bb83-d926-40ec-95de-5b5222d81616")
	)
	(fp_line
		(start 11 -58.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "04f3b255-84f6-432c-990f-9946a2754206")
	)
	(fp_line
		(start 11 -40.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "0ae5492b-054c-4d04-87e4-e2d589b98b96")
	)
	(fp_line
		(start 11 -28.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "75649bc8-c1e9-4401-aa3a-0dda5762478e")
	)
	(fp_line
		(start 11 -2.89)
		(end 15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "5d42408a-9d86-431f-8f09-281b87e72034")
	)
	(fp_line
		(start 15 -108.89)
		(end 15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9b3bec11-1c2e-4d1e-98d1-3b24096c4544")
	)
	(fp_line
		(start 15 -78.89)
		(end 15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "b67de0ba-64b9-4bc4-921b-a690a22ba891")
	)
	(fp_line
		(start 15 -40.89)
		(end 15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ed51600e-e92d-4994-8f81-0c94a7069553")
	)
	(fp_line
		(start 15 -28.89)
		(end 15 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a1213e84-7f0a-475f-a2ad-4f37a54a796e")
	)
	(fp_line
		(start 15 -2.89)
		(end 15 -58.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "e8eaa609-5ee4-442f-829e-cca10b6a5d59")
	)
	(fp_line
		(start -11 -2.89)
		(end -10.425 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "ef47feb2-ff01-4fc6-83e7-b678df578b2d")
	)
	(fp_line
		(start -9.925 -2.39)
		(end -9.925 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "0f55a34f-16ac-44ae-b324-9e518338ffb5")
	)
	(fp_line
		(start 4.025 -1.79)
		(end 4.025 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "ef052d65-7d31-4bb2-be27-1eba79b5f870")
	)
	(fp_line
		(start 4.025 1.11)
		(end -9.925 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3b490415-4b99-4cfe-9b7b-176fea5679cf")
	)
	(fp_line
		(start 5.225 -1.79)
		(end 5.225 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "cc69705d-a12e-49d6-be20-65e230d0a302")
	)
	(fp_line
		(start 5.225 1.11)
		(end 9.925 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "cf09ab38-b81a-4e6f-911c-3d9a7d5b1184")
	)
	(fp_line
		(start 9.925 -2.39)
		(end 9.925 1.11)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "91a4dabd-03ac-4e80-934f-783a0e86f665")
	)
	(fp_line
		(start 10.425 -2.89)
		(end 11 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2f817b17-536b-4c2f-bd3a-be47d4d733d3")
	)
	(fp_arc
		(start -10.425 -2.89)
		(mid -10.071447 -2.743553)
		(end -9.925 -2.39)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "5371f54c-011e-4222-bffa-ef3e56856db4")
	)
	(fp_arc
		(start 4.025 -1.79)
		(mid 4.625 -2.39)
		(end 5.225 -1.79)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f03b335d-ee70-428d-8ddc-c70f5e6f432a")
	)
	(fp_arc
		(start 9.925 -2.39)
		(mid 10.071447 -2.743553)
		(end 10.425 -2.89)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "56464fd9-0c09-42c2-8877-fe450ade8437")
	)
	(fp_line
		(start -0.71 -109.6)
		(end 0.71 -108.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "81b378b7-cab6-4ee6-b399-41ba2bfc2143")
	)
	(fp_line
		(start -0.71 -79.6)
		(end 0.71 -78.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "ebec3253-45ff-414f-a267-0424484881ad")
	)
	(fp_line
		(start -0.71 -59.6)
		(end 0.71 -58.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "f304e90b-64e0-48a4-b5b7-d9ca9e1248d0")
	)
	(fp_line
		(start -0.71 -41.6)
		(end 0.71 -40.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "cad7ac4c-344b-4c3e-92c5-15f007ab4ad5")
	)
	(fp_line
		(start -0.71 -29.6)
		(end 0.71 -28.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "91dfd78b-b281-4a68-b471-e8f78e507d97")
	)
	(fp_line
		(start 0.71 -109.6)
		(end -0.71 -108.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "4ac0a155-54d8-47ea-84fd-cb2386ee41c2")
	)
	(fp_line
		(start 0.71 -79.6)
		(end -0.71 -78.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "8f776ea3-f0ef-40b4-9d9f-208250fde3f1")
	)
	(fp_line
		(start 0.71 -59.6)
		(end -0.71 -58.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "598fabb6-73e7-43f8-9e6b-76e4088a2b35")
	)
	(fp_line
		(start 0.71 -41.6)
		(end -0.71 -40.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "57126008-c467-42d0-8ea1-15c019ab5b8e")
	)
	(fp_line
		(start 0.71 -29.6)
		(end -0.71 -28.18)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "User.3")
		(uuid "545acf8e-f2fc-4a9f-9e73-d38a1b20181a")
	)
	(fp_rect
		(start -15 -108.89)
		(end 15 -105.09)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "4746ff9e-8e16-4965-bfc9-c3ac748582cf")
	)
	(fp_rect
		(start -15 -78.89)
		(end 15 -75.09)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "1428f8c0-df31-4cb6-be19-5576671ae5c5")
	)
	(fp_rect
		(start -15 -58.89)
		(end 15 -55.09)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "9f806709-f435-4987-b70d-e2a81ceff9c4")
	)
	(fp_rect
		(start -15 -40.89)
		(end 15 -37.09)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "8204e817-9c96-4256-a202-2c4f9f2b2089")
	)
	(fp_rect
		(start -15 -28.89)
		(end 15 -25.09)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "a6198dba-f55d-4452-b7eb-9a2624bfe92f")
	)
	(fp_text user "C"
		(at 5.29 -2.37 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "88397dbc-8c4b-4303-ad85-eb91c9f1cf49")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c85f7fe0-22ef-4fad-b6e9-25f448a35594")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "22, 30mm width and 30, 42, 60, 80, 110mm length shown in Blue (User.2 Layer)"
		(at 0.02 14.055 0)
		(unlocked yes)
		(layer "User.2")
		(uuid "7658fade-61e9-4ef6-acb5-59bc0c631491")
		(effects
			(font
				(size 2 2)
				(thickness 0.2)
			)
		)
	)
	(fp_text user "Place grounded \"M.2 Mounting Pad\" footprint from library on Teal (User.3 Layer) X's"
		(at -0.13 9.4 0)
		(unlocked yes)
		(layer "User.3")
		(uuid "baea5827-685f-4314-9f95-7cc0e482adde")
		(effects
			(font
				(size 2 2)
				(thickness 0.2)
			)
		)
	)
	(fp_text user "Yellow areas (User.4 Layer) reserverd for RF recepticals or for components when no RF recepticals used."
		(at 0.165 4.83 0)
		(unlocked yes)
		(layer "User.4")
		(uuid "1c693502-7135-4f9e-9212-a1db191c3cdd")
		(effects
			(font
				(size 2 2)
				(thickness 0.2)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "00022239-06dd-41ac-8323-01ad8b242688")
		(pts
			(xy -15 -110) (xy 15 -110)
		)
		(height -17.83)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "30"
			(at 0 -131.23 0)
			(layer "User.2")
			(uuid "00022239-06dd-41ac-8323-01ad8b242688")
			(effects
				(font
					(size 3 3)
					(thickness 0.4)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "0308f5da-1fce-4b49-9520-852c0965b404")
		(pts
			(xy -11 -108.89) (xy 11 -108.89)
		)
		(height -12.48)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "22"
			(at 0 -124.77 0)
			(layer "User.2")
			(uuid "0308f5da-1fce-4b49-9520-852c0965b404")
			(effects
				(font
					(size 3 3)
					(thickness 0.4)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "06cb66bb-6ada-45ea-97c0-9a96b19b9695")
		(pts
			(xy 9.925 1.11) (xy 9.925 -28.89)
		)
		(height 20.795)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "30"
			(at 27.42 -13.89 90)
			(layer "User.2")
			(uuid "06cb66bb-6ada-45ea-97c0-9a96b19b9695")
			(effects
				(font
					(size 3 3)
					(thickness 0.3)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "07cb8170-2d65-45ae-8306-85aa16104a11")
		(pts
			(xy 9.925 1.11) (xy 9.925 -40.89)
		)
		(height 32.695)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "42"
			(at 39.32 -19.89 90)
			(layer "User.2")
			(uuid "07cb8170-2d65-45ae-8306-85aa16104a11")
			(effects
				(font
					(size 3 3)
					(thickness 0.3)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "2f4c16dd-d765-4fce-9700-abc494314154")
		(pts
			(xy 9.925 1.11) (xy 9.925 -108.89)
		)
		(height 69.74)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "110"
			(at 76.365 -53.89 90)
			(layer "User.2")
			(uuid "2f4c16dd-d765-4fce-9700-abc494314154")
			(effects
				(font
					(size 3 3)
					(thickness 0.3)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "8e7b4a1a-6d9d-42ab-bc28-7d1fbc72dbdd")
		(pts
			(xy 9.91 1.11) (xy 9.91 -78.89)
		)
		(height 58.985)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "80"
			(at 65.595 -38.89 90)
			(layer "User.2")
			(uuid "8e7b4a1a-6d9d-42ab-bc28-7d1fbc72dbdd")
			(effects
				(font
					(size 3 3)
					(thickness 0.3)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "bd592960-1622-47b7-a51f-c9fb7513c6ce")
		(pts
			(xy 9.925 1.11) (xy 9.925 -58.89)
		)
		(height 45.245)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "60"
			(at 51.87 -28.89 90)
			(layer "User.2")
			(uuid "bd592960-1622-47b7-a51f-c9fb7513c6ce")
			(effects
				(font
					(size 3 3)
					(thickness 0.3)
				)
			)
		)
	)
	(pad "1" smd rect
		(at 9.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "3d4ee158-1c68-4654-ac1b-db6aadfd4193")
	)
	(pad "2" smd rect
		(at 9 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "ab2a0152-3f56-4468-b760-b2c3162a4a30")
	)
	(pad "3" smd rect
		(at 8.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "3181608a-b4fd-41c4-ad79-0ccd5f672c07")
	)
	(pad "4" smd rect
		(at 8.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "dbd26d0f-59dc-4418-a777-ae35712ace8e")
	)
	(pad "5" smd rect
		(at 8.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "4ca3510b-5b02-4795-8f25-aa28137af661")
	)
	(pad "6" smd rect
		(at 8 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "e70dc44a-d7a9-4c5f-ad31-e2db7cef2b01")
	)
	(pad "7" smd rect
		(at 7.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "a546dcda-fa2a-4818-9ddf-f8d69a756a01")
	)
	(pad "8" smd rect
		(at 7.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "fc270a2c-d4a8-4265-988a-e3d8380a7f42")
	)
	(pad "9" smd rect
		(at 7.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "199fc270-9276-4324-9015-ef98ecc6a81d")
	)
	(pad "10" smd rect
		(at 7 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "c15aba62-3280-438d-b936-c316320ae6bc")
	)
	(pad "11" smd rect
		(at 6.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "0c6191ed-ce78-448b-a1ed-408ae7cb1715")
	)
	(pad "12" smd rect
		(at 6.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "843a8efb-7e4e-4990-a4be-339205ea75e6")
	)
	(pad "13" smd rect
		(at 6.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "771c4e82-d291-445e-897e-bb46e27fa502")
	)
	(pad "14" smd rect
		(at 6 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "37eb73c7-8e65-4b95-81bb-913abf91683b")
	)
	(pad "15" smd rect
		(at 5.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "ac72e029-0f3c-4dd8-97ca-46debe1f8a78")
	)
	(pad "24" smd rect
		(at 3.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "dedfd1e0-0d0b-4490-b63a-b1f0be7a798b")
	)
	(pad "25" smd rect
		(at 3.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "7367b1b8-17d8-42f4-9488-41dbc04f3ec7")
	)
	(pad "26" smd rect
		(at 3 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "c03cb1d3-ce35-4a83-8ad7-7dbc1beb5310")
	)
	(pad "27" smd rect
		(at 2.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "5bbc2b6e-96ae-49cd-afac-c8b62186a3c1")
	)
	(pad "28" smd rect
		(at 2.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "cf971939-e7d7-4b60-9ba8-c15ce4202000")
	)
	(pad "29" smd rect
		(at 2.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "71a1a2b7-b8ba-4f2c-91e9-8d6d41f76f94")
	)
	(pad "30" smd rect
		(at 2 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "90881e95-0686-46f7-b3dc-e7533420d5f7")
	)
	(pad "31" smd rect
		(at 1.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "f28777f6-8773-4981-8549-f601df33b8a7")
	)
	(pad "32" smd rect
		(at 1.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "444c9c13-16b5-4ccd-9ee4-e9c9dc60ac71")
	)
	(pad "33" smd rect
		(at 1.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "02a93394-a9cc-49be-9f42-8076ec4c15f6")
	)
	(pad "34" smd rect
		(at 1 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "6bf64faf-eb45-4407-9665-fcfc2c51ce71")
	)
	(pad "35" smd rect
		(at 0.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "d1b6c7db-5061-41ea-be98-b2acdd54895f")
	)
	(pad "36" smd rect
		(at 0.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "6fd7a7ff-2817-4f26-96a3-b34553a11f72")
	)
	(pad "37" smd rect
		(at 0.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "c0e43607-94f8-496b-acdd-5f1261bbef75")
	)
	(pad "38" smd rect
		(at 0 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "d038712e-1cb1-4579-a428-72b9632d1724")
	)
	(pad "39" smd rect
		(at -0.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "58bd3a0d-6f28-4dfa-8d23-88293eb4df29")
	)
	(pad "40" smd rect
		(at -0.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "bd6abd44-447b-40f1-804c-ca0dcfd4786f")
	)
	(pad "41" smd rect
		(at -0.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "94b6194c-d33a-4abf-96df-123600e22663")
	)
	(pad "42" smd rect
		(at -1 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "aed1104b-7d87-4ea4-a09a-b232ca78fd39")
	)
	(pad "43" smd rect
		(at -1.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "ddb2d6f3-6a24-4d7b-86c2-65a0849daba6")
	)
	(pad "44" smd rect
		(at -1.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "f0875a53-5846-49e6-bdf5-6b6471426377")
	)
	(pad "45" smd rect
		(at -1.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "98c1f934-5c06-43f7-9ee4-cc30d40d97b2")
	)
	(pad "46" smd rect
		(at -2 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "72767cf5-5bef-4551-81b6-5e1b0a100e2e")
	)
	(pad "47" smd rect
		(at -2.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "87ce3df8-c567-4963-99e5-a5fb4228b918")
	)
	(pad "48" smd rect
		(at -2.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "ccb9321a-a9d5-4c50-9dfe-aa8984736e30")
	)
	(pad "49" smd rect
		(at -2.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "a77f0c5c-f780-42c0-9f30-2ec609724ac3")
	)
	(pad "50" smd rect
		(at -3 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "4b1949eb-32cf-4864-a6df-5e147b0e825e")
	)
	(pad "51" smd rect
		(at -3.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "aea5f8db-3d7c-43cc-afc0-4d2b72483424")
	)
	(pad "52" smd rect
		(at -3.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "9d2dd827-0497-4320-96e3-476c99a6c63b")
	)
	(pad "53" smd rect
		(at -3.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "6cc90286-dbd1-4a79-bb36-383fb71ab547")
	)
	(pad "54" smd rect
		(at -4 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "dca8c69b-0ebe-4726-a60f-29d5e32c3fbb")
	)
	(pad "55" smd rect
		(at -4.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "533f07d0-724f-4bc5-a378-3a05451b7ae4")
	)
	(pad "56" smd rect
		(at -4.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "30fd98f9-0cfd-4e4c-8cce-6ece9c46c99c")
	)
	(pad "57" smd rect
		(at -4.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "6f2ada47-1cc8-4836-83c9-c4649a1c89a5")
	)
	(pad "58" smd rect
		(at -5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "14cbeec0-3020-42d1-be12-fb85df50f50e")
	)
	(pad "59" smd rect
		(at -5.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "cbe873bf-d11c-4792-b0bd-a6d507780af0")
	)
	(pad "60" smd rect
		(at -5.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "f2e08787-2ab6-4fd7-8913-d3197583f780")
	)
	(pad "61" smd rect
		(at -5.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "a627ab2c-efef-466d-b8e4-49e2ed250886")
	)
	(pad "62" smd rect
		(at -6 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "80b17273-ce6a-4bd4-9bb0-abb9535d1006")
	)
	(pad "63" smd rect
		(at -6.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "b8d2cf28-ca14-4cc2-999f-7ab93dea54f9")
	)
	(pad "64" smd rect
		(at -6.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "ef9d0a1c-6356-4f87-a3ec-e350ca82843b")
	)
	(pad "65" smd rect
		(at -6.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "d048e7f8-3541-4a32-a7d7-7b0ff5e252f6")
	)
	(pad "66" smd rect
		(at -7 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "473c7e8a-65fd-4911-9eb7-10e353b343b4")
	)
	(pad "67" smd rect
		(at -7.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "a64604f2-f8ce-484c-b214-1dead7340d77")
	)
	(pad "68" smd rect
		(at -7.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "14de7a5a-588b-41fc-80c2-92c8d927295b")
	)
	(pad "69" smd rect
		(at -7.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "99701112-b2a5-4f95-8556-198358f00cdb")
	)
	(pad "70" smd rect
		(at -8 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "c3ef7a3e-8238-438e-bf3e-1d012e57f5df")
	)
	(pad "71" smd rect
		(at -8.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "e3e7b4c2-36bc-42a0-b859-52669aef63f3")
	)
	(pad "72" smd rect
		(at -8.5 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "332fbe63-eaf0-4a3e-8edc-9813e23824ca")
	)
	(pad "73" smd rect
		(at -8.75 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "c06572c1-d764-4172-b897-7d0b4b14fdd5")
	)
	(pad "74" smd rect
		(at -9 -0.29 180)
		(size 0.35 2.2)
		(layers "B.Cu")
		(thermal_bridge_angle 45)
		(uuid "424d8695-af46-4f73-b82c-12353796f215")
	)
	(pad "75" smd rect
		(at -9.25 -0.04 180)
		(size 0.35 1.7)
		(layers "F.Cu")
		(thermal_bridge_angle 45)
		(uuid "7ae3fec0-d8d7-46f7-8952-778afd51c0fc")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "87e697a5-1f05-4587-bd13-db6526ec55c7")
		(name "Front Component Keepout")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 11 -2.89) (xy 11 1.11) (xy -11 1.11) (xy -11 -2.89)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(uuid "ace17c97-ffe4-4c62-add0-b497c1831dfe")
		(name "Rear Component Keepout")
		(hatch full 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 15 1.11) (xy 15 -4.09) (xy -15 -4.09) (xy -15 1.11)
			)
		)
	)
	(embedded_fonts no)
)
