# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2009 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II
# Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition
# Date created = 03:22:36  August 28, 2022
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		sp2_max_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY MAX7000S
set_global_assignment -name DEVICE "EPM7128STC100-10"
set_global_assignment -name TOP_LEVEL_ENTITY sp2_max
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "9.0 SP2"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "03:22:36  AUGUST 28, 2022"
set_global_assignment -name LAST_QUARTUS_VERSION "9.0 SP2"
set_location_assignment PIN_6 -to CMOS_AS
set_location_assignment PIN_8 -to WR_PDOS
set_location_assignment PIN_9 -to WD
set_location_assignment PIN_10 -to WSTB
set_location_assignment PIN_12 -to TR43
set_location_assignment PIN_12 -to TR[43]
set_location_assignment PIN_13 -to CLK_WG
set_location_assignment PIN_14 -to FDAT
set_location_assignment PIN_16 -to QDAT
set_location_assignment PIN_17 -to XA0
set_location_assignment PIN_17 -to XA[0]
set_location_assignment PIN_19 -to SINC_2
set_location_assignment PIN_19 -to SINC_[2]
set_location_assignment PIN_20 -to SINC_1
set_location_assignment PIN_20 -to SINC_[1]
set_location_assignment PIN_21 -to XA1
set_location_assignment PIN_21 -to XA[1]
set_location_assignment PIN_23 -to XA2
set_location_assignment PIN_23 -to XA[2]
set_location_assignment PIN_25 -to RSTB
set_location_assignment PIN_29 -to SR
set_location_assignment PIN_30 -to SL
set_location_assignment PIN_31 -to CLK14
set_location_assignment PIN_31 -to CLK[14]
set_location_assignment PIN_32 -to CLKZZ
set_location_assignment PIN_33 -to UNUSED33
set_location_assignment PIN_33 -to UNUSED[33]
set_location_assignment PIN_35 -to AUD
set_location_assignment PIN_36 -to TG42_BUF
set_location_assignment PIN_37 -to XACS
set_location_assignment PIN_40 -to HDD_C3
set_location_assignment PIN_40 -to HDD_C[3]
set_location_assignment PIN_41 -to HDD_C2
set_location_assignment PIN_41 -to HDD_C[2]
set_location_assignment PIN_42 -to HDD_C1
set_location_assignment PIN_42 -to HDD_C[1]
set_location_assignment PIN_44 -to FDD_C0
set_location_assignment PIN_44 -to FDD_C[0]
set_location_assignment PIN_45 -to FDD_C1
set_location_assignment PIN_45 -to FDD_C[1]
set_location_assignment PIN_46 -to FDD_C2
set_location_assignment PIN_46 -to FDD_C[2]
set_location_assignment PIN_47 -to HDD_C0
set_location_assignment PIN_47 -to HDD_C[0]
set_location_assignment PIN_48 -to HD_DIR
set_location_assignment PIN_52 -to HD_CS
set_location_assignment PIN_53 -to UNUSED53
set_location_assignment PIN_53 -to UNUSED[53]
set_location_assignment PIN_54 -to /CONF_X
set_location_assignment PIN_56 -to 10K_CLK
set_location_assignment PIN_57 -to WR_CNF
set_location_assignment PIN_58 -to 10K_D0
set_location_assignment PIN_58 -to 10K_D[0]
set_location_assignment PIN_60 -to D0
set_location_assignment PIN_60 -to D[0]
set_location_assignment PIN_61 -to VGA_IN
set_location_assignment PIN_64 -to SINC_V
set_location_assignment PIN_65 -to UNUSED65
set_location_assignment PIN_65 -to UNUSED[65]
set_location_assignment PIN_67 -to SINC
set_location_assignment PIN_68 -to SINC_H
set_location_assignment PIN_69 -to SINC_IN
set_location_assignment PIN_71 -to XHD_RES
set_location_assignment PIN_75 -to XHD_WR
set_location_assignment PIN_76 -to XHD_RD
set_location_assignment PIN_78 -to UNUSED78
set_location_assignment PIN_78 -to UNUSED[78]
set_location_assignment PIN_79 -to XHD1_CS1
set_location_assignment PIN_79 -to XHD1_CS[1]
set_location_assignment PIN_80 -to XHD1_CS2
set_location_assignment PIN_80 -to XHD1_CS[2]
set_location_assignment PIN_81 -to XHD2_CS1
set_location_assignment PIN_81 -to XHD2_CS[1]
set_location_assignment PIN_83 -to XHD2_CS2
set_location_assignment PIN_83 -to XHD2_CS[2]
set_location_assignment PIN_84 -to BEEP
set_location_assignment PIN_85 -to TG42_OUT
set_location_assignment PIN_87 -to TG42_IN
set_location_assignment PIN_88 -to XHR_RDY
set_location_assignment PIN_89 -to EPM_RES
set_location_assignment PIN_90 -to PW_GOOD
set_location_assignment PIN_92 -to RDAT
set_location_assignment PIN_93 -to /WG_WR
set_location_assignment PIN_94 -to STE
set_location_assignment PIN_96 -to DENS_X
set_location_assignment PIN_97 -to /WG_RD
set_location_assignment PIN_98 -to WDAT
set_location_assignment PIN_99 -to CMOS_DRD
set_location_assignment PIN_100 -to CMOS_DWR
set_global_assignment -name FMAX_REQUIREMENT "100 MHz"
set_global_assignment -name CUT_OFF_CLEAR_AND_PRESET_PATHS ON
set_global_assignment -name CUT_OFF_IO_PIN_FEEDBACK ON
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to LR_T1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to LR_T[1]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to LR_T0
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to LR_T[0]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to CLK_WG
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD_RD
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD_RES
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD_WR
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD1_CS1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD1_CS[1]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD1_CS2
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD1_CS[2]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD2_CS1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD2_CS[1]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD2_CS2
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to XHD2_CS[2]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to 10K_CLK
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to 10K_D0
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT OFF -to 10K_D[0]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P0
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P[0]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P[1]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P2
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to REG_P[2]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to TG42_BUF
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to TG42_OUT
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG0
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG[0]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG[1]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG2
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to STWG[2]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to XCT0
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to XCT[0]
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to XCT1
set_instance_assignment -name MAX7000_INDIVIDUAL_TURBO_BIT ON -to XCT[1]
set_global_assignment -name SECURITY_BIT ON
set_global_assignment -name ENABLE_VREFB_PIN OFF
set_global_assignment -name ENABLE_VREFA_PIN OFF
set_global_assignment -name MAX7000B_VCCIO_IOBANK2 3.3V
set_global_assignment -name MAX7000B_VCCIO_IOBANK1 3.3V
set_global_assignment -name DISABLE_NCS_AND_OE_PULLUPS_ON_CONFIG_DEVICE OFF
set_global_assignment -name FLEX10K_CONFIG_DEVICE_JTAG_USER_CODE FFFFFFFF
set_global_assignment -name FLEX6K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE OFF
set_global_assignment -name FLEX10K_ENABLE_LOW_VOLTAGE_MODE_ON_CONFIG_DEVICE ON
set_global_assignment -name ENABLE_JTAG_BST_SUPPORT OFF
set_global_assignment -name FLEX6K_CONFIGURATION_SCHEME "PASSIVE SERIAL"
set_global_assignment -name MAX7000_ENABLE_JTAG_BST_SUPPORT ON
set_global_assignment -name FLEX10K_ENABLE_LOCK_OUTPUT OFF
set_global_assignment -name MAX7000_JTAG_USER_CODE FFFF
set_global_assignment -name FLEX10K_CONFIGURATION_SCHEME "PASSIVE SERIAL"
set_global_assignment -name FLEX10K_JTAG_USER_CODE 7F
set_global_assignment -name ENABLE_INIT_DONE_OUTPUT OFF
set_global_assignment -name ENABLE_DEVICE_WIDE_OE OFF
set_global_assignment -name ENABLE_DEVICE_WIDE_RESET OFF
set_global_assignment -name RESERVE_NCEO_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_RDYNBUSY_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_NWS_NRS_NCS_CS_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RESERVE_DATA7_THROUGH_DATA1_AFTER_CONFIGURATION "USE AS REGULAR IO"
set_global_assignment -name RELEASE_CLEARS_BEFORE_TRI_STATES OFF
set_global_assignment -name AUTO_RESTART_CONFIGURATION OFF
set_global_assignment -name USER_START_UP_CLOCK OFF
set_global_assignment -name AUTO_GLOBAL_REGISTER_CONTROLS OFF
set_global_assignment -name AUTO_GLOBAL_CLOCK OFF
set_global_assignment -name AUTO_IMPLEMENT_IN_ROM OFF
set_global_assignment -name AUTO_OPEN_DRAIN_PINS ON
set_global_assignment -name STATE_MACHINE_PROCESSING AUTO
set_global_assignment -name AUTO_PACKED_REGISTERS OFF
set_global_assignment -name AUTO_FAST_INPUT_REGISTERS OFF
set_global_assignment -name AUTO_FAST_OUTPUT_REGISTERS OFF
set_global_assignment -name AUTO_GLOBAL_OE ON
set_global_assignment -name FLEX6K_OPTIMIZATION_TECHNIQUE AREA
set_global_assignment -name FLEX10K_OPTIMIZATION_TECHNIQUE AREA
set_global_assignment -name SAVE_DISK_SPACE ON
set_global_assignment -name SMART_RECOMPILE OFF
set_global_assignment -name SIMULATION_MODE TIMING
set_global_assignment -name EDA_SHOW_LMF_MAPPING_MESSAGES OFF -section_id eda_design_synthesis
set_global_assignment -name EDA_INPUT_GND_NAME GND -section_id eda_design_synthesis
set_global_assignment -name EDA_INPUT_VCC_NAME VCC -section_id eda_design_synthesis
set_global_assignment -name END_TIME "25 us"
set_global_assignment -name START_TIME "0 ns"
set_global_assignment -name GLITCH_INTERVAL "0 ns"
set_global_assignment -name GLITCH_DETECTION OFF
set_global_assignment -name CHECK_OUTPUTS OFF
set_global_assignment -name SETUP_HOLD_DETECTION OFF
set_global_assignment -name CUT_OFF_READ_DURING_WRITE_PATHS OFF
set_global_assignment -name NUMBER_OF_SOURCES_PER_DESTINATION_TO_REPORT 10
set_global_assignment -name EXCLUDE_TPD_PATHS_LESS_THAN "0 ns"
set_global_assignment -name MISC_FILE "C:/Sprinter/src/altera/quartus/max/sp2_max.dpf"