 -- Copyright (C) 1991-2009 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCC           : Dedicated power pin, which MUST be connected to VCC.
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   For transceiver I/O banks (Bank 13, 14, 15, 16 and 17),
 --           	    connect each pin marked GND* either individually through a 10k Ohm resistor
 --           	    to GND or tie all pins together and connect through a single 10k Ohm resistor
 --           	    to GND.
 --           	    For non-transceiver I/O banks, connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 -- NON_MIGRATABLE: This pin cannot be migrated.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition
CHIP  "sp2_max"  ASSIGNED TO AN: EPM7128STC100-10

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
UNUSED55                     : 1         : input  : TTL               :         :           : N              
UNUSED72                     : 2         : input  : TTL               :         :           : N              
VCCIO                        : 3         : power  :                   : 5.0V    :           :                
TDI                          : 4         : input  : TTL               :         :           : N              
UNUSED70                     : 5         : input  : TTL               :         :           : N              
CMOS_AS                      : 6         : output : TTL               :         :           : Y              
UNUSED27                     : 7         : input  : TTL               :         :           : N              
WR_PDOS                      : 8         : output : TTL               :         :           : Y              
WD                           : 9         : input  : TTL               :         :           : Y              
WSTB                         : 10        : input  : TTL               :         :           : Y              
GND                          : 11        : gnd    :                   :         :           :                
TR43                         : 12        : input  : TTL               :         :           : Y              
CLK_WG                       : 13        : output : TTL               :         :           : Y              
FDAT                         : 14        : output : TTL               :         :           : Y              
TMS                          : 15        : input  : TTL               :         :           : N              
QDAT                         : 16        : output : TTL               :         :           : Y              
XA[0]                        : 17        : input  : TTL               :         :           : Y              
VCCIO                        : 18        : power  :                   : 5.0V    :           :                
SINC_2                       : 19        : bidir  : TTL               :         :           : Y              
SINC_1                       : 20        : bidir  : TTL               :         :           : Y              
XA[1]                        : 21        : input  : TTL               :         :           : Y              
UNUSED22                     : 22        : input  : TTL               :         :           : N              
XA[2]                        : 23        : input  : TTL               :         :           : Y              
UNUSED50                     : 24        : input  : TTL               :         :           : N              
RSTB                         : 25        : input  : TTL               :         :           : Y              
GND                          : 26        : gnd    :                   :         :           :                
UNUSED2                      : 27        : input  : TTL               :         :           : N              
UNUSED28                     : 28        : input  : TTL               :         :           : N              
SR                           : 29        : input  : TTL               :         :           : Y              
SL                           : 30        : input  : TTL               :         :           : Y              
CLK14                        : 31        : output : TTL               :         :           : Y              
CLKZZ                        : 32        : bidir  : TTL               :         :           : Y              
UNUSED33                     : 33        : input  : TTL               :         :           : Y              
VCCIO                        : 34        : power  :                   : 5.0V    :           :                
AUD                          : 35        : output : TTL               :         :           : Y              
TG42_BUF                     : 36        : output : TTL               :         :           : Y              
XACS                         : 37        : input  : TTL               :         :           : Y              
GND                          : 38        : gnd    :                   :         :           :                
VCCINT                       : 39        : power  :                   : 5.0V    :           :                
HDD_C[3]                     : 40        : input  : TTL               :         :           : Y              
HDD_C[2]                     : 41        : input  : TTL               :         :           : Y              
HDD_C[1]                     : 42        : input  : TTL               :         :           : Y              
GND                          : 43        : gnd    :                   :         :           :                
FDD_C[0]                     : 44        : input  : TTL               :         :           : Y              
FDD_C[1]                     : 45        : input  : TTL               :         :           : Y              
FDD_C[2]                     : 46        : input  : TTL               :         :           : Y              
HDD_C[0]                     : 47        : input  : TTL               :         :           : Y              
HD_DIR                       : 48        : output : TTL               :         :           : Y              
UNUSED49                     : 49        : input  : TTL               :         :           : N              
UNUSED1                      : 50        : input  : TTL               :         :           : N              
VCCIO                        : 51        : power  :                   : 5.0V    :           :                
HD_CS                        : 52        : output : TTL               :         :           : Y              
UNUSED53                     : 53        : input  : TTL               :         :           : Y              
/CONF_X                      : 54        : bidir  : TTL               :         :           : Y              
UNUSED63                     : 55        : input  : TTL               :         :           : N              
10K_CLK                      : 56        : output : TTL               :         :           : Y              
WR_CNF                       : 57        : input  : TTL               :         :           : Y              
10K_D0                       : 58        : output : TTL               :         :           : Y              
GND                          : 59        : gnd    :                   :         :           :                
D0                           : 60        : input  : TTL               :         :           : Y              
VGA_IN                       : 61        : input  : TTL               :         :           : Y              
TCK                          : 62        : input  : TTL               :         :           : N              
UNUSED77                     : 63        : input  : TTL               :         :           : N              
SINC_V                       : 64        : output : TTL               :         :           : Y              
UNUSED65                     : 65        : input  : TTL               :         :           : Y              
VCCIO                        : 66        : power  :                   : 5.0V    :           :                
SINC                         : 67        : output : TTL               :         :           : Y              
SINC_H                       : 68        : output : TTL               :         :           : Y              
SINC_IN                      : 69        : input  : TTL               :         :           : Y              
UNUSED24                     : 70        : input  : TTL               :         :           : N              
XHD_RES                      : 71        : output : TTL               :         :           : Y              
UNUSED5                      : 72        : input  : TTL               :         :           : N              
TDO                          : 73        : output : TTL               :         :           : N              
GND                          : 74        : gnd    :                   :         :           :                
XHD_WR                       : 75        : output : TTL               :         :           : Y              
XHD_RD                       : 76        : output : TTL               :         :           : Y              
UNUSED7                      : 77        : input  : TTL               :         :           : N              
UNUSED78                     : 78        : input  : TTL               :         :           : Y              
XHD1_CS[1]                   : 79        : output : TTL               :         :           : Y              
XHD1_CS[2]                   : 80        : output : TTL               :         :           : Y              
XHD2_CS[1]                   : 81        : output : TTL               :         :           : Y              
VCCIO                        : 82        : power  :                   : 5.0V    :           :                
XHD2_CS[2]                   : 83        : output : TTL               :         :           : Y              
BEEP                         : 84        : output : TTL               :         :           : Y              
TG42_OUT                     : 85        : output : TTL               :         :           : Y              
GND                          : 86        : gnd    :                   :         :           :                
TG42_IN                      : 87        : input  : TTL               :         :           : Y              
XHR_RDY                      : 88        : input  : TTL               :         :           : Y              
EPM_RES                      : 89        : input  : TTL               :         :           : Y              
PW_GOOD                      : 90        : input  : TTL               :         :           : Y              
VCCINT                       : 91        : power  :                   : 5.0V    :           :                
RDAT                         : 92        : input  : TTL               :         :           : Y              
/WG_WR                       : 93        : output : TTL               :         :           : Y              
STE                          : 94        : input  : TTL               :         :           : Y              
GND                          : 95        : gnd    :                   :         :           :                
DENS_X                       : 96        : output : TTL               :         :           : Y              
/WG_RD                       : 97        : output : TTL               :         :           : Y              
WDAT                         : 98        : output : TTL               :         :           : Y              
CMOS_DRD                     : 99        : output : TTL               :         :           : Y              
CMOS_DWR                     : 100       : output : TTL               :         :           : Y              
