# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition
# Date created = 22:21:41  July 29, 2025
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		divmmc_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY MAX3000A
set_global_assignment -name DEVICE "EPM3256ATC144-10"
set_global_assignment -name TOP_LEVEL_ENTITY divmmc
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "22:21:41  JULY 29, 2025"
set_global_assignment -name LAST_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name VHDL_FILE divmmc.vhd
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 144
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR "-1"
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name MAX7000_DEVICE_IO_STANDARD "3.3-V LVTTL"
set_location_assignment PIN_53 -to A[0]
set_location_assignment PIN_54 -to A[1]
set_location_assignment PIN_48 -to D[7]
set_location_assignment PIN_47 -to D[0]
set_location_assignment PIN_46 -to D[6]
set_location_assignment PIN_45 -to D[1]
set_location_assignment PIN_1 -to A[15]
set_location_assignment PIN_2 -to A[14]
set_location_assignment PIN_5 -to A[13]
set_location_assignment PIN_6 -to A[12]
set_location_assignment PIN_44 -to D[5]
set_location_assignment PIN_43 -to D[2]
set_location_assignment PIN_22 -to m1
set_location_assignment PIN_49 -to ramoe
set_location_assignment PIN_32 -to D[3]
set_location_assignment PIN_31 -to D[4]
set_location_assignment PIN_30 -to romoe
set_location_assignment PIN_18 -to romcs
set_location_assignment PIN_16 -to reset
set_location_assignment PIN_15 -to wr
set_location_assignment PIN_14 -to rd
set_location_assignment PIN_12 -to iorq
set_location_assignment PIN_90 -to bankout[2]
set_location_assignment PIN_96 -to card[1]
set_location_assignment PIN_97 -to card[0]
set_location_assignment PIN_55 -to A[10]
set_location_assignment PIN_56 -to A[2]
set_location_assignment PIN_61 -to A[3]
set_location_assignment PIN_62 -to A[11]
set_location_assignment PIN_63 -to A[4]
set_location_assignment PIN_65 -to A[9]
set_location_assignment PIN_98 -to spi_clock
set_location_assignment PIN_99 -to spi_dataout
set_location_assignment PIN_100 -to spi_datain
set_location_assignment PIN_81 -to bankout[1]
set_location_assignment PIN_68 -to A[6]
set_location_assignment PIN_80 -to romwr
set_location_assignment PIN_66 -to A[5]
set_location_assignment PIN_67 -to A[8]
set_location_assignment PIN_82 -to bankout[3]
set_location_assignment PIN_83 -to bankout[5]
set_location_assignment PIN_84 -to ramwr
set_location_assignment PIN_87 -to bankout[0]
set_location_assignment PIN_88 -to bankout[4]
set_location_assignment PIN_138 -to eprom
set_location_assignment PIN_137 -to poweron
set_location_assignment PIN_136 -to mapcondout
set_location_assignment PIN_75 -to A[7]
set_location_assignment PIN_125 -to clock
set_location_assignment PIN_36 -to mreq
set_global_assignment -name USE_CONFIGURATION_DEVICE ON
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"