# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition
# Date created = 00:30:12  January 12, 2026
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		Multi_Controller_IDE_FDD_SD_RTC_01_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY MAX7000S
set_global_assignment -name DEVICE "EPM7128STC100-7"
set_global_assignment -name TOP_LEVEL_ENTITY Multi_Controller_IDE_FDD_SD_RTC_01
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "00:30:12  MAY 12, 2026"
set_global_assignment -name LAST_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 100
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR "-1"
set_global_assignment -name AHDL_FILE Multi_Controller_IDE_FDD_SD_RTC_01.tdf
set_global_assignment -name MAX7000_DEVICE_IO_STANDARD "3.3-V LVTTL"
set_location_assignment PIN_47 -to CD[7]
set_location_assignment PIN_49 -to CD[0]
set_location_assignment PIN_50 -to CD[1]
set_location_assignment PIN_52 -to CD[2]
set_location_assignment PIN_60 -to CD[3]
set_location_assignment PIN_63 -to CD[4]
set_location_assignment PIN_57 -to CD[5]
set_location_assignment PIN_55 -to CD[6]
set_location_assignment PIN_92 -to SD_MISO
set_location_assignment PIN_93 -to SD_SCK
set_location_assignment PIN_94 -to SD_MOSI
set_location_assignment PIN_96 -to SD_CS[0]
set_location_assignment PIN_35 -to GLOBAL_CLK
set_location_assignment PIN_41 -to C_IORQGE
set_location_assignment PIN_77 -to C_M1
set_location_assignment PIN_69 -to C_MREQ
set_location_assignment PIN_71 -to C_RD
set_location_assignment PIN_75 -to C_RESET
set_location_assignment PIN_72 -to C_WR
set_location_assignment PIN_70 -to C_IORQ
set_location_assignment PIN_54 -to BUS_A[0]
set_location_assignment PIN_56 -to BUS_A[1]
set_location_assignment PIN_58 -to BUS_A[2]
set_location_assignment PIN_61 -to BUS_A[3]
set_location_assignment PIN_87 -to BUS_A[4]
set_location_assignment PIN_42 -to BUS_A[14]
set_location_assignment PIN_44 -to BUS_A[13]
set_location_assignment PIN_45 -to BUS_A[12]
set_location_assignment PIN_46 -to BUS_A[11]
set_location_assignment PIN_90 -to BUS_A[10]
set_location_assignment PIN_89 -to BUS_A[9]
set_location_assignment PIN_88 -to BUS_A[8]
set_location_assignment PIN_64 -to BUS_A[7]
set_location_assignment PIN_76 -to BUS_A[6]
set_location_assignment PIN_67 -to BUS_A[5]
set_location_assignment PIN_33 -to pin33_NOT_USED
set_location_assignment PIN_53 -to pin53_NOT_USED
set_location_assignment PIN_65 -to pin65_NOT_USED
set_location_assignment PIN_78 -to pin78_NOT_USED
set_location_assignment PIN_85 -to BT_MAGIC
set_location_assignment PIN_84 -to SW_Z_PAGE
set_location_assignment PIN_80 -to SW_SD
set_location_assignment PIN_81 -to SW_IDE
set_location_assignment PIN_83 -to SW_DOS
set_location_assignment PIN_13 -to VG93_TR43
set_location_assignment PIN_12 -to VG93_DRQ
set_location_assignment PIN_10 -to VG93_INRQ
set_location_assignment PIN_9 -to VG93_SL
set_location_assignment PIN_8 -to VG93_S
set_location_assignment PIN_7 -to VG93_SR
set_location_assignment PIN_6 -to VG93_RAWR
set_location_assignment PIN_5 -to VG93_CLK
set_location_assignment PIN_2 -to VG93_RES
set_location_assignment PIN_97 -to FDD_SEL_A
set_location_assignment PIN_98 -to FDD_SEL_B
set_location_assignment PIN_14 -to VG93_WD
set_location_assignment PIN_99 -to FDD_SIDE
set_location_assignment PIN_16 -to VG93_WF/DE
set_location_assignment PIN_1 -to FDD_WRD
set_location_assignment PIN_32 -to FDD_RDD
set_location_assignment PIN_100 -to VG93_HRDY
set_location_assignment PIN_25 -to IDE_HDD[15]
set_location_assignment PIN_24 -to IDE_HDD[14]
set_location_assignment PIN_23 -to IDE_HDD[13]
set_location_assignment PIN_22 -to IDE_HDD[12]
set_location_assignment PIN_21 -to IDE_HDD[11]
set_location_assignment PIN_20 -to IDE_HDD[10]
set_location_assignment PIN_19 -to IDE_HDD[9]
set_location_assignment PIN_17 -to IDE_HDD[8]
set_location_assignment PIN_30 -to IDE_IOW
set_location_assignment PIN_37 -to IDE_IOR
set_location_assignment PIN_36 -to IDE_EBL
set_location_assignment PIN_29 -to RTC_AS
set_location_assignment PIN_27 -to RTC_DS
set_location_assignment PIN_28 -to RTC_RW
set_location_assignment PIN_48 -to C_DOS
set_location_assignment PIN_40 -to C_RS
set_location_assignment PIN_68 -to C_NMI
set_location_assignment PIN_79 -to RTC_CS
set_location_assignment PIN_31 -to VG93_IOFDC
set_global_assignment -name OPTIMIZE_HOLD_TIMING OFF
set_global_assignment -name OPTIMIZE_MULTI_CORNER_TIMING OFF
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
set_global_assignment -name BDF_FILE Multi_Controller_IDE_FDD_SD_RTC_01.bdf
set_global_assignment -name USE_CONFIGURATION_DEVICE ON
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85