 -- Copyright (C) 1991-2013 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCC           : Dedicated power pin, which MUST be connected to VCC.
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin. Connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 -- NON_MIGRATABLE: This pin cannot be migrated.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II 64-Bit Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition
CHIP  "Multi_Controller_IDE_FDD_SD_RTC_01"  ASSIGNED TO AN: EPM7128STC100-7

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
FDD_WRD                      : 1         : output : 3.3-V LVTTL       :         :           : Y              
VG93_RES                     : 2         : output : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 3         : power  :                   : 3.3V    :           :                
TDI                          : 4         : input  : 3.3-V LVTTL       :         :           : N              
VG93_CLK                     : 5         : output : 3.3-V LVTTL       :         :           : Y              
VG93_RAWR                    : 6         : output : 3.3-V LVTTL       :         :           : Y              
VG93_SR                      : 7         : input  : 3.3-V LVTTL       :         :           : Y              
VG93_S                       : 8         : output : 3.3-V LVTTL       :         :           : Y              
VG93_SL                      : 9         : input  : 3.3-V LVTTL       :         :           : Y              
VG93_INRQ                    : 10        : input  : 3.3-V LVTTL       :         :           : Y              
GND                          : 11        : gnd    :                   :         :           :                
VG93_DRQ                     : 12        : input  : 3.3-V LVTTL       :         :           : Y              
VG93_TR43                    : 13        : input  : 3.3-V LVTTL       :         :           : Y              
VG93_WD                      : 14        : input  : 3.3-V LVTTL       :         :           : Y              
TMS                          : 15        : input  : 3.3-V LVTTL       :         :           : N              
VG93_WF/DE                   : 16        : input  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[8]                   : 17        : bidir  : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 18        : power  :                   : 3.3V    :           :                
IDE_HDD[9]                   : 19        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[10]                  : 20        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[11]                  : 21        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[12]                  : 22        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[13]                  : 23        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[14]                  : 24        : bidir  : 3.3-V LVTTL       :         :           : Y              
IDE_HDD[15]                  : 25        : bidir  : 3.3-V LVTTL       :         :           : Y              
GND                          : 26        : gnd    :                   :         :           :                
RTC_DS                       : 27        : output : 3.3-V LVTTL       :         :           : Y              
RTC_RW                       : 28        : output : 3.3-V LVTTL       :         :           : Y              
RTC_AS                       : 29        : output : 3.3-V LVTTL       :         :           : Y              
IDE_IOW                      : 30        : output : 3.3-V LVTTL       :         :           : Y              
VG93_IOFDC                   : 31        : output : 3.3-V LVTTL       :         :           : Y              
FDD_RDD                      : 32        : input  : 3.3-V LVTTL       :         :           : Y              
pin33_NOT_USED               : 33        : input  : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 34        : power  :                   : 3.3V    :           :                
GLOBAL_CLK                   : 35        : input  : 3.3-V LVTTL       :         :           : Y              
IDE_EBL                      : 36        : output : 3.3-V LVTTL       :         :           : Y              
IDE_IOR                      : 37        : output : 3.3-V LVTTL       :         :           : Y              
GND                          : 38        : gnd    :                   :         :           :                
VCCINT                       : 39        : power  :                   : 5.0V    :           :                
C_RS                         : 40        : input  : 3.3-V LVTTL       :         :           : Y              
C_IORQGE                     : 41        : output : 3.3-V LVTTL       :         :           : Y              
BUS_A[14]                    : 42        : input  : 3.3-V LVTTL       :         :           : Y              
GND                          : 43        : gnd    :                   :         :           :                
BUS_A[13]                    : 44        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[12]                    : 45        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[11]                    : 46        : input  : 3.3-V LVTTL       :         :           : Y              
CD[7]                        : 47        : bidir  : 3.3-V LVTTL       :         :           : Y              
C_DOS                        : 48        : bidir  : 3.3-V LVTTL       :         :           : Y              
CD[0]                        : 49        : bidir  : 3.3-V LVTTL       :         :           : Y              
CD[1]                        : 50        : bidir  : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 51        : power  :                   : 3.3V    :           :                
CD[2]                        : 52        : bidir  : 3.3-V LVTTL       :         :           : Y              
pin53_NOT_USED               : 53        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[0]                     : 54        : input  : 3.3-V LVTTL       :         :           : Y              
CD[6]                        : 55        : bidir  : 3.3-V LVTTL       :         :           : Y              
BUS_A[1]                     : 56        : input  : 3.3-V LVTTL       :         :           : Y              
CD[5]                        : 57        : bidir  : 3.3-V LVTTL       :         :           : Y              
BUS_A[2]                     : 58        : input  : 3.3-V LVTTL       :         :           : Y              
GND                          : 59        : gnd    :                   :         :           :                
CD[3]                        : 60        : bidir  : 3.3-V LVTTL       :         :           : Y              
BUS_A[3]                     : 61        : input  : 3.3-V LVTTL       :         :           : Y              
TCK                          : 62        : input  : 3.3-V LVTTL       :         :           : N              
CD[4]                        : 63        : bidir  : 3.3-V LVTTL       :         :           : Y              
BUS_A[7]                     : 64        : input  : 3.3-V LVTTL       :         :           : Y              
pin65_NOT_USED               : 65        : input  : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 66        : power  :                   : 3.3V    :           :                
BUS_A[5]                     : 67        : input  : 3.3-V LVTTL       :         :           : Y              
C_NMI                        : 68        : output : 3.3-V LVTTL       :         :           : Y              
C_MREQ                       : 69        : input  : 3.3-V LVTTL       :         :           : Y              
C_IORQ                       : 70        : input  : 3.3-V LVTTL       :         :           : Y              
C_RD                         : 71        : input  : 3.3-V LVTTL       :         :           : Y              
C_WR                         : 72        : input  : 3.3-V LVTTL       :         :           : Y              
TDO                          : 73        : output : 3.3-V LVTTL       :         :           : N              
GND                          : 74        : gnd    :                   :         :           :                
C_RESET                      : 75        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[6]                     : 76        : input  : 3.3-V LVTTL       :         :           : Y              
C_M1                         : 77        : input  : 3.3-V LVTTL       :         :           : Y              
pin78_NOT_USED               : 78        : input  : 3.3-V LVTTL       :         :           : Y              
RTC_CS                       : 79        : output : 3.3-V LVTTL       :         :           : Y              
SW_SD                        : 80        : input  : 3.3-V LVTTL       :         :           : Y              
SW_IDE                       : 81        : input  : 3.3-V LVTTL       :         :           : Y              
VCCIO                        : 82        : power  :                   : 3.3V    :           :                
SW_DOS                       : 83        : input  : 3.3-V LVTTL       :         :           : Y              
SW_Z_PAGE                    : 84        : input  : 3.3-V LVTTL       :         :           : Y              
BT_MAGIC                     : 85        : input  : 3.3-V LVTTL       :         :           : Y              
GND                          : 86        : gnd    :                   :         :           :                
BUS_A[4]                     : 87        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[8]                     : 88        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[9]                     : 89        : input  : 3.3-V LVTTL       :         :           : Y              
BUS_A[10]                    : 90        : input  : 3.3-V LVTTL       :         :           : Y              
VCCINT                       : 91        : power  :                   : 5.0V    :           :                
SD_MISO                      : 92        : input  : 3.3-V LVTTL       :         :           : Y              
SD_SCK                       : 93        : output : 3.3-V LVTTL       :         :           : Y              
SD_MOSI                      : 94        : output : 3.3-V LVTTL       :         :           : Y              
GND                          : 95        : gnd    :                   :         :           :                
SD_CS[0]                     : 96        : output : 3.3-V LVTTL       :         :           : Y              
FDD_SEL_A                    : 97        : output : 3.3-V LVTTL       :         :           : Y              
FDD_SEL_B                    : 98        : output : 3.3-V LVTTL       :         :           : Y              
FDD_SIDE                     : 99        : output : 3.3-V LVTTL       :         :           : Y              
VG93_HRDY                    : 100       : output : 3.3-V LVTTL       :         :           : Y              
