# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 64-Bit
# Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Full Version
# Date created = 12:04:27  October 04, 2020
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		zx_multisound_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY MAX3000A
set_global_assignment -name DEVICE "EPM3256ATC144-10"
set_global_assignment -name TOP_LEVEL_ENTITY zx_multisound
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "12:04:27  OCTOBER 04, 2020"
set_global_assignment -name LAST_QUARTUS_VERSION "13.0 SP1"
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 144
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR "-1"
set_global_assignment -name SDC_FILE clocks.sdc
set_global_assignment -name VERILOG_FILE ../rtl/top.v
set_global_assignment -name VHDL_INPUT_VERSION VHDL_2008
set_global_assignment -name VHDL_SHOW_LMF_MAPPING_MESSAGES OFF
set_global_assignment -name VERILOG_INPUT_VERSION SYSTEMVERILOG_2005
set_global_assignment -name VERILOG_SHOW_LMF_MAPPING_MESSAGES OFF
set_global_assignment -name MAX7000_DEVICE_IO_STANDARD "3.3-V LVTTL"
set_global_assignment -name SAVE_DISK_SPACE OFF
set_global_assignment -name TIMEQUEST_MULTICORNER_ANALYSIS OFF
set_global_assignment -name SYNTH_TIMING_DRIVEN_SYNTHESIS OFF
set_location_assignment PIN_2 -to n_gram2
set_location_assignment PIN_5 -to gma[17]
set_location_assignment PIN_6 -to gma[16]
set_location_assignment PIN_7 -to gma[18]
set_location_assignment PIN_8 -to n_gram1
set_location_assignment PIN_9 -to n_gm1
set_location_assignment PIN_10 -to n_grst
set_location_assignment PIN_11 -to ga[0]
set_location_assignment PIN_12 -to ga[1]
set_location_assignment PIN_14 -to ga[2]
set_location_assignment PIN_15 -to ga[3]
set_location_assignment PIN_16 -to ga[4]
set_location_assignment PIN_18 -to ga[5]
set_location_assignment PIN_19 -to ga[6]
set_location_assignment PIN_21 -to ga[7]
set_location_assignment PIN_22 -to ga[8]
set_location_assignment PIN_23 -to ga[9]
set_location_assignment PIN_25 -to ga[10]
set_location_assignment PIN_27 -to n_gwr
set_location_assignment PIN_28 -to n_grd
set_location_assignment PIN_29 -to n_giorq
set_location_assignment PIN_30 -to n_gmreq
set_location_assignment PIN_31 -to ga[11]
set_location_assignment PIN_32 -to ga[12]
set_location_assignment PIN_34 -to ga[13]
set_location_assignment PIN_35 -to ga[14]
set_location_assignment PIN_36 -to ga[15]
set_location_assignment PIN_37 -to gd[3]
set_location_assignment PIN_38 -to gd[5]
set_location_assignment PIN_39 -to gd[6]
set_location_assignment PIN_40 -to gd[2]
set_location_assignment PIN_41 -to gd[7]
set_location_assignment PIN_42 -to gd[4]
set_location_assignment PIN_43 -to gclk
set_location_assignment PIN_44 -to n_gint
set_location_assignment PIN_45 -to gd[0]
set_location_assignment PIN_46 -to gd[1]
set_location_assignment PIN_47 -to n_grom
set_location_assignment PIN_48 -to gma[15]
set_location_assignment PIN_49 -to cfg[0]
set_location_assignment PIN_53 -to cfg[1]
set_location_assignment PIN_54 -to cfg[2]
set_location_assignment PIN_55 -to cfg[3]
set_location_assignment PIN_56 -to cfg[4]
set_location_assignment PIN_60 -to dac3_out
set_location_assignment PIN_61 -to dac2_out
set_location_assignment PIN_62 -to dac1_out
set_location_assignment PIN_63 -to dac0_out
set_location_assignment PIN_69 -to ym_m
set_location_assignment PIN_70 -to fm1_ena
set_location_assignment PIN_74 -to aa0
set_location_assignment PIN_75 -to n_ard
set_location_assignment PIN_78 -to n_awr
set_location_assignment PIN_79 -to n_ym1_cs
set_location_assignment PIN_80 -to n_ym2_cs
set_location_assignment PIN_81 -to n_rstout
set_location_assignment PIN_82 -to fm2_ena
set_location_assignment PIN_83 -to ad[0]
set_location_assignment PIN_84 -to ad[1]
set_location_assignment PIN_86 -to ad[2]
set_location_assignment PIN_87 -to ad[3]
set_location_assignment PIN_88 -to ad[4]
set_location_assignment PIN_90 -to ad[5]
set_location_assignment PIN_91 -to ad[6]
set_location_assignment PIN_92 -to ad[7]
set_location_assignment PIN_93 -to n_saa_cs
set_location_assignment PIN_96 -to saa_clk
set_location_assignment PIN_97 -to midi_clk
set_location_assignment PIN_98 -to a[14]
set_location_assignment PIN_99 -to a[15]
set_location_assignment PIN_100 -to a[12]
set_location_assignment PIN_101 -to a[13]
set_location_assignment PIN_102 -to d[7]
set_location_assignment PIN_103 -to d[0]
set_location_assignment PIN_106 -to d[1]
set_location_assignment PIN_107 -to d[2]
set_location_assignment PIN_108 -to n_dos
set_location_assignment PIN_109 -to a[0]
set_location_assignment PIN_110 -to d[6]
set_location_assignment PIN_111 -to a[1]
set_location_assignment PIN_112 -to d[5]
set_location_assignment PIN_113 -to a[2]
set_location_assignment PIN_116 -to d[3]
set_location_assignment PIN_117 -to a[3]
set_location_assignment PIN_118 -to d[4]
set_location_assignment PIN_119 -to n_iorqge
set_location_assignment PIN_120 -to n_mreq
set_location_assignment PIN_121 -to n_iorq
set_location_assignment PIN_122 -to n_rd
set_location_assignment PIN_125 -to clkx
set_location_assignment PIN_126 -to n_wr
set_location_assignment PIN_127 -to rst_n
set_location_assignment PIN_128 -to clk32
set_location_assignment PIN_131 -to n_iodos
set_location_assignment PIN_132 -to n_wait
set_location_assignment PIN_133 -to a[7]
set_location_assignment PIN_134 -to a[6]
set_location_assignment PIN_136 -to a[5]
set_location_assignment PIN_137 -to n_m1
set_location_assignment PIN_138 -to a[4]
set_location_assignment PIN_139 -to a[8]
set_location_assignment PIN_140 -to a[9]
set_location_assignment PIN_141 -to a[10]
set_location_assignment PIN_142 -to a[11]
set_global_assignment -name MAX7000_OPTIMIZATION_TECHNIQUE BALANCED
set_global_assignment -name PRE_MAPPING_RESYNTHESIS OFF
set_global_assignment -name OPTIMIZE_HOLD_TIMING OFF
set_global_assignment -name OPTIMIZE_MULTI_CORNER_TIMING ON
set_global_assignment -name FITTER_EFFORT "STANDARD FIT"
set_global_assignment -name RESERVE_ALL_UNUSED_PINS_NO_OUTPUT_GND "AS INPUT TRI-STATED"
