(footprint "HDR-TH_12P-P2.54-V-M"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "12-Штырьковый разъем, папа")
	(property "Reference" "XP?"
		(at 0.0508 -2.413 180)
		(layer "F.SilkS")
		(uuid "88fc269a-ff35-455e-9422-2e3a88c1bc28")
		(effects
			(font
				(size 1.016 1.016)
				(thickness 0.127)
			)
			(justify bottom)
		)
	)
	(property "Value" "Value"
		(at 0 1.905 0)
		(layer "F.SilkS")
		(uuid "549e48ed-22f0-4e83-8cd1-a6b2ca1b259a")
		(effects
			(font
				(size 1.016 1.016)
				(thickness 0.127)
			)
			(justify top)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(layer "B.Fab")
		(hide yes)
		(uuid "68d65570-1f65-4bf6-add0-d9014d875d2c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(layer "B.Fab")
		(hide yes)
		(uuid "72abd884-7e07-4677-aab0-9de3b0d563e9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
			(justify mirror)
		)
	)
	(fp_line
		(start -15.24 -1.27)
		(end -15.24 1.27)
		(stroke
			(width 0.2032)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dbbad495-3323-4df8-bf39-3a1c523f2074")
	)
	(fp_line
		(start -15.24 -1.27)
		(end 15.24 -1.27)
		(stroke
			(width 0.2032)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3c5cb654-2257-4076-aea1-449155a59631")
	)
	(fp_line
		(start -15.24 1.27)
		(end 15.24 1.27)
		(stroke
			(width 0.2032)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2e99c202-0644-4904-a3e3-a80a2e1d8803")
	)
	(fp_line
		(start 15.24 -1.27)
		(end 15.24 1.27)
		(stroke
			(width 0.2032)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d3f67b95-65a7-4d84-af28-81073a5d6985")
	)
	(fp_rect
		(start -15.24 -1.27)
		(end 15.24 1.27)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "03ff1a6e-74d4-4aad-b6a6-93c868610705")
	)
	(fp_circle
		(center -13.9702 0)
		(end -13.7576 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "e2cd0e59-37c5-4534-a6c4-01cbcddd447b")
	)
	(fp_circle
		(center -11.4302 0)
		(end -11.2176 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "75404ca7-0982-4f96-a4ba-5f10f7059ffd")
	)
	(fp_circle
		(center -8.8902 0)
		(end -8.6776 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "f4e33a1e-bcf0-429f-8764-774373b8325f")
	)
	(fp_circle
		(center -6.3502 0)
		(end -6.1376 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "af1a9e74-58a2-4812-983f-c3bfa889709e")
	)
	(fp_circle
		(center -3.8102 0)
		(end -3.5976 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "0f99d787-39a2-4031-893a-ffd95af7684a")
	)
	(fp_circle
		(center -1.2702 0)
		(end -1.0576 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "6ee14c81-c8f6-4c09-9354-1b6a2d31cffa")
	)
	(fp_circle
		(center 1.2698 0)
		(end 1.4824 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "0dba25a7-afa6-4835-bee7-0ea8f52db423")
	)
	(fp_circle
		(center 3.8098 0)
		(end 4.0224 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "81932f10-fd15-4231-975d-1d044d64d074")
	)
	(fp_circle
		(center 6.3498 0)
		(end 6.5624 0)
		(stroke
			(width 0.425)
			(type default)
		)
		(fill no)
		(layer "User.4")
		(uuid "ca3c9ea5-6ee0-4769-81d8-dfad3d310d67")
	)
	(fp_circle
		(center -15.3672 1.397)
		(end -15.3372 1.397)
		(stroke
			(width 0.06)
			(type default)
		)
		(fill no)
		(layer "User.5")
		(uuid "99cd1266-efb1-485b-ac2b-2e7fbe90bbe2")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "f72eccbd-bfa6-4482-89b4-d0adbd90c8a3")
		(effects
			(font
				(size 1.016 1.016)
				(thickness 0.127)
			)
		)
	)
	(pad "1" thru_hole rect
		(at -13.9702 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "27b37459-1333-4bdb-9f3f-907e00c0359c")
	)
	(pad "2" thru_hole circle
		(at -11.4302 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "28106bb2-cc83-42dd-be42-02fa95028e12")
	)
	(pad "3" thru_hole circle
		(at -8.8902 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "14fd7fa4-367a-4184-9fe8-96e4cbe50ff4")
	)
	(pad "4" thru_hole circle
		(at -6.3502 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "fa6a035b-b06c-4b40-a327-84b5a26df197")
	)
	(pad "5" thru_hole circle
		(at -3.8102 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "2f07295d-7b8b-4723-8842-fefc63f8078a")
	)
	(pad "6" thru_hole circle
		(at -1.2702 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "ef761d6e-e80e-4313-ae1e-f5a6598511bb")
	)
	(pad "7" thru_hole circle
		(at 1.2698 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "f07ec165-fda7-4ec2-95fd-40557af67af2")
	)
	(pad "8" thru_hole circle
		(at 3.8098 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "f4d80297-eb20-406c-89c9-4907d0adced6")
	)
	(pad "9" thru_hole circle
		(at 6.3498 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "82477d2e-1e03-46cc-aa4c-6abb28cdd2a9")
	)
	(pad "10" thru_hole circle
		(at 8.89 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "ed8d61b9-8cfb-412e-bff8-33b24bb7842b")
	)
	(pad "11" thru_hole circle
		(at 11.43 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "1e0a34cf-70ed-4429-be28-a8d184078548")
	)
	(pad "12" thru_hole circle
		(at 13.97 0 180)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0508)
		(solder_paste_margin 0)
		(thermal_bridge_angle 0)
		(uuid "b276e469-b125-4ce5-8895-6a6b9c68c9da")
	)
	(embedded_fonts no)
	(model "${KICAD9_3RD_PARTY}/HDR-12P-M-P2.54.step"
		(offset
			(xyz -13.97 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -180 -0 -0)
		)
	)
)
