(footprint "M.2 Mounting Pad"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.82 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8b2e1c62-1f10-4651-9f2d-cc0756985f42")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "M.2 Mounting Pad"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2cc7b09f-9586-4c34-8903-9fb5ccdd4c08")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "191dc3c0-f422-4ff8-84ec-4a825593b916")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0bf31a89-78ec-4dd8-9ab3-913f7857014c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "9f188612-bdd0-4cb4-9579-ba791c3cb90a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 5.5 5.5)
		(drill 3.5)
		(property pad_prop_castellated)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "cc590ad5-81d2-46aa-b4dc-4b10a598f102")
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 5.5 5.5)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape oval)
				(size 6 8)
				(thermal_bridge_angle 45)
				(zone_connect -1)
			)
		)
	)
	(embedded_fonts no)
)
