Project Information              c:\prj\sprinter\firmware\97\flex\sprint08.rpt

MAX+plus II Compiler Report File
Version 10.0 9/14/2000
Compiled: 08/05/2024 19:36:00

Copyright (C) 1988-2000 Altera Corporation
Any megafunction design, and related net list (encrypted or decrypted),
support information, device programming or simulation file, and any other
associated documentation or information provided by Altera or a partner
under Altera's Megafunction Partnership Program may be used only to
program PLD devices (but not masked PLD devices) from Altera.  Any other
use of such megafunction design, net list, support information, device
programming or simulation file, or any other related documentation or
information is prohibited for any other purpose, including, but not
limited to modification, reverse engineering, de-compiling, or use with
any other silicon devices, unless such use is explicitly licensed under
a separate agreement with Altera or a megafunction partner.  Title to
the intellectual property, including patents, copyrights, trademarks,
trade secrets, or maskworks, embodied in any such megafunction design,
net list, support information, device programming or simulation file, or
any other related documentation or information provided by Altera or a
megafunction partner, remains with Altera, the megafunction partner, or
their respective licensors.  No other licenses, including any licenses
needed under any third party's intellectual property, are provided herein.



***** Project compilation was successful


Sprinter_97


** DEVICE SUMMARY **

Chip/                     Input Output Bidir  Memory  Memory  			 LCs
POF       Device          Pins  Pins   Pins   Bits % Utilized  LCs  % Utilized

sprint08  EPF10K10QC208-3  8      55     70   6144      100%    567      98 %

User Pins:                 8      55     70 



Project Information              c:\prj\sprinter\firmware\97\flex\sprint08.rpt

** PROJECT COMPILATION MESSAGES **

Warning: Line 375, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "MC" was declared but never used
Warning: Line 271, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "MS_MOUSE" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD4" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO4" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO14" was declared but never used
Warning: Line 589, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FN_ACC2" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF7" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD5" was declared but never used
Warning: Line 311, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC5" was declared but never used
Warning: Line 643, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC0_X" was declared but never used
Warning: Line 586, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RASX" was declared but never used
Warning: Line 565, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "AY_DRD" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF6" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD6" was declared but never used
Warning: Line 311, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC6" was declared but never used
Warning: Line 336, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "VLAB17" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD7" was declared but never used
Warning: Line 311, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC7" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO9" was declared but never used
Warning: Line 336, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "VLAB16" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO8" was declared but never used
Warning: Line 458, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SND_A_LD" was declared but never used
Warning: Line 336, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "VLAB15" was declared but never used
Warning: Line 301, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FIN0" was declared but never used
Warning: Line 348, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "WR_MODE2X" was declared but never used
Warning: Line 602, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RBRVA10" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO3" was declared but never used
Warning: Line 336, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "VLAB14" was declared but never used
Warning: Line 453, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SND_TEST" was declared but never used
Warning: Line 311, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC2" was declared but never used
Warning: Line 301, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FIN1" was declared but never used
Warning: Line 500, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CB_CMD" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO2" was declared but never used
Warning: Line 503, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "ID_CMD" was declared but never used
Warning: Line 311, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "SC3" was declared but never used
Warning: Line 301, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FIN2" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF1" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO1" was declared but never used
Warning: Line 477, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "COV_BL_X2" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO11" was declared but never used
Warning: Line 316, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "BRD6" was declared but never used
Warning: Line 301, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FIN3" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF0" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO0" was declared but never used
Warning: Line 477, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "COV_BL_X1" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO10" was declared but never used
Warning: Line 621, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "COV_AR6" was declared but never used
Warning: Line 316, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "BRD7" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD1" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO7" was declared but never used
Warning: Line 477, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "COV_BL_X0" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO13" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF2" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD2" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO6" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO12" was declared but never used
Warning: Line 611, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "ASS_DIR7" was declared but never used
Warning: Line 418, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "CNF5" was declared but never used
Warning: Line 444, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "LWR_MODE2" was declared but never used
Warning: Line 391, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "RGMOD3" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO5" was declared but never used
Warning: Line 656, File c:\prj\sprinter\firmware\97\flex\sprint08.tdf:
   Symbolic name "FDO15" was declared but never used
Warning: I/O error -- can't read initial memory content file 'PGA_INI4.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'PGA_INI4.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'KBD_INI2.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'SND_INI.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'AY.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'AY.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'COVOX.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'COVOX.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'COVOX.MIF'-- setting all initial values to 0
Warning: I/O error -- can't read initial memory content file 'FORTH.MIF'-- setting all initial values to 0
Warning: Flipflop 'ACC_END' stuck at VCC
Warning: Flipflop 'PN7' stuck at GND
Warning: Flipflop 'PN6' stuck at GND
Warning: Flipflop 'KBDR2' stuck at GND
Warning: Flipflop 'KBDR1' stuck at GND
Warning: Flipflop 'AGR6' stuck at GND
Warning: Flipflop 'AGR7' stuck at GND
Warning: Flipflop 'KBDR0' stuck at GND
Warning: Flipflop ':637' stuck at VCC
Warning: Flipflop ':638' stuck at GND
Warning: TRI or OPNDRN buffer ':1900' is permanently disabled
Warning: TRI or OPNDRN buffer ':1911' is permanently disabled
Warning: TRI or OPNDRN buffer ':1912' is permanently disabled
Warning: TRI or OPNDRN buffer ':1908' is permanently disabled
Warning: TRI or OPNDRN buffer ':1907' is permanently disabled
Warning: TRI or OPNDRN buffer ':1909' is permanently disabled
Warning: TRI or OPNDRN buffer ':1910' is permanently disabled
Warning: TRI or OPNDRN buffer ':1914' is permanently disabled
Warning: TRI or OPNDRN buffer ':1913' is permanently disabled
Warning: TRI or OPNDRN buffer ':1905' is permanently disabled
Warning: TRI or OPNDRN buffer ':2016' is permanently disabled
Warning: TRI or OPNDRN buffer ':2017' is permanently disabled
Warning: TRI or OPNDRN buffer ':1906' is permanently disabled
Warning: TRI or OPNDRN buffer ':1904' is permanently disabled
Warning: TRI or OPNDRN buffer ':1915' is permanently disabled
Warning: TRI or OPNDRN buffer ':1903' is permanently disabled
Warning: TRI or OPNDRN buffer ':1902' is permanently disabled
Warning: TRI or OPNDRN buffer ':1901' is permanently disabled
Warning: TRI or OPNDRN buffer ':2010' is permanently disabled
Warning: TRI or OPNDRN buffer ':2004' is permanently disabled
Warning: TRI or OPNDRN buffer ':1998' is permanently disabled
Warning: TRI or OPNDRN buffer ':1992' is permanently disabled
Warning: TRI or OPNDRN buffer ':1986' is permanently disabled
Warning: TRI or OPNDRN buffer ':1980' is permanently disabled
Warning: TRI or OPNDRN buffer ':1974' is permanently disabled
Warning: TRI or OPNDRN buffer ':1968' is permanently disabled
Warning: TRI or OPNDRN buffer ':2011' is permanently disabled
Warning: TRI or OPNDRN buffer ':2005' is permanently disabled
Warning: TRI or OPNDRN buffer ':1999' is permanently disabled
Warning: TRI or OPNDRN buffer ':1993' is permanently disabled
Warning: TRI or OPNDRN buffer ':1987' is permanently disabled
Warning: TRI or OPNDRN buffer ':1981' is permanently disabled
Warning: TRI or OPNDRN buffer ':1975' is permanently disabled
Warning: TRI or OPNDRN buffer ':1969' is permanently disabled
Warning: TRI or OPNDRN buffer ':2012' is permanently disabled
Warning: TRI or OPNDRN buffer ':2006' is permanently disabled
Warning: TRI or OPNDRN buffer ':2000' is permanently disabled
Warning: TRI or OPNDRN buffer ':1994' is permanently disabled
Warning: TRI or OPNDRN buffer ':1988' is permanently disabled
Warning: TRI or OPNDRN buffer ':1982' is permanently disabled
Warning: TRI or OPNDRN buffer ':1976' is permanently disabled
Warning: TRI or OPNDRN buffer ':1970' is permanently disabled
Warning: TRI or OPNDRN buffer ':1900' is permanently disabled
Warning: TRI or OPNDRN buffer ':1911' is permanently disabled
Warning: TRI or OPNDRN buffer ':1912' is permanently disabled
Warning: TRI or OPNDRN buffer ':1908' is permanently disabled
Warning: TRI or OPNDRN buffer ':1907' is permanently disabled
Warning: TRI or OPNDRN buffer ':1909' is permanently disabled
Warning: TRI or OPNDRN buffer ':1910' is permanently disabled
Warning: TRI or OPNDRN buffer ':1914' is permanently disabled
Warning: TRI or OPNDRN buffer ':1913' is permanently disabled
Warning: TRI or OPNDRN buffer ':1905' is permanently disabled
Warning: TRI or OPNDRN buffer ':2016' is permanently disabled
Warning: TRI or OPNDRN buffer ':2017' is permanently disabled
Warning: TRI or OPNDRN buffer ':1906' is permanently disabled
Warning: TRI or OPNDRN buffer ':1904' is permanently disabled
Warning: TRI or OPNDRN buffer ':1915' is permanently disabled
Warning: TRI or OPNDRN buffer ':1903' is permanently disabled
Warning: TRI or OPNDRN buffer ':1902' is permanently disabled
Warning: TRI or OPNDRN buffer ':1901' is permanently disabled
Warning: TRI or OPNDRN buffer ':2010' is permanently disabled
Warning: TRI or OPNDRN buffer ':2004' is permanently disabled
Warning: TRI or OPNDRN buffer ':1998' is permanently disabled
Warning: TRI or OPNDRN buffer ':1992' is permanently disabled
Warning: TRI or OPNDRN buffer ':1986' is permanently disabled
Warning: TRI or OPNDRN buffer ':1980' is permanently disabled
Warning: TRI or OPNDRN buffer ':1974' is permanently disabled
Warning: TRI or OPNDRN buffer ':1968' is permanently disabled
Warning: TRI or OPNDRN buffer ':2011' is permanently disabled
Warning: TRI or OPNDRN buffer ':2005' is permanently disabled
Warning: TRI or OPNDRN buffer ':1999' is permanently disabled
Warning: TRI or OPNDRN buffer ':1993' is permanently disabled
Warning: TRI or OPNDRN buffer ':1987' is permanently disabled
Warning: TRI or OPNDRN buffer ':1981' is permanently disabled
Warning: TRI or OPNDRN buffer ':1975' is permanently disabled
Warning: TRI or OPNDRN buffer ':1969' is permanently disabled
Warning: TRI or OPNDRN buffer ':2012' is permanently disabled
Warning: TRI or OPNDRN buffer ':2006' is permanently disabled
Warning: TRI or OPNDRN buffer ':2000' is permanently disabled
Warning: TRI or OPNDRN buffer ':1994' is permanently disabled
Warning: TRI or OPNDRN buffer ':1988' is permanently disabled
Warning: TRI or OPNDRN buffer ':1982' is permanently disabled
Warning: TRI or OPNDRN buffer ':1976' is permanently disabled
Warning: TRI or OPNDRN buffer ':1970' is permanently disabled
Warning: Flipflop ':2150' stuck at VCC
Warning: No Clock transition on flipflop ':1921'
Warning: Ignored unnecessary INPUT pin 'MS_MOUSE'


Project Information              c:\prj\sprinter\firmware\97\flex\sprint08.rpt

** EMBEDDED ARRAYS **


|lpm_ram_dq:161|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "PGA_INI4.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:161|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:161|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:195|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "PGA_INI4.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:195|altram:sram|segment0_7,
               |lpm_ram_dq:195|altram:sram|segment0_6,
               |lpm_ram_dq:195|altram:sram|segment0_5,
               |lpm_ram_dq:195|altram:sram|segment0_4,
               |lpm_ram_dq:195|altram:sram|segment0_3,
               |lpm_ram_dq:195|altram:sram|segment0_2,
               |lpm_ram_dq:195|altram:sram|segment0_1,
               |lpm_ram_dq:195|altram:sram|segment0_0
);



|lpm_ram_dq:229|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
         )
         OF SEGMENTS (
               |lpm_ram_dq:229|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:229|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:260|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
         )
         OF SEGMENTS (
               |lpm_ram_dq:260|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:260|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:291|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "KBD_INI2.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:291|altram:sram|segment0_7,
               |lpm_ram_dq:291|altram:sram|segment0_6,
               |lpm_ram_dq:291|altram:sram|segment0_5,
               |lpm_ram_dq:291|altram:sram|segment0_4,
               |lpm_ram_dq:291|altram:sram|segment0_3,
               |lpm_ram_dq:291|altram:sram|segment0_2,
               |lpm_ram_dq:291|altram:sram|segment0_1,
               |lpm_ram_dq:291|altram:sram|segment0_0
);



|lpm_ram_dq:323|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "SND_INI.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:323|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:323|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:355|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0#MEM_REG_DATAOUT_CLK1;
               file         = "AY.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:355|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:355|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:386|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0#MEM_REG_DATAOUT_CLK1;
               file         = "AY.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:386|altram:sram|segment0_7,
               |lpm_ram_dq:386|altram:sram|segment0_6,
               |lpm_ram_dq:386|altram:sram|segment0_5,
               |lpm_ram_dq:386|altram:sram|segment0_4,
               |lpm_ram_dq:386|altram:sram|segment0_3,
               |lpm_ram_dq:386|altram:sram|segment0_2,
               |lpm_ram_dq:386|altram:sram|segment0_1,
               |lpm_ram_dq:386|altram:sram|segment0_0
);



|lpm_ram_dq:417|altram:sram|content: MEMORY (
               width        =    8;
               depth        =    4;
               segmentsize  =    4;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "COVOX.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:417|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:417|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:443|altram:sram|content: MEMORY (
               width        =    8;
               depth        =    4;
               segmentsize  =    4;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "COVOX.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:443|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:443|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:469|altram:sram|content: MEMORY (
               width        =    8;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "COVOX.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:469|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:469|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);



|lpm_ram_dq:559|altram:sram|content: MEMORY (
               width        =   16;
               depth        =  256;
               segmentsize  =  256;
               mode         = MEM_INITIALIZED#MEM_REG_DATAIN_CLK0#MEM_REG_WADDR_CLK0#MEM_REG_WCTRL_CLK0;
               file         = "FORTH.MIF";
         )
         OF SEGMENTS (
               |lpm_ram_dq:559|altram:sram|segment0_15,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_14,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_13,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_12,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_11,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_10,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_9,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_8,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_7,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_6,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_5,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_4,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_3,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_2,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_1,		/* This segment is removed by logic synthesis */
               |lpm_ram_dq:559|altram:sram|segment0_0		/* This segment is removed by logic synthesis */
);




Project Information              c:\prj\sprinter\firmware\97\flex\sprint08.rpt

** FILE HIERARCHY **



|lpm_ram_dq:161|
|lpm_ram_dq:161|altram:sram|
|lpm_ram_dq:195|
|lpm_ram_dq:195|altram:sram|
|lpm_ram_dq:229|
|lpm_ram_dq:229|altram:sram|
|lpm_ram_dq:260|
|lpm_ram_dq:260|altram:sram|
|lpm_ram_dq:291|
|lpm_ram_dq:291|altram:sram|
|lpm_ram_dq:323|
|lpm_ram_dq:323|altram:sram|
|lpm_ram_dq:355|
|lpm_ram_dq:355|altram:sram|
|lpm_ram_dq:386|
|lpm_ram_dq:386|altram:sram|
|lpm_ram_dq:417|
|lpm_ram_dq:417|altram:sram|
|lpm_ram_dq:443|
|lpm_ram_dq:443|altram:sram|
|lpm_ram_dq:469|
|lpm_ram_dq:469|altram:sram|
|lpm_add_sub:501|
|lpm_add_sub:501|addcore:adder|
|lpm_add_sub:501|altshift:result_ext_latency_ffs|
|lpm_add_sub:501|altshift:carry_ext_latency_ffs|
|lpm_add_sub:501|altshift:oflow_ext_latency_ffs|
|lpm_ram_dq:559|
|lpm_ram_dq:559|altram:sram|
|lpm_add_sub:607|
|lpm_add_sub:607|addcore:adder|
|lpm_add_sub:607|altshift:result_ext_latency_ffs|
|lpm_add_sub:607|altshift:carry_ext_latency_ffs|
|lpm_add_sub:607|altshift:oflow_ext_latency_ffs|


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

***** Logic for device 'sprint08' compiled without errors.




Device: EPF10K10QC208-3

FLEX 10K Configuration Scheme: Passive Serial

Device Options:
    User-Supplied Start-Up Clock               = OFF
    Auto-Restart Configuration on Frame Error  = OFF
    Release Clears Before Tri-States           = OFF
    Enable Chip_Wide Reset                     = OFF
    Enable Chip-Wide Output Enable             = OFF
    Enable INIT_DONE Output                    = OFF
    JTAG User Code                             = 7f
    MultiVolt I/O                              = OFF



Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** ERROR SUMMARY **

Info: Chip 'sprint08' in device 'EPF10K10QC208-3' has less than 20% of logic cells available for future logic changes -- if your project is likely to change, Altera recommends using a larger device
Info: Chip 'sprint08' in device 'EPF10K10QC208-3' has less than 20% of pins available for future logic changes -- if your project is likely to change, Altera recommends using a larger device
                                                                                                                         
                                                            T                                                            
                                                            U                 R                                          
                                                          K R                 E                                          
                                        S                 B B G       V       S               S     S                    
                  V           G     C   I   V C         G D O N       C     V E           G V N     N V V V   /          
                  _     / V S N     L   N M C A V V V V N _ _ D   T   C   V C R V V V     N _ D     D C _ _   W          
                  W V   I A I D     K V C X C S D D D D D D L I / G / I A D C V D D D M / D W _ V A _ C W W X A   V V V  
                D R A A N 1 N I A A Z A _ A I _ 2 0 0 0 I A E N R 4 W N 1 1 I E 3 0 3 D W I R R A 1 R I R R A I D A A A  
                2 0 2 5 T 3 C O 7 3 1 4 H 1 O 1 2 2 5 1 O T D T D 2 R T 4 6 O D 6 3 0 3 E O 3 0 5 3 1 O 2 1 2 T 6 3 6 0  
              ----------------------------------------------------------------------------------------------------------_ 
             / 208 206 204 202 200 198 196 194 192 190 188 186 184 182 180 178 176 174 172 170 168 166 164 162 160 158   |_ 
            /    207 205 203 201 199 197 195 193 191 189 187 185 183 181 179 177 175 173 171 169 167 165 163 161 159 157    | 
      #TCK |  1                                                                                                         156 | ^DATA0 
^CONF_DONE |  2                                                                                                         155 | ^DCLK 
     ^nCEO |  3                                                                                                         154 | ^nCE 
      #TDO |  4                                                                                                         153 | #TDI 
     VCCIO |  5                                                                                                         152 | GNDIO 
    VCCINT |  6                                                                                                         151 | GNDINT 
      N.C. |  7                                                                                                         150 | VD17 
      N.C. |  8                                                                                                         149 | D4 
      N.C. |  9                                                                                                         148 | XA0 
      VD31 | 10                                                                                                         147 | VD32 
      VD21 | 11                                                                                                         146 | VCCIO 
      VD15 | 12                                                                                                         145 | VCCINT 
      VD11 | 13                                                                                                         144 | VD27 
      N.C. | 14                                                                                                         143 | VD35 
      N.C. | 15                                                                                                         142 | SND_L0 
       VA8 | 16                                                                                                         141 | VD37 
      VD14 | 17                                                                                                         140 | N.C. 
      VD25 | 18                                                                                                         139 | N.C. 
      VA11 | 19                                                                                                         138 | VCCIO 
     GNDIO | 20                                                                                                         137 | VCCINT 
    GNDINT | 21                                                                                                         136 | MD6 
     VCCIO | 22                                                                                                         135 | CAS_2 
    VCCINT | 23                                                                                                         134 | VD00 
      MXA6 | 24                                                                                                         133 | VD07 
        D5 | 25                                                                                                         132 | VD06 
       MD5 | 26                                                                                                         131 | RAS_0 
     MXA10 | 27                                             EPF10K10QC208-3                                             130 | GNDIO 
     CAS_0 | 28                                                                                                         129 | GNDINT 
    BEEPER | 29                                                                                                         128 | A6 
       MD1 | 30                                                                                                         127 | A1 
       MD2 | 31                                                                                                         126 | N.C. 
     GNDIO | 32                                                                                                         125 | N.C. 
    GNDINT | 33                                                                                                         124 | GNDIO 
     VCCIO | 34                                                                                                         123 | GNDINT 
    VCCINT | 35                                                                                                         122 | MD0 
      N.C. | 36                                                                                                         121 | KBD_CLK 
      N.C. | 37                                                                                                         120 | MD7 
       A10 | 38                                                                                                         119 | D3 
        A9 | 39                                                                                                         118 | VCCIO 
        A8 | 40                                                                                                         117 | VCCINT 
       A11 | 41                                                                                                         116 | VD13 
     VCCIO | 42                                                                                                         115 | VD23 
    VCCINT | 43                                                                                                         114 | N.C. 
       VA1 | 44                                                                                                         113 | N.C. 
        D0 | 45                                                                                                         112 | VA7 
        A4 | 46                                                                                                         111 | VD20 
      VA15 | 47                                                                                                         110 | VCCIO 
     GNDIO | 48                                                                                                         109 | VCCINT 
    GNDINT | 49                                                                                                         108 | ^MSEL0 
      #TMS | 50                                                                                                         107 | ^MSEL1 
     #TRST | 51                                                                                                         106 | VCCINT 
  ^nSTATUS | 52                                                                                                         105 | ^nCONFIG 
           |      54  56  58  60  62  64  66  68  70  72  74  76  78  80  82  84  86  88  90  92  94  96  98 100 102 104  _| 
            \   53  55  57  59  61  63  65  67  69  71  73  75  77  79  81  83  85  87  89  91  93  95  97  99 101 103   | 
             \----------------------------------------------------------------------------------------------------------- 
                M M C T V V G M V M D M A V C V M / M G V M V V V / / / G G V V / V A V V X G R D / A A V V T X M S V V  
                X X L A A A N X A X 1 X 2 C A D X R X N D X D C C I M M N N D C N _ 0 D D A N A 7 R 1 1 _ C A A D N A D  
                A A K P 1 1 D A 9 A   A   C S 1 A E A D 0 A 2 C C O 1 R D D 2 C M C   1 3 C D S   F 2 5 C C P 1 4 D 1 3  
                7 9 _ E 4 2 I 0   8   3   I _ 2 4 S 5 I 4 2 4 I I       I I 6 I I S   0 3 S I _         S I E     _ 0 4  
                    P _     O             O 3     E   O       N N       N N   O   1         O 1         0 O _     L      
                    I O                           T           T T       T T                                 I     1      
                    X U                                                                                     N            
                      T                                                                                                  
                                                                                                                         
                                                                                                                         


N.C. = No Connect. This pin has no internal connection to the device.
VCCINT = Dedicated power pin, which MUST be connected to VCC (5.0 volts).
VCCIO = Dedicated power pin, which MUST be connected to VCC (5.0 volts).
GNDINT = Dedicated ground pin or unused dedicated input, which MUST be connected to GND.
GNDIO = Dedicated ground pin, which MUST be connected to GND.
RESERVED = Unused I/O pin, which MUST be left unconnected.

^ = Dedicated configuration pin.
+ = Reserved configuration pin, which is tri-stated during user mode.
* = Reserved configuration pin, which drives out in user mode.
PDn = Power Down pin. 
@ = Special-purpose pin. 
# = JTAG Boundary-Scan Testing/In-System Programming or Configuration Pin. The JTAG inputs TMS and TDI should be tied to VCC and TCK should be tied to GND when not in use.
& = JTAG pin used for I/O. When used as user I/O, JTAG pins must be kept stable before and during configuration.  JTAG pin stability prevents accidental loading of JTAG instructions.


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** RESOURCE USAGE **

Logic                Column       Row                                   
Array                Interconnect Interconnect         Clears/     External  
Block   Logic Cells  Driven       Driven       Clocks  Presets   Interconnect
A1       8/ 8(100%)   1/ 8( 12%)   5/ 8( 62%)    2/2    0/2      14/22( 63%)   
A2       8/ 8(100%)   0/ 8(  0%)   7/ 8( 87%)    1/2    0/2      10/22( 45%)   
A3       8/ 8(100%)   4/ 8( 50%)   2/ 8( 25%)    1/2    2/2      11/22( 50%)   
A4       8/ 8(100%)   0/ 8(  0%)   4/ 8( 50%)    1/2    0/2      11/22( 50%)   
A5       8/ 8(100%)   1/ 8( 12%)   3/ 8( 37%)    1/2    1/2      11/22( 50%)   
A6       8/ 8(100%)   2/ 8( 25%)   3/ 8( 37%)    2/2    1/2      10/22( 45%)   
A7       8/ 8(100%)   0/ 8(  0%)   2/ 8( 25%)    1/2    0/2      11/22( 50%)   
A8       8/ 8(100%)   3/ 8( 37%)   5/ 8( 62%)    2/2    0/2      11/22( 50%)   
A9       8/ 8(100%)   0/ 8(  0%)   3/ 8( 37%)    1/2    1/2       7/22( 31%)   
A10      8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    1/2    0/2       9/22( 40%)   
A11      8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    1/2    0/2      11/22( 50%)   
A12      8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    2/2    0/2      13/22( 59%)   
A13      8/ 8(100%)   4/ 8( 50%)   4/ 8( 50%)    1/2    0/2       3/22( 13%)   
A14      8/ 8(100%)   0/ 8(  0%)   2/ 8( 25%)    1/2    0/2      10/22( 45%)   
A15      8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    2/2    2/2       9/22( 40%)   
A16      8/ 8(100%)   4/ 8( 50%)   4/ 8( 50%)    1/2    0/2       5/22( 22%)   
A17      8/ 8(100%)   0/ 8(  0%)   3/ 8( 37%)    2/2    1/2       8/22( 36%)   
A18      5/ 8( 62%)   3/ 8( 37%)   4/ 8( 50%)    2/2    0/2       5/22( 22%)   
A19      8/ 8(100%)   0/ 8(  0%)   4/ 8( 50%)    1/2    0/2      12/22( 54%)   
A20      8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    1/2    1/2       8/22( 36%)   
A21      8/ 8(100%)   1/ 8( 12%)   2/ 8( 25%)    2/2    0/2      10/22( 45%)   
A22      8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    1/2    0/2      11/22( 50%)   
A23      8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    1/2    1/2       5/22( 22%)   
A24      8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    2/2    0/2      11/22( 50%)   
B1       8/ 8(100%)   0/ 8(  0%)   3/ 8( 37%)    1/2    1/2      15/22( 68%)   
B2       8/ 8(100%)   1/ 8( 12%)   3/ 8( 37%)    1/2    0/2      12/22( 54%)   
B3       8/ 8(100%)   4/ 8( 50%)   3/ 8( 37%)    1/2    0/2      11/22( 50%)   
B4       7/ 8( 87%)   2/ 8( 25%)   3/ 8( 37%)    2/2    2/2      13/22( 59%)   
B5       8/ 8(100%)   1/ 8( 12%)   5/ 8( 62%)    2/2    1/2      16/22( 72%)   
B6       8/ 8(100%)   3/ 8( 37%)   4/ 8( 50%)    2/2    1/2      13/22( 59%)   
B7       8/ 8(100%)   1/ 8( 12%)   3/ 8( 37%)    2/2    2/2      10/22( 45%)   
B8       8/ 8(100%)   2/ 8( 25%)   6/ 8( 75%)    2/2    1/2      11/22( 50%)   
B9       8/ 8(100%)   4/ 8( 50%)   8/ 8(100%)    1/2    1/2      13/22( 59%)   
B10      8/ 8(100%)   2/ 8( 25%)   3/ 8( 37%)    2/2    2/2      13/22( 59%)   
B11      8/ 8(100%)   4/ 8( 50%)   4/ 8( 50%)    2/2    0/2       3/22( 13%)   
B12      8/ 8(100%)   0/ 8(  0%)   3/ 8( 37%)    0/2    0/2      13/22( 59%)   
B13      8/ 8(100%)   1/ 8( 12%)   4/ 8( 50%)    2/2    1/2      15/22( 68%)   
B14      8/ 8(100%)   5/ 8( 62%)   1/ 8( 12%)    2/2    0/2      13/22( 59%)   
B15      8/ 8(100%)   1/ 8( 12%)   0/ 8(  0%)    1/2    0/2      10/22( 45%)   
B16      8/ 8(100%)   3/ 8( 37%)   3/ 8( 37%)    2/2    2/2      12/22( 54%)   
B17      8/ 8(100%)   3/ 8( 37%)   2/ 8( 25%)    2/2    0/2      11/22( 50%)   
B18      8/ 8(100%)   2/ 8( 25%)   2/ 8( 25%)    1/2    0/2       8/22( 36%)   
B19      8/ 8(100%)   4/ 8( 50%)   2/ 8( 25%)    2/2    1/2      15/22( 68%)   
B20      8/ 8(100%)   5/ 8( 62%)   6/ 8( 75%)    2/2    1/2       3/22( 13%)   
B21      8/ 8(100%)   3/ 8( 37%)   3/ 8( 37%)    2/2    1/2      11/22( 50%)   
B22      8/ 8(100%)   2/ 8( 25%)   5/ 8( 62%)    2/2    1/2      13/22( 59%)   
B23      8/ 8(100%)   5/ 8( 62%)   1/ 8( 12%)    2/2    2/2      11/22( 50%)   
B24      8/ 8(100%)   2/ 8( 25%)   3/ 8( 37%)    2/2    0/2       5/22( 22%)   
C1       8/ 8(100%)   0/ 8(  0%)   7/ 8( 87%)    2/2    0/2       8/22( 36%)   
C2       8/ 8(100%)   4/ 8( 50%)   1/ 8( 12%)    1/2    0/2      10/22( 45%)   
C3       8/ 8(100%)   0/ 8(  0%)   5/ 8( 62%)    2/2    1/2       7/22( 31%)   
C4       8/ 8(100%)   2/ 8( 25%)   3/ 8( 37%)    2/2    0/2      14/22( 63%)   
C5       8/ 8(100%)   0/ 8(  0%)   2/ 8( 25%)    2/2    2/2      11/22( 50%)   
C6       8/ 8(100%)   0/ 8(  0%)   8/ 8(100%)    2/2    0/2      13/22( 59%)   
C7       8/ 8(100%)   1/ 8( 12%)   1/ 8( 12%)    2/2    0/2      14/22( 63%)   
C8       8/ 8(100%)   1/ 8( 12%)   3/ 8( 37%)    2/2    2/2      12/22( 54%)   
C9       8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    1/2    1/2      10/22( 45%)   
C10      8/ 8(100%)   5/ 8( 62%)   3/ 8( 37%)    1/2    0/2       3/22( 13%)   
C11      8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    2/2    0/2       6/22( 27%)   
C12      8/ 8(100%)   1/ 8( 12%)   3/ 8( 37%)    2/2    1/2      11/22( 50%)   
C13      7/ 8( 87%)   6/ 8( 75%)   4/ 8( 50%)    2/2    0/2       9/22( 40%)   
C14      8/ 8(100%)   0/ 8(  0%)   6/ 8( 75%)    1/2    0/2       2/22(  9%)   
C15      8/ 8(100%)   6/ 8( 75%)   3/ 8( 37%)    2/2    1/2       6/22( 27%)   
C16      7/ 8( 87%)   3/ 8( 37%)   3/ 8( 37%)    2/2    1/2      14/22( 63%)   
C17      8/ 8(100%)   5/ 8( 62%)   4/ 8( 50%)    2/2    0/2      11/22( 50%)   
C18      6/ 8( 75%)   3/ 8( 37%)   4/ 8( 50%)    2/2    0/2       4/22( 18%)   
C19      8/ 8(100%)   0/ 8(  0%)   1/ 8( 12%)    2/2    0/2       5/22( 22%)   
C20      8/ 8(100%)   2/ 8( 25%)   1/ 8( 12%)    2/2    0/2      14/22( 63%)   
C21      8/ 8(100%)   2/ 8( 25%)   4/ 8( 50%)    2/2    0/2       6/22( 27%)   
C22      7/ 8( 87%)   2/ 8( 25%)   3/ 8( 37%)    2/2    1/2      11/22( 50%)   
C23      8/ 8(100%)   2/ 8( 25%)   2/ 8( 25%)    2/2    0/2      14/22( 63%)   
C24      8/ 8(100%)   2/ 8( 25%)   1/ 8( 12%)    2/2    0/2      14/22( 63%)   


Embedded             Column       Row                                   
Array     Embedded   Interconnect Interconnect         Read/      External  
Block     Cells      Driven       Driven       Clocks  Write    Interconnect
A25      8/8 (100%)   7/8 ( 87%)   8/8 (100%)    1/2    2/2      18/22( 81%)   
B25      8/8 (100%)   8/8 (100%)   4/8 ( 50%)    1/2    2/2      17/22( 77%)   
C25      8/8 (100%)   0/8 (  0%)   8/8 (100%)    1/2    2/2      15/22( 68%)   


Total dedicated input pins used:                 6/6      (100%)
Total I/O pins used:                           127/128    ( 99%)
Total logic cells used:                        567/576    ( 98%)
Total embedded cells used:                      24/24     (100%)
Total EABs used:                                 3/3      (100%)
Average fan-in:                                 2.66/4    ( 66%)
Total fan-in:                                1510/2304    ( 65%)

Total input pins required:                       8
Total input I/O cell registers required:         0
Total output pins required:                     55
Total output I/O cell registers required:        0
Total buried I/O cell registers required:        0
Total bidirectional pins required:              70
Total reserved pins required                     0
Total logic cells required:                    567
Total flipflops required:                      332
Total packed registers required:                 0
Total logic cells in carry chains:               0
Total number of carry chains:                    0
Total logic cells in cascade chains:             0
Total number of cascade chains:                  0
Total single-pin Clock Enables required:         0
Total single-pin Output Enables required:        0

Synthesized logic cells:                        85/ 576   ( 14%)

Logic Cell and Embedded Cell Counts

Column:  01  02  03  04  05  06  07  08  09  10  11  12  EA  13  14  15  16  17  18  19  20  21  22  23  24  Total(LC/EC)
 A:      8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   5   8   8   8   8   8   8    189/8  
 B:      8   8   8   7   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8   8    191/8  
 C:      8   8   8   8   8   8   8   8   8   8   8   8   8   7   8   8   7   8   6   8   8   8   7   8   8    187/8  

Total:  24  24  24  23  24  24  24  24  24  24  24  24  24  23  24  24  23  24  19  24  24  24  23  24  24    567/24 



Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** INPUTS **

                                                    Fan-In    Fan-Out
 Pin     LC     EC   Row  Col  Primitive    Code      INP  FBK  OUT  FBK  Name
  87      -     -    -    10      BIDIR                0    0    0    2  A0
 127      -     -    B    --      BIDIR                0    0    0    1  A1
  65      -     -    -    18      BIDIR                0    0    0    1  A2
 199      -     -    -    20      BIDIR                0    0    0    1  A3
  46      -     -    C    --      BIDIR                0    0    0    1  A4
 205      -     -    -    23      BIDIR                0    0    0    1  A5
 128      -     -    B    --      BIDIR                0    0    0    2  A6
 200      -     -    -    20      BIDIR                0    0    0    1  A7
  40      -     -    C    --      BIDIR                0    0    0    3  A8
  39      -     -    C    --      BIDIR                0    0    0    3  A9
  38      -     -    C    --      BIDIR                0    0    0    3  A10
  41      -     -    C    --      BIDIR                0    0    0    3  A11
  95      -     -    -    06      BIDIR                0    0    0    3  A12
 167      -     -    -    06      BIDIR                0    0    0    4  A13
 180      -     -    -    12      BIDIR                0    0    0   10  A14
  96      -     -    -    05      BIDIR                0    0    0   11  A15
  45      -     -    C    --      BIDIR                0    1    0   16  D0
  63      -     -    -    19      BIDIR                0    1    0   16  D1
 208      -     -    -    24      BIDIR                0    1    0   14  D2
 119      -     -    C    --      BIDIR                0    1    0   13  D3
 149      -     -    A    --      BIDIR                0    1    0   12  D4
  25      -     -    B    --      BIDIR                0    1    0    9  D5
 160      -     -    -    02      BIDIR                0    1    0    8  D6
  93      -     -    -    07      BIDIR                0    1    0    8  D7
 204      -     -    -    22     OPNDRN                0    1    0    0  /INT
  78      -     -    -    --      INPUT  G             0    0    0   43  /IO
 121      -     -    C    --      BIDIR                0    0    0    1  KBD_CLK
 187      -     -    -    13      BIDIR                0    0    0    1  KBD_DAT
 122      -     -    C    --      BIDIR                0    1    0    1  MD0
  30      -     -    B    --      BIDIR                0    1    0    1  MD1
  31      -     -    B    --      BIDIR                0    1    0    1  MD2
 173      -     -    -    09      BIDIR                0    1    0    1  MD3
 101      -     -    -    03      BIDIR                0    1    0    2  MD4
  26      -     -    B    --      BIDIR                0    1    0    2  MD5
 136      -     -    B    --      BIDIR                0    1    0    2  MD6
 120      -     -    C    --      BIDIR                0    1    0    2  MD7
  80      -     -    -    --      INPUT  G             0    0    0    8  /MR
  79      -     -    -    --      INPUT  G             0    0    0    5  /M1
  85      -     -    -    11     OPNDRN                0    0    0    0  /NMI
 184      -     -    -    --      INPUT                0    0    0    5  /RD
  70      -     -    -    15     OPNDRN                0    1    0   22  /RESET
  94      -     -    -    07      INPUT                0    0    0    2  /RF
  99      -     -    -    04      INPUT                0    0    0    1  TAPE_IN
 183      -     -    -    --      INPUT  G             0    0    0    8  TG42
 134      -     -    B    --      BIDIR                0    1    0    2  VD00
 189      -     -    -    14      BIDIR                0    1    0    2  VD01
 191      -     -    -    15      BIDIR                0    1    0    2  VD02
 175      -     -    -    10      BIDIR                0    1    0    2  VD03
  73      -     -    -    14      BIDIR                0    1    0    2  VD04
 190      -     -    -    15      BIDIR                0    1    0    2  VD05
 132      -     -    B    --      BIDIR                0    1    0    2  VD06
 133      -     -    B    --      BIDIR                0    1    0    2  VD07
  88      -     -    -    10      BIDIR                0    1    0    0  VD10
  13      -     -    A    --      BIDIR                0    1    0    0  VD11
  68      -     -    -    16      BIDIR                0    1    0    0  VD12
 116      -     -    C    --      BIDIR                0    1    0    0  VD13
  17      -     -    A    --      BIDIR                0    1    0    0  VD14
  12      -     -    A    --      BIDIR                0    1    0    0  VD15
 179      -     -    -    12      BIDIR                0    1    0    0  VD16
 150      -     -    A    --      BIDIR                0    1    0    0  VD17
 111      -     -    C    --      BIDIR                0    1    0    0  VD20
  11      -     -    A    --      BIDIR                0    1    0    0  VD21
 192      -     -    -    16      BIDIR                0    1    0    0  VD22
 115      -     -    C    --      BIDIR                0    1    0    0  VD23
  75      -     -    -    13      BIDIR                0    1    0    0  VD24
  18      -     -    A    --      BIDIR                0    1    0    0  VD25
  83      -     -    -    12      BIDIR                0    1    0    0  VD26
 144      -     -    A    --      BIDIR                0    1    0    0  VD27
 174      -     -    -    09      BIDIR                0    1    0    0  VD30
  10      -     -    A    --      BIDIR                0    1    0    0  VD31
 147      -     -    A    --      BIDIR                0    1    0    0  VD32
  89      -     -    -    09      BIDIR                0    1    0    0  VD33
 104      -     -    -    01      BIDIR                0    1    0    0  VD34
 143      -     -    A    --      BIDIR                0    1    0    0  VD35
 176      -     -    -    11      BIDIR                0    1    0    0  VD36
 141      -     -    A    --      BIDIR                0    1    0    0  VD37
 161      -     -    -    03     OPNDRN                0    1    0    0  /WAIT
 182      -     -    -    --      INPUT                0    0    0    7  /WR


Code:

s = Synthesized pin or logic cell
+ = Synchronous flipflop
/ = Slow slew-rate output
! = NOT gate push-back
r = Fitter-inserted logic cell
@ = Uses single-pin Clock Enable
& = Uses single-pin Output Enable
G = Global Source. Fan-out destinations counted here do not include destinations
that are driven using global routing resources. Refer to the Auto Global Signals,
Clock Signals, Clear Signals, Synchronous Load Signals, and Synchronous Clear Signals
Sections of this Report File for information on which signals' fan-outs are used as
Clock, Clear, Preset, Output Enable, and synchronous Load signals.


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** OUTPUTS **

       Fed By Fed By                                Fan-In    Fan-Out
 Pin     LC     EC   Row  Col  Primitive    Code      INP  FBK  OUT  FBK  Name
  87      -     -    -    10        TRI                0    0    0    2  A0
 127      -     -    B    --        TRI                0    0    0    1  A1
  65      -     -    -    18        TRI                0    0    0    1  A2
 199      -     -    -    20        TRI                0    0    0    1  A3
  46      -     -    C    --        TRI                0    0    0    1  A4
 205      -     -    -    23        TRI                0    0    0    1  A5
 128      -     -    B    --        TRI                0    0    0    2  A6
 200      -     -    -    20        TRI                0    0    0    1  A7
  40      -     -    C    --        TRI                0    0    0    3  A8
  39      -     -    C    --        TRI                0    0    0    3  A9
  38      -     -    C    --        TRI                0    0    0    3  A10
  41      -     -    C    --        TRI                0    0    0    3  A11
  95      -     -    -    06        TRI                0    0    0    3  A12
 167      -     -    -    06        TRI                0    0    0    4  A13
 180      -     -    -    12        TRI                0    0    0   10  A14
  96      -     -    -    05        TRI                0    0    0   11  A15
  29      -     -    B    --     OUTPUT                0    1    0    0  BEEPER
  28      -     -    B    --     OUTPUT                0    1    0    0  CAS_0
 193      -     -    -    17     OUTPUT                0    1    0    0  CAS_1
 135      -     -    B    --     OUTPUT                0    1    0    0  CAS_2
  67      -     -    -    17     OUTPUT                0    1    0    0  CAS_3
  55      -     -    -    23     OUTPUT                0    1    0    0  CLK_PIX
 198      -     -    -    19     OUTPUT                0    1    0    0  CLKZ1
  45      -     -    C    --        TRI                0    1    0   16  D0
  63      -     -    -    19        TRI                0    1    0   16  D1
 208      -     -    -    24        TRI                0    1    0   14  D2
 119      -     -    C    --        TRI                0    1    0   13  D3
 149      -     -    A    --        TRI                0    1    0   12  D4
  25      -     -    B    --        TRI                0    1    0    9  D5
 160      -     -    -    02        TRI                0    1    0    8  D6
  93      -     -    -    07        TRI                0    1    0    8  D7
 204      -     -    -    22     OPNDRN                0    1    0    0  /INT
 121      -     -    C    --        TRI                0    0    0    1  KBD_CLK
 187      -     -    -    13        TRI                0    0    0    1  KBD_DAT
 122      -     -    C    --        TRI                0    1    0    1  MD0
  30      -     -    B    --        TRI                0    1    0    1  MD1
  31      -     -    B    --        TRI                0    1    0    1  MD2
 173      -     -    -    09        TRI                0    1    0    1  MD3
 101      -     -    -    03        TRI                0    1    0    2  MD4
  26      -     -    B    --        TRI                0    1    0    2  MD5
 136      -     -    B    --        TRI                0    1    0    2  MD6
 120      -     -    C    --        TRI                0    1    0    2  MD7
  60      -     -    -    21     OUTPUT                0    1    0    0  MXA0
 195      -     -    -    17     OUTPUT                0    1    0    0  MXA1
  74      -     -    -    13     OUTPUT                0    1    0    0  MXA2
  64      -     -    -    18     OUTPUT                0    1    0    0  MXA3
  69      -     -    -    16     OUTPUT                0    1    0    0  MXA4
  71      -     -    -    14     OUTPUT                0    1    0    0  MXA5
  24      -     -    B    --     OUTPUT                0    1    0    0  MXA6
  53      -     -    -    24     OUTPUT                0    1    0    0  MXA7
  62      -     -    -    19     OUTPUT                0    1    0    0  MXA8
  54      -     -    -    24     OUTPUT                0    1    0    0  MXA9
  27      -     -    B    --     OUTPUT                0    1    0    0  MXA10
  85      -     -    -    11     OPNDRN                0    0    0    0  /NMI
 131      -     -    B    --     OUTPUT                0    1    0    0  RAS_0
  92      -     -    -    08     OUTPUT                0    1    0    0  RAS_1
  70      -     -    -    15     OPNDRN                0    1    0   22  /RESET
 202      -     -    -    21     OUTPUT                0    1    0    0  SINC
 196      -     -    -    18     OUTPUT                0    1    0    0  SINC_H
 142      -     -    A    --     OUTPUT                0    1    0    0  SND_L0
 102      -     -    -    02     OUTPUT                0    0    0    0  SND_L1
 169      -     -    -    07     OUTPUT                0    1    0    0  SND_R0
 166      -     -    -    05     OUTPUT                0    0    0    0  SND_R1
  56      -     -    -    22     OUTPUT                0    1    0    0  TAPE_OUT
 186      -     -    -    13     OUTPUT                0    1    0    0  TURBO_LED
 157      -     -    -    01     OUTPUT                0    1    0    0  VA0
  44      -     -    C    --     OUTPUT                0    1    0    0  VA1
 206      -     -    -    23     OUTPUT                0    1    0    0  VA2
 159      -     -    -    02     OUTPUT                0    1    0    0  VA3
 197      -     -    -    18     OUTPUT                0    1    0    0  VA4
 168      -     -    -    06     OUTPUT                0    1    0    0  VA5
 158      -     -    -    01     OUTPUT                0    1    0    0  VA6
 112      -     -    C    --     OUTPUT                0    1    0    0  VA7
  16      -     -    A    --     OUTPUT                0    1    0    0  VA8
  61      -     -    -    20     OUTPUT                0    1    0    0  VA9
 103      -     -    -    01     OUTPUT                0    1    0    0  VA10
  19      -     -    A    --     OUTPUT                0    1    0    0  VA11
  58      -     -    -    21     OUTPUT                0    1    0    0  VA12
 203      -     -    -    21     OUTPUT                0    1    0    0  VA13
  57      -     -    -    22     OUTPUT                0    1    0    0  VA14
  47      -     -    C    --     OUTPUT                0    1    0    0  VA15
  97      -     -    -    05     OUTPUT                0    0    0    0  V_CS0
  86      -     -    -    11     OUTPUT                0    0    0    0  V_CS1
 134      -     -    B    --        TRI                0    1    0    2  VD00
 189      -     -    -    14        TRI                0    1    0    2  VD01
 191      -     -    -    15        TRI                0    1    0    2  VD02
 175      -     -    -    10        TRI                0    1    0    2  VD03
  73      -     -    -    14        TRI                0    1    0    2  VD04
 190      -     -    -    15        TRI                0    1    0    2  VD05
 132      -     -    B    --        TRI                0    1    0    2  VD06
 133      -     -    B    --        TRI                0    1    0    2  VD07
  88      -     -    -    10        TRI                0    1    0    0  VD10
  13      -     -    A    --        TRI                0    1    0    0  VD11
  68      -     -    -    16        TRI                0    1    0    0  VD12
 116      -     -    C    --        TRI                0    1    0    0  VD13
  17      -     -    A    --        TRI                0    1    0    0  VD14
  12      -     -    A    --        TRI                0    1    0    0  VD15
 179      -     -    -    12        TRI                0    1    0    0  VD16
 150      -     -    A    --        TRI                0    1    0    0  VD17
 111      -     -    C    --        TRI                0    1    0    0  VD20
  11      -     -    A    --        TRI                0    1    0    0  VD21
 192      -     -    -    16        TRI                0    1    0    0  VD22
 115      -     -    C    --        TRI                0    1    0    0  VD23
  75      -     -    -    13        TRI                0    1    0    0  VD24
  18      -     -    A    --        TRI                0    1    0    0  VD25
  83      -     -    -    12        TRI                0    1    0    0  VD26
 144      -     -    A    --        TRI                0    1    0    0  VD27
 174      -     -    -    09        TRI                0    1    0    0  VD30
  10      -     -    A    --        TRI                0    1    0    0  VD31
 147      -     -    A    --        TRI                0    1    0    0  VD32
  89      -     -    -    09        TRI                0    1    0    0  VD33
 104      -     -    -    01        TRI                0    1    0    0  VD34
 143      -     -    A    --        TRI                0    1    0    0  VD35
 176      -     -    -    11        TRI                0    1    0    0  VD36
 141      -     -    A    --        TRI                0    1    0    0  VD37
 207      -     -    -    24     OUTPUT                0    1    0    0  V_WR0
 163      -     -    -    04     OUTPUT                0    0    0    0  V_WR1
 164      -     -    -    04     OUTPUT                0    0    0    0  V_WR2
 170      -     -    -    08     OUTPUT                0    0    0    0  V_WR3
 161      -     -    -    03     OPNDRN                0    1    0    0  /WAIT
 172      -     -    -    08     OUTPUT                0    1    0    0  /WE
  90      -     -    -    08     OUTPUT                0    1    0    0  XACS
 148      -     -    A    --     OUTPUT                0    1    0    0  XA0
 100      -     -    -    03     OUTPUT                0    1    0    0  XA1
 162      -     -    -    03     OUTPUT                0    1    0    0  XA2


Code:

s = Synthesized pin or logic cell
+ = Synchronous flipflop
/ = Slow slew-rate output
! = NOT gate push-back
r = Fitter-inserted logic cell
@ = Uses single-pin Clock Enable
& = Uses single-pin Output Enable


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** BURIED LOGIC **

                                                    Fan-In    Fan-Out
 IOC     LC     EC   Row  Col  Primitive    Code      INP  FBK  OUT  FBK  Name
   -      8     -    A    21       DFFE                0    2    0    2  AA0
   -      2     -    B    17       DFFE                0    2    0    2  AA1
   -      5     -    B    14       DFFE                0    2    0    2  AA2
   -      1     -    C    13       DFFE                0    2    0    2  AA3
   -      4     -    C    13       DFFE                0    2    0    2  AA4
   -      4     -    B    14       DFFE                0    2    0    2  AA5
   -      4     -    B    13       DFFE                0    2    0    2  AA6
   -      7     -    C    23       DFFE                0    2    0    3  AA7
   -      8     -    C    20       DFFE                0    2    0    2  AA8
   -      4     -    C    24       DFFE                0    2    0    2  AA9
   -      8     -    C    13       DFFE                0    2    0    5  AA10
   -      7     -    C    13       DFFE                0    2    0    4  AA11
   -      5     -    B    17       DFFE                0    2    0    2  AA12
   -      3     -    B    14       DFFE                0    2    0    2  AA13
   -      4     -    B    01       DFFE                0    4    0    1  AROM16
   -      5     -    B    12      LCELL                0    4    0    1  AR0
   -      3     -    B    12      LCELL                0    3    0    1  AR1
   -      5     -    B    01      LCELL                0    3    0    1  AR2
   -      2     -    B    01      LCELL                0    2    0    1  AR3
   -      4     -    A    05      LCELL                0    2    0    1  AX128
   -      2     -    A    01       DFFE                0    5    0    1  AY_AAX0
   -      2     -    A    19       DFFE   +            0    4    0    1  AY_AA0
   -      4     -    A    19       DFFE   +            0    4    0    1  AY_AA1
   -      5     -    A    19       DFFE   +            0    4    0    1  AY_AA2
   -      6     -    A    19       DFFE   +            0    4    0    1  AY_AA3
   -      3     -    A    15       DFFE                0    3    0    4  AY_ABLK
   -      8     -    A    01       DFFE                0    2    0    2  AY_ADR0
   -      6     -    A    04       DFFE                0    2    0    2  AY_ADR1
   -      3     -    A    04       DFFE                0    2    0    2  AY_ADR2
   -      2     -    A    04       DFFE                0    2    0    2  AY_ADR3
   -      1     -    A    19       DFFE   +            0    3    0    3  AY_AMP0
   -      8     -    A    19       DFFE   +            0    3    0    2  AY_AMP1
   -      3     -    A    19       DFFE   +            0    3    0    2  AY_AMP2
   -      7     -    A    19       DFFE   +            0    3    0    2  AY_AMP3
   -      6     -    A    01        OR2    s           0    4    0    1  AY_AX0~1
   -      1     -    A    01        OR2                0    3    0    8  AY_AX0
   -      8     -    A    04        OR2    s           0    4    0    1  AY_AX1~1
   -      5     -    A    04        OR2                0    3    0    8  AY_AX1
   -      1     -    A    04        OR2    s           0    4    0    1  AY_AX2~1
   -      1     -    A    22        OR2                0    3    0    8  AY_AX2
   -      4     -    A    04        OR2    s           0    4    0    1  AY_AX3~1
   -      1     -    A    02        OR2                0    3    0    8  AY_AX3
   -      3     -    A    24        OR2                0    4    0    8  AY_AX4
   -      5     -    A    08       AND2                0    3    0    8  AY_AX5
   -      6     -    A    15       DFFE                0    3    0    1  AY_BBLK
   -      2     -    A    15       DFFE                0    4    0    4  AY_BINV
   -      8     -    A    11       DFFE   +            0    4    0    2  AY_C
   -      1     -    B    20       DFFE   +            0    1    0   26  AY_CCC0
   -      8     -    A    10       DFFE   +            0    1    0   29  AY_CCC1
   -      7     -    B    11       DFFE   +            0    1    0   48  AY_CCC2
   -      3     -    B    21       DFFE   +            0    1    0    2  AY_CCC3
   -      2     -    B    24       DFFE   +            0    1    0    2  AY_CCC4
   -      8     -    A    24       DFFE   +            0    1    0    3  AY_CCC5
   -      1     -    A    24       DFFE   +            0    1    0    3  AY_CCC6
   -      7     -    A    08       DFFE   +            0    1    0    4  AY_CCC7
   -      6     -    A    24       DFFE   +            0    1    0    7  AY_CCC8
   -      6     -    A    09       DFFE   +    !       0    3    0   10  AY_CX
   -      1     -    A    03       DFFE   +            0    2    0    1  AY_DAT_WR
   -      7     -    A    10       DFFE   +            0    3    0    4  AY_DAT0
   -      8     -    A    02       DFFE   +            0    3    0    4  AY_DAT1
   -      5     -    A    02       DFFE   +            0    4    0    4  AY_DAT2
   -      7     -    A    02       DFFE   +            0    3    0    4  AY_DAT3
   -      4     -    A    11       DFFE   +            0    3    0    7  AY_DAT4
   -      7     -    A    11       DFFE   +            0    4    0    3  AY_DAT5
   -      5     -    A    11       DFFE   +            0    3    0    2  AY_DAT6
   -      6     -    A    11       DFFE   +            0    4    0    2  AY_DAT7
   -      5     -    C    23       DFFE   +            0    2    0    1  AY_DD0
   -      5     -    C    20       DFFE   +            0    2    0    1  AY_DD1
   -      7     -    C    24       DFFE   +            0    2    0    1  AY_DD2
   -      8     -    C    04       DFFE   +            0    2    0    1  AY_DD3
   -      8     -    A    08       DFFE   +            0    2    0    1  AY_DD4
   -      7     -    B    03       DFFE   +            0    2    0    1  AY_DD5
   -      6     -    B    02       DFFE   +            0    2    0    1  AY_DD6
   -      7     -    C    07       DFFE   +            0    2    0    1  AY_DD7
   -      2     -    A    10        OR2                0    4    0    1  AY_DI0
   -      2     -    A    24        OR2                0    4    0    1  AY_DI1
   -      6     -    A    12        OR2                0    4    0    1  AY_DI2
   -      2     -    A    02        OR2                0    4    0    1  AY_DI3
   -      4     -    A    01        OR2                0    4    0    1  AY_DI4
   -      2     -    A    12        OR2                0    4    0    1  AY_DI5
   -      3     -    A    01        OR2                0    4    0    1  AY_DI6
   -      1     -    A    11        OR2                0    4    0    1  AY_DI7
   -      7     -    B    16       DFFE        !       0    5    0    6  AY_D_WR
   -      7     -    A    17       DFFE                0    2    0   10  AY_F_RES
   -      7     -    A    15       DFFE                0    4    0    2  AY_GF0
   -      4     -    A    15       DFFE                0    4    0    1  AY_GF1
   -      1     -    A    15       DFFE                0    4    0    4  AY_GF2
   -      8     -    A    15       DFFE                0    4    0    1  AY_GF3
   -      4     -    A    22       DFFE   +            0    4    0    2  AY_OUTS1
   -      7     -    A    07       DFFE   +            0    4    0    2  AY_OUTS2
   -      6     -    A    07       DFFE   +            0    4    0    2  AY_OUTS3
   -      3     -    A    05       DFFE   +            0    2    0    1  AY_OUT1
   -      2     -    A    07       DFFE   +            0    2    0    1  AY_OUT2
   -      1     -    A    12       DFFE   +            0    2    0    1  AY_OUT3
   -      5     -    A    05        OR2                0    3    0    6  AY_Q
   -      8     -    A    07        OR2    s           0    4    0    1  AY_Q~1
   -      3     -    A    21       DFFE   +            0    2    0    1  AY_SHR
   -      1     -    A    17       DFFE   +            0    2    0    4  AY_SH0
   -      8     -    A    17       DFFE   +            0    2    0    1  AY_SH1
   -      5     -    A    17       DFFE   +            0    2    0    1  AY_SH2
   -      4     -    A    17       DFFE   +            0    2    0    1  AY_SH3
   -      6     -    A    17       DFFE   +            0    2    0    2  AY_SH4
   -      6     -    A    21       DFFE   +            0    2    0    1  AY_SH5
   -      7     -    A    21       DFFE   +            0    2    0    1  AY_SH6
   -      4     -    A    21       DFFE   +            0    2    0    1  AY_SH7
   -      3     -    A    23       DFFE   +            0    3    0    3  AY_VAR
   -      8     -    A    23       DFFE   +            0    4    0    3  AY_VA0
   -      1     -    A    23       DFFE   +            0    4    0    2  AY_VA1
   -      7     -    A    23       DFFE   +            0    3    0    2  AY_VA2
   -      5     -    A    23       DFFE   +            0    4    0    4  AY_VA3
   -      1     -    A    10        OR2                0    4    0    8  AY_WR
   -      3     -    A    14       DFFE                0    2    0    1  AY_XXM0
   -      4     -    A    14       DFFE                0    2    0    1  AY_XXM1
   -      6     -    A    14       DFFE                0    2    0    1  AY_XXM2
   -      8     -    A    14       DFFE                0    2    0    1  AY_XXM3
   -      4     -    A    24       DFFE                0    2    0    1  AY_XXM4
   -      1     -    A    14       DFFE                0    2    0    2  AY_XXM5
   -      2     -    A    05       DFFE   +            0    3    0    3  AY_XX0
   -      3     -    A    20       DFFE   +            0    4    0    2  AY_XX1
   -      8     -    A    20       DFFE   +            0    4    0    2  AY_XX2
   -      5     -    A    20       DFFE   +            0    4    0    2  AY_XX3
   -      1     -    A    20       DFFE   +            0    3    0    2  AY_XX4
   -      4     -    A    20       DFFE   +            0    4    0    1  AY_XX5
   -      8     -    A    05       DFFE   +            0    2    0    1  AY_X_0
   -      4     -    A    07       DFFE   +            0    2    0    1  AY_X_1
   -      7     -    A    12       DFFE   +            0    2    0    1  AY_X_2
   -      7     -    A    05       DFFE   +            0    2    0    1  AY_X_3
   -      3     -    A    07       DFFE   +            0    2    0    1  AY_X_4
   -      5     -    A    12       DFFE   +            0    2    0    1  AY_X_5
   -      8     -    C    16       DFFE        !       0    4    0    8  BLANK
   -      2     -    B    10      LCELL                2    1    0    8  BLK_R
   -      6     -    C    18       DFFE                0    5    0    8  BORD
   -      2     -    B    22       DFFE                0    3    0    2  BRD0
   -      5     -    B    22       DFFE                0    3    0    2  BRD1
   -      1     -    B    22       DFFE                0    3    0    2  BRD2
   -      6     -    B    22       DFFE                0    3    1    0  BRD3
   -      7     -    B    24       DFFE                0    3    0    1  BRD4
   -      2     -    B    14       DFFE   +            0    2    0    8  CAS
   -      3     -    B    13       DFFE                0    4    0    1  CNF3
   -      8     -    B    13       DFFE                0    4    0    1  CNF4
   -      7     -    B    05      LCELL                0    4    0    2  CORRECT_1F
   -      2     -    C    19       DFFE                0    1    0    2  CTF0
   -      1     -    C    19       DFFE                0    2    0    1  CTF1
   -      4     -    C    19       DFFE                0    2    0    2  CTF2
   -      6     -    C    19       DFFE                0    3    0    1  CTF3
   -      7     -    C    19       DFFE                0    4    0    1  CTF4
   -      4     -    A    18       DFFE                0    1    0    4  CTH0
   -      6     -    A    18       DFFE                0    2    0    5  CTH1
   -      2     -    A    18       DFFE                0    3    0    9  CTH2
   -      3     -    C    17       DFFE                0    3    0    4  CTH3
   -      5     -    C    17       DFFE                0    3    0    5  CTH4
   -      6     -    C    17       DFFE                0    3    0    9  CTH5
   -      5     -    C    15       DFFE                0    1    0    4  CTV0
   -      2     -    C    15       DFFE                0    2    0    2  CTV1
   -      3     -    C    15       DFFE                0    3    0    7  CTV2
   -      1     -    C    21       DFFE                0    1    0    5  CTV3
   -      4     -    C    21       DFFE                0    3    0    4  CTV4
   -      2     -    C    21       DFFE                0    4    0    4  CTV5
   -      2     -    C    18       DFFE                0    3    0    8  CTV6
   -      1     -    C    18       DFFE                0    4    0    7  CTV7
   -      5     -    C    18       DFFE                0    4    0    7  CTV8
   -      8     -    B    20       DFFE   +            0    1    0    6  CT0
   -      3     -    B    20       DFFE   +            0    1    0   16  CT2
   -      3     -    B    24       DFFE   +            0    2    0    5  CT3
   -      1     -    B    24       DFFE   +            0    3    0    4  CT4
   -      8     -    B    24       DFFE   +            0    3    0    8  CT5
   -      6     -    B    19       DFFE                0    5    0    1  DCOL0
   -      1     -    B    19       DFFE                0    5    0    1  DCOL1
   -      4     -    B    22       DFFE                0    5    0    1  DCOL2
   -      2     -    B    19       DFFE                0    5    0    1  DCOL3
   -      5     -    B    19       DFFE                0    5    0    1  DCOL4
   -      8     -    B    22       DFFE                0    5    0    1  DCOL5
   -      8     -    B    19       DFFE                0    4    0    1  DCOL6
   -      7     -    B    19       DFFE                0    4    0    1  DCOL7
   -      1     -    B    03      LCELL                0    4    0    1  DCP_CX
   -      6     -    B    05       DFFE                1    5    0    5  DCP3
   -      1     -    B    09       DFFE                1    4    0    7  DCP4
   -      7     -    B    09       DFFE                1    3    0    4  DCP5
   -      8     -    B    09       DFFE                1    4    0   11  DD0
   -      4     -    B    09       DFFE                1    4    0   11  DD1
   -      2     -    B    09       DFFE                1    4    0   11  DD2
   -      3     -    B    09       DFFE                1    3    0    8  DD6
   -      6     -    B    09       DFFE                1    3    0   19  DD7
   -      5     -    C    08       DFFE        !       0    5    0    6  DOS
   -      4     -    B    11       DFFE                0    3    0    1  DOS_ON_
   -      1     -    C    02       DFFE   +            0    1    0    1  DPIC
   -      2     -    B    15       DFFE                0    2    0    1  D_PIC00
   -      3     -    B    15       DFFE                0    4    0    1  D_PIC01
   -      4     -    B    15       DFFE                0    4    0    1  D_PIC02
   -      5     -    B    15       DFFE                0    4    0    1  D_PIC03
   -      6     -    B    15       DFFE                0    4    0    1  D_PIC04
   -      7     -    B    15       DFFE                0    4    0    1  D_PIC05
   -      8     -    B    15       DFFE                0    4    0    1  D_PIC06
   -      1     -    B    15       DFFE                0    4    0    1  D_PIC07
   -      1     -    B    04        OR2                1    3    0    0  D_RD
   -      3     -    B    18       DFFE                1    4    0    1  E_CAS_0
   -      6     -    B    18       DFFE                1    4    0    1  E_CAS_1
   -      1     -    B    18       DFFE                1    4    0    1  E_CAS_2
   -      8     -    B    18       DFFE                1    4    0    1  E_CAS_3
   -      4     -    B    17        GND    s           0    0    0    8  ~GND~
   -      2     -    A    06       DFFE                0    5    0    1  IN_OUT_CMD
   -      1     -    C    22       DFFE        !       0    2    1    0  INTT
   -      2     -    B    20       DFFE        !       1    1    0    1  /IOM
   -      5     -    B    07       DFFE        !       1    2    0    9  /IOM1
   -      2     -    B    07        OR2    s           2    2    0    1  IO_WAIT~1
   -      5     -    B    16        OR2                1    1    0    1  /IOWR
   -      3     -    C    09        OR2                0    4    0    8  KA8
   -      7     -    C    09        OR2                0    4    0    8  KA9
   -      4     -    C    04        OR2                0    4    0    8  KA10
   -      2     -    C    12        OR2                0    4    0    8  KA11
   -      1     -    C    07        OR2                0    4    0    8  KA12
   -      1     -    C    09        OR2                0    3    0    8  KA13
   -      2     -    C    09        OR2                0    3    0    8  KA14
   -      8     -    C    09        OR2                0    3    0    8  KA15
   -      2     -    C    05       DFFE                0    4    0    1  KB_ALT
   -      5     -    C    01      LCELL                0    4    0    2  KB_ALT_X
   -      3     -    C    05       DFFE                0    4    0    2  KB_CTRL
   -      6     -    C    01      LCELL                0    4    0    1  KB_CTRL_X
   -      8     -    C    03       DFFE        !       0    4    0    5  KB_CT0
   -      6     -    C    03       DFFE        !       0    4    0    6  KB_CT1
   -      3     -    C    03       DFFE        !       0    4    0   12  KB_CT2
   -      2     -    C    16       DFFE                0    2    0   13  KBD_CC
   -      7     -    C    16       DFFE                0    2    0    1  KBD_DD
   -      4     -    C    23       DFFE   +    !       0    2    0    1  KBD0
   -      3     -    C    20       DFFE   +    !       0    2    0    1  KBD1
   -      1     -    C    01       DFFE                0    2    0    5  KB_D1
   -      6     -    C    24       DFFE   +    !       0    2    0    1  KBD2
   -      2     -    C    01       DFFE                0    2    0    6  KB_D2
   -      7     -    C    04       DFFE   +    !       0    2    0    1  KBD3
   -      7     -    C    14       DFFE                0    2    0    6  KB_D3
   -      7     -    C    12       DFFE   +    !       0    2    0    1  KBD4
   -      5     -    C    14       DFFE                0    2    0    5  KB_D4
   -      5     -    C    07       DFFE   +    !       0    2    0    1  KBD5
   -      1     -    C    14       DFFE                0    2    0    7  KB_D5
   -      6     -    C    14       DFFE                0    2    0    5  KB_D6
   -      2     -    C    14       DFFE                0    2    0    5  KB_D7
   -      4     -    C    14       DFFE                0    2    0    5  KB_D8
   -      8     -    C    14       DFFE                0    2    0    1  KB_D9
   -      3     -    C    14       DFFE                0    2    0    1  KB_D10
   -      4     -    C    01       DFFE                0    3    0    1  KB_EXT
   -      4     -    C    05       DFFE        !       0    5    0    1  KB_F12
   -      4     -    C    08       DFFE   +            0    0    0    6  KB_MA0
   -      1     -    C    12       DFFE   +            0    1    0    3  KB_MA1
   -      8     -    C    12       DFFE   +            0    2    0    5  KB_MA2
   -      6     -    C    12       DFFE   +            0    4    0    6  KB_MXA
   -      5     -    C    03       DFFE                0    4    0   10  KB_OFF
   -      6     -    C    05       DFFE        !       0    6    0    1  KB_RESET
   -      1     -    C    05      LCELL                0    4    0    3  KB_XXX
   -      3     -    B    10       DFFE   +            1    0    0    3  K_CLK
   -      6     -    C    04        OR2                1    2    0    1  KDCA0
   -      4     -    C    12        OR2                1    2    0    1  KDCA1
   -      4     -    C    07        OR2                1    2    0    1  KDCA2
   -      5     -    C    04       DFFE                0    2    0    1  KDD3
   -      3     -    C    12       DFFE                0    2    0    1  KDD4
   -      2     -    C    07       DFFE                0    2    0    1  KDD5
   -      6     -    C    09       DFFE        !       0    3    0    2  KDD6
   -      4     -    C    09       DFFE        !       0    3    0    2  KDD7
   -      2     -    C    11       DFFE                0    4    0    1  KDXX0
   -      3     -    C    11       DFFE                0    4    0    1  KDXX1
   -      5     -    C    11       DFFE                0    4    0    1  KDXX2
   -      7     -    C    11       DFFE                0    4    0    1  KDXX3
   -      1     -    C    11       DFFE                0    4    0    1  KDXX4
   -      8     -    C    11       DFFE                0    4    0    1  KDXX5
   -      6     -    C    11       DFFE                0    4    0    1  KDX0
   -      4     -    C    11       DFFE                0    4    0    1  KDX1
   -      8     -    C    06       DFFE                0    4    0    1  KDX2
   -      7     -    C    06       DFFE                0    4    0    1  KDX3
   -      5     -    C    06       DFFE                0    4    0    1  KDX4
   -      3     -    C    06       DFFE                0    4    0    1  KDX5
   -      6     -    B    24      LCELL                0    3    0    7  LD_PIC
   -      7     -    B    17       DFFE   +            0    1    0    9  LMC_END
   -      -     4    B    --   MEM_SGMT                0   10    0    2  |lpm_ram_dq:195|altram:sram|segment0_0
   -      -     2    B    --   MEM_SGMT                0   10    0    2  |lpm_ram_dq:195|altram:sram|segment0_1
   -      -     6    B    --   MEM_SGMT                0   10    0    2  |lpm_ram_dq:195|altram:sram|segment0_2
   -      -     7    B    --   MEM_SGMT                0   10    1    2  |lpm_ram_dq:195|altram:sram|segment0_3
   -      -     1    B    --   MEM_SGMT                0   10    0    4  |lpm_ram_dq:195|altram:sram|segment0_4
   -      -     3    B    --   MEM_SGMT                0   10    0    4  |lpm_ram_dq:195|altram:sram|segment0_5
   -      -     8    B    --   MEM_SGMT                0   10    0    5  |lpm_ram_dq:195|altram:sram|segment0_6
   -      -     5    B    --   MEM_SGMT                0   10    0    5  |lpm_ram_dq:195|altram:sram|segment0_7
   -      -     3    C    --   MEM_SGMT                0   10    0    8  |lpm_ram_dq:291|altram:sram|segment0_0
   -      -     7    C    --   MEM_SGMT                0   10    0    8  |lpm_ram_dq:291|altram:sram|segment0_1
   -      -     6    C    --   MEM_SGMT                0   10    0    8  |lpm_ram_dq:291|altram:sram|segment0_2
   -      -     1    C    --   MEM_SGMT                0   10    0    3  |lpm_ram_dq:291|altram:sram|segment0_3
   -      -     5    C    --   MEM_SGMT                0   10    0    3  |lpm_ram_dq:291|altram:sram|segment0_4
   -      -     4    C    --   MEM_SGMT                0   10    0    3  |lpm_ram_dq:291|altram:sram|segment0_5
   -      -     8    C    --   MEM_SGMT                0    9    0    1  |lpm_ram_dq:291|altram:sram|segment0_6
   -      -     2    C    --   MEM_SGMT                0    9    0    1  |lpm_ram_dq:291|altram:sram|segment0_7
   -      -     1    A    --   MEM_SGMT                1   10    0   12  |lpm_ram_dq:386|altram:sram|segment0_0
   -      -     7    A    --   MEM_SGMT                1   10    0   11  |lpm_ram_dq:386|altram:sram|segment0_1
   -      -     3    A    --   MEM_SGMT                1   10    0    9  |lpm_ram_dq:386|altram:sram|segment0_2
   -      -     4    A    --   MEM_SGMT                1   10    0    4  |lpm_ram_dq:386|altram:sram|segment0_3
   -      -     6    A    --   MEM_SGMT                1   10    0    5  |lpm_ram_dq:386|altram:sram|segment0_4
   -      -     2    A    --   MEM_SGMT                1   10    0   10  |lpm_ram_dq:386|altram:sram|segment0_5
   -      -     5    A    --   MEM_SGMT                1   10    0   11  |lpm_ram_dq:386|altram:sram|segment0_6
   -      -     8    A    --   MEM_SGMT                1   10    0   10  |lpm_ram_dq:386|altram:sram|segment0_7
   -      1     -    B    21      LCELL                0    1    0    8  LWR_COL
   -      8     -    C    18      LCELL                0    1    0    9  LWR_PIC
   -      2     -    A    21        OR2                0    3    1    0  MA0
   -      3     -    B    17        OR2                0    3    1    0  MA1
   -      6     -    B    14        OR2                0    3    1    0  MA2
   -      4     -    C    17        OR2                0    3    1    0  MA3
   -      5     -    C    16        OR2                0    3    1    0  MA4
   -      8     -    B    14        OR2                0    3    1    0  MA5
   -      1     -    B    13        OR2                0    3    1    0  MA6
   -      3     -    C    23        OR2                0    3    1    0  MA7
   -      6     -    C    20        OR2                0    3    1    0  MA8
   -      2     -    C    24        OR2                0    3    1    0  MA9
   -      8     -    B    08       DFFE                0    4    0   13  MC_END
   -      3     -    B    08       DFFE        !       0    3    0    1  MC_START
   -      7     -    B    08       DFFE                0    3    0    8  MC_SYCLE
   -      3     -    B    04       DFFE   +    !       3    2    0    2  MC1
   -      8     -    B    12        OR2                0    4    0    1  MPGS0
   -      4     -    B    12        OR2                0    4    0    1  MPGS1
   -      6     -    B    01        OR2                0    4    0    1  MPGS2
   -      3     -    B    01        OR2                0    4    0    1  MPGS3
   -      8     -    C    10       DFFE    s           0    2    1    0  MXVD0~1
   -      4     -    C    10       DFFE    s           0    2    1    0  MXVD0~2
   -      3     -    B    05       DFFE    s           0    2    1    0  MXVD0~3
   -      1     -    C    10       DFFE                0    2    1    1  MXVD0
   -      2     -    A    13       DFFE    s           0    2    1    0  MXVD1~1
   -      4     -    A    13       DFFE    s           0    2    1    0  MXVD1~2
   -      5     -    A    13       DFFE    s           0    2    1    0  MXVD1~3
   -      1     -    A    13       DFFE                0    2    1    1  MXVD1
   -      1     -    A    16       DFFE    s           0    2    1    0  MXVD2~1
   -      8     -    A    16       DFFE    s           0    2    1    0  MXVD2~2
   -      7     -    A    16       DFFE    s           0    2    1    0  MXVD2~3
   -      4     -    A    12       DFFE                0    2    1    1  MXVD2
   -      6     -    C    10       DFFE    s           0    2    1    0  MXVD3~1
   -      5     -    C    10       DFFE    s           0    2    1    0  MXVD3~2
   -      7     -    C    10       DFFE    s           0    2    1    0  MXVD3~3
   -      3     -    C    10       DFFE                0    2    1    1  MXVD3
   -      3     -    A    13       DFFE    s           0    2    1    0  MXVD4~1
   -      6     -    A    13       DFFE    s           0    2    1    0  MXVD4~2
   -      8     -    A    13       DFFE    s           0    2    1    0  MXVD4~3
   -      7     -    A    01       DFFE                0    2    1    1  MXVD4
   -      6     -    A    16       DFFE    s           0    2    1    0  MXVD5~1
   -      2     -    A    16       DFFE    s           0    2    1    0  MXVD5~2
   -      3     -    A    16       DFFE    s           0    2    1    0  MXVD5~3
   -      5     -    A    16       DFFE                0    2    1    1  MXVD5
   -      8     -    B    11       DFFE    s           0    2    1    0  MXVD6~1
   -      2     -    B    11       DFFE    s           0    2    1    0  MXVD6~2
   -      5     -    B    11       DFFE    s           0    2    1    0  MXVD6~3
   -      6     -    B    11       DFFE                0    2    1    1  MXVD6
   -      5     -    A    06       DFFE    s           0    2    1    0  MXVD7~1
   -      1     -    A    06       DFFE    s           0    2    1    0  MXVD7~2
   -      4     -    A    06       DFFE    s           0    2    1    0  MXVD7~3
   -      7     -    A    06       DFFE                0    2    1    1  MXVD7
   -      3     -    B    23       DFFE        !       0    6    0    1  MXWE
   -      6     -    B    12        OR2                0    4    0    8  PGS0
   -      7     -    B    12        OR2                0    4    0    8  PGS1
   -      8     -    B    01        OR2                0    4    0    8  PGS2
   -      1     -    B    01        OR2                0    4    0    8  PGS3
   -      6     -    B    10        OR2                0    4    0    8  PGS4
   -      2     -    B    02        OR2                0    4    0    8  PGS5
   -      1     -    B    02        OR2                0    4    0    8  PGS6
   -      3     -    B    02        OR2                0    3    0    8  PGS7
   -      8     -    B    06       DFFE                0    4    0    3  PN0
   -      2     -    B    06       DFFE                0    4    0    3  PN1
   -      7     -    B    06       DFFE                0    4    0    3  PN2
   -      5     -    B    06       DFFE                0    4    0    1  PN3
   -      1     -    B    06       DFFE                0    4    0    2  PN4
   -      4     -    B    06       DFFE                0    4    0    1  PN5
   -      8     -    A    06       DFFE                0    5    0    1  PRF_CMD
   -      2     -    C    17        OR2                1    2    0    1  RA3
   -      4     -    C    16        OR2                1    2    0    1  RA4
   -      8     -    C    23        OR2                1    2    0    1  RA7
   -      7     -    C    20        OR2                1    2    0    1  RA8
   -      8     -    C    24        OR2                2    1    0    1  RA9
   -      8     -    B    17        OR2                1    2    0    1  RA12
   -      7     -    B    14        OR2                1    2    0    1  RA13
   -      2     -    C    06       DFFE                0    3    0   15  RXA0
   -      6     -    C    06       DFFE                0    3    0   10  RXA1
   -      2     -    B    12      LCELL                0    3    0    2  SC_LCELL
   -      5     -    B    10      LCELL                0    2    0    1  SC_PGS
   -      3     -    B    16       DFFE                0    4    0    4  SC0
   -      4     -    B    16       DFFE                0    4    0    1  SC1
   -      6     -    B    16       DFFE                0    4    0    4  SC4
   -      1     -    C    23        OR2    s           1    3    0    1  SD0~1
   -      6     -    C    23        OR2                0    4    1    0  SD0
   -      1     -    C    20        OR2    s           1    3    0    1  SD1~1
   -      4     -    C    20        OR2                0    4    1    0  SD1
   -      3     -    C    24        OR2    s           1    3    0    1  SD2~1
   -      1     -    C    24        OR2                0    4    1    0  SD2
   -      4     -    B    05        OR2    s           1    3    0    1  SD3~1
   -      3     -    C    04        OR2                0    4    1    0  SD3
   -      8     -    B    03        OR2    s           1    3    0    1  SD4~1
   -      1     -    A    08        OR2                0    4    1    0  SD4
   -      3     -    B    03        OR2    s           1    3    0    1  SD5~1
   -      2     -    B    03        OR2                0    4    1    0  SD5
   -      4     -    B    02        OR2    s           1    3    0    1  SD6~1
   -      5     -    B    02        OR2                0    4    1    0  SD6
   -      8     -    C    07        OR2    s           1    3    0    1  SD7~1
   -      3     -    C    07        OR2                0    4    1    0  SD7
   -      7     -    C    17       DFFE                0    5    0    4  SINC_HH
   -      3     -    C    16       DFFE                0    3    0    1  SINC_VV
   -      7     -    C    22        OR2                0    3    0    1  SVA2
   -      3     -    C    22        OR2                0    3    0    1  SVA3
   -      4     -    C    22        OR2                0    2    0    1  SVA5
   -      1     -    B    17        OR2                0    2    0    1  SVA6
   -      5     -    B    13       DFFE                0    4    0    6  SYS
   -      8     -    B    16       DFFE        !       0    4    0    1  TB_SW
   -      5     -    B    23       DFFE   +            0    3    0    1  TSN_W3
   -      6     -    C    13       DFFE   +            0    2    1    2  TURBO
   -      6     -    B    20       DFFE   +            0    3    0   31  VCM0
   -      5     -    B    20       DFFE   +            0    3    0   19  VCM1
   -      4     -    B    20       DFFE   +            0    3    0    8  VCM2
   -      2     -    C    02       DFFE   +            0    3    1    0  VLA2
   -      5     -    C    19       DFFE   +            0    3    1    0  VLA3
   -      4     -    B    23       DFFE   +            0    4    1    0  VLA4
   -      7     -    C    02       DFFE   +            0    4    1    0  VLA5
   -      6     -    B    17       DFFE   +            0    4    1    0  VLA6
   -      6     -    B    06       DFFE   +            0    4    1    0  VLA7
   -      8     -    C    02       DFFE   +            0    2    1    0  VLA8
   -      6     -    C    02       DFFE   +            0    2    1    0  VLA9
   -      5     -    A    21       DFFE   +            0    4    1    0  VLA10
   -      3     -    B    19       DFFE   +            0    3    1    0  VLA11
   -      5     -    C    02       DFFE   +            0    3    1    0  VLA12
   -      8     -    A    22       DFFE   +            0    3    1    0  VLA13
   -      2     -    B    21       DFFE   +            0    3    1    0  VLA14
   -      7     -    C    21       DFFE   +            0    3    1    0  VLA15
   -      5     -    C    21       DFFE   +            0    3    1    0  VLA16
   -      8     -    C    21       DFFE   +            0    3    1    0  VLA17
   -      7     -    B    04        OR2    s           1    2    0    1  V_WAIT~1
   -      8     -    B    23       DFFE   +    !       0    4    0    3  V_WE
   -      4     -    B    04        OR2                0    3    1    0  /WAITT
   -      1     -    B    08       AND2        !       2    2    1    1  /WE1
   -      4     -    B    21       DFFE   +            0    2    0    1  WR_COL
   -      1     -    C    06       AND2        !       0    4    0    8  WR_KBD
   -      2     -    B    23       DFFE   +            0    2    0    1  WR_PIC
   -      3     -    A    03       AND2                0    2    1    0  XC0
   -      6     -    A    03        OR2                0    2    1    0  XC1
   -      4     -    A    03        OR2                0    2    1    0  XC2
   -      3     -    B    07        OR2                0    2    1    0  XC3
   -      8     -    B    10       DFFE                0    2    0    1  :1921
   -      4     -    B    10      LCELL                1    2    0    9  :1922
   -      7     -    B    10      LCELL                0    4    0    1  :1924
   -      1     -    B    12      LCELL                0    4    0    2  :1926
   -      8     -    A    03       DFFE   +    !       2    1    0    3  :1929
   -      8     -    B    07       DFFE                0    5    0    1  :1930
   -      7     -    B    21       DFFE   +            0    2    0   10  :1958
   -      3     -    B    11       DFFE                0    2    0    1  :1962
   -      5     -    B    04       DFFE        !       1    1    0    1  :1964
   -      1     -    C    16      LCELL    s           0    1    1    0  ~1966~1
   -      7     -    A    13      LCELL    s           0    1    1    0  ~1972~1
   -      7     -    B    22      LCELL    s           0    1    1    0  ~1978~1
   -      2     -    C    10      LCELL    s           0    1    1    0  ~1984~1
   -      2     -    A    03      LCELL    s           0    1    1    0  ~1990~1
   -      3     -    C    13      LCELL    s           0    1    1    0  ~1996~1
   -      1     -    B    11      LCELL    s           0    1    1    0  ~2002~1
   -      2     -    C    04      LCELL    s           0    1    1    0  ~2008~1
   -      7     -    B    23      LCELL                0    1    1    0  :2013
   -      4     -    C    15       DFFE                0    2    1    0  :2019
   -      5     -    C    22       DFFE                0    4    0    1  :2024
   -      7     -    C    05       DFFE        !       0    3    0    1  :2032
   -      7     -    B    20       DFFE   +            0    4    1    0  :2034
   -      6     -    B    07       DFFE                0    5    0    1  :2040
   -      4     -    B    07       DFFE                0    3    0    1  :2041
   -      1     -    B    07       DFFE                0    2    0    1  :2042
   -      5     -    A    03       DFFE   +            0    5    0    1  :2043
   -      5     -    B    09      LCELL                0    4    0    8  :2054
   -      1     -    A    18       DFFE                0    2    1    1  :2058
   -      8     -    C    22       DFFE                0    5    1    0  :2061
   -      6     -    B    21       DFFE   +            0    1    0    1  :2069
   -      1     -    B    23      LCELL                0    1    1    0  :2071
   -      8     -    C    01      LCELL                0    4    0    1  :2140
   -      7     -    C    03      LCELL                0    4    0    2  :2142
   -      5     -    C    09      LCELL                0    2    0    8  :2143
   -      4     -    C    06      LCELL                1    2    0    8  :2144
   -      1     -    C    03      LCELL                0    3    0    1  :2149
   -      2     -    B    16      LCELL                1    3    0    5  :2195
   -      5     -    A    01      LCELL                0    2    0    1  :2198
   -      3     -    A    17       DFFE   +            0    3    0    1  :2199
   -      8     -    A    09      LCELL                0    4    0    1  :2200
   -      4     -    A    09       DFFE   +            0    4    0    1  :2201
   -      1     -    A    09       DFFE   +            0    4    0    1  :2202
   -      5     -    A    09       DFFE   +            0    3    0    1  :2203
   -      2     -    A    11      LCELL                0    4    0    1  :2204
   -      4     -    A    23       DFFE   +            0    3    0    1  :2205
   -      7     -    A    03       DFFE   +            0    1    0    9  :2206
   -      5     -    A    10       DFFE   +            0    3    0    2  :2207
   -      3     -    A    10       DFFE   +            0    1    0    1  :2208
   -      4     -    A    10       DFFE   +            0    1    0    1  :2209
   -      1     -    A    05      LCELL                0    4    0    1  :2213
   -      1     -    A    07      LCELL                0    4    0    1  :2214
   -      3     -    A    12      LCELL                0    4    0    1  :2215
   -      5     -    A    24       DFFE   +            0    4    0    6  :2216
   -      7     -    A    22       DFFE   +            0    4    0    9  :2217
   -      1     -    A    21      LCELL                0    3    0    1  :2218
   -      3     -    A    22       DFFE   +            0    4    0    5  :2219
   -      2     -    A    22       DFFE   +            0    3    0    6  :2220
   -      3     -    A    08       DFFE    s           0    4    1    0  ~2224~1
   -      6     -    A    08       DFFE                0    4    1    0  :2224
   -      1     -    B    10       AND2        !       0    2    0    3  :2292
   -      8     -    B    02       AND2                0    1    0    2  :2324
   -      7     -    B    07       AND2        !       1    3    0    8  :2363
   -      3     -    A    06       AND2    s           0    4    0    1  ~2463~1
   -      5     -    A    15       AND2    s           0    2    0    1  ~2463~2
   -      5     -    B    03        OR2                1    2    0   19  :3452
   -      3     -    B    22       AND2        !       0    3    0    5  :3466
   -      8     -    C    15       AND2                0    4    0    1  :3493
   -      2     -    B    13       AND2        !       0    3    0    1  :3497
   -      7     -    C    15       AND2                0    4    0    1  :3505
   -      7     -    B    13       AND2                0    4    0    2  :3511
   -      1     -    B    16       AND2        !       0    3    0    4  :3513
   -      3     -    B    06        OR2                0    3    0    6  :3534
   -      3     -    C    08       AND2    s           0    4    0    1  ~3551~1
   -      6     -    C    08       AND2                0    4    0    1  :3551
   -      4     -    A    08       AND2                1    2    0    1  :3613
   -      6     -    C    07       AND2                1    2    0    1  :3622
   -      6     -    B    03       AND2                1    2    0    8  :3626
   -      4     -    B    03       AND2                1    2    0    7  :3645
   -      2     -    C    23       AND2                0    2    0    1  :3646
   -      2     -    C    20       AND2                0    2    0    1  :3648
   -      5     -    C    24       AND2                0    2    0    1  :3650
   -      1     -    C    04       AND2                0    2    0    1  :3652
   -      7     -    B    02       AND2                2    2    0    1  :3657
   -      5     -    B    05        OR2                0    2    0    2  :3661
   -      5     -    B    24        OR2                0    3    1    0  :3682
   -      5     -    B    18        OR2                0    4    1    0  :3754
   -      4     -    B    18        OR2                0    4    1    0  :3759
   -      2     -    B    08        OR2                0    4    1    0  :3764
   -      7     -    B    18        OR2                0    4    1    0  :3769
   -      4     -    B    08        OR2    s           0    3    1    0  ~3773~1
   -      5     -    B    08        OR2                0    3    1    0  :3773
   -      4     -    B    24       AND2                0    2    0    1  :3864
   -      3     -    C    18        OR2                0    2    0    4  :4028
   -      3     -    C    21       AND2                0    3    0    4  :4039
   -      3     -    C    19       AND2                0    2    0    3  :4069
   -      6     -    C    21       AND2    s   !       0    3    0    2  ~4089~1
   -      7     -    B    01        OR2        !       0    4    0    1  :4106
   -      3     -    C    02        OR2    s           0    4    0    1  ~4228~1
   -      8     -    C    19        OR2    s           0    4    0    1  ~4231~1
   -      6     -    B    23        OR2    s           0    3    0    1  ~4234~1
   -      3     -    A    18        OR2    s           0    4    0    1  ~4246~1
   -      4     -    B    19        OR2    s           0    4    0    1  ~4249~1
   -      4     -    C    02        OR2    s           0    4    0    1  ~4252~1
   -      1     -    C    17        OR2    s           0    4    0    1  ~4255~1
   -      5     -    B    21        OR2    s           0    4    0    1  ~4258~1
   -      1     -    B    14        OR2    s           0    4    0    1  ~4261~1
   -      6     -    B    13        OR2    s           0    4    0    1  ~4264~1
   -      8     -    C    17        OR2    s           0    4    0    1  ~4267~1
   -      4     -    C    03       AND2        !       0    3    0    1  :4686
   -      2     -    C    03       AND2        !       0    3    0    3  :4724
   -      7     -    C    01       AND2    s           0    4    0    1  ~4735~1
   -      3     -    C    01       AND2    s           0    4    0    2  ~4735~2
   -      5     -    C    05       AND2    s   !       0    2    0    1  ~4777~1
   -      8     -    C    05       AND2    s           0    4    0    1  ~4777~2
   -      6     -    A    06       AND2    s           0    2    0    1  ~6697~1
   -      7     -    A    04        OR2                0    4    0    4  :6723
   -      2     -    A    08       AND2        !       0    2    0   16  :6740
   -      6     -    A    22       AND2                0    2    0    1  :6811
   -      5     -    A    07       AND2                0    2    0    2  :6813
   -      7     -    A    09        OR2        !       0    4    0    1  :6854
   -      6     -    A    10       AND2        !       0    2    0    4  :6859
   -      3     -    A    02        OR2                0    3    0    1  :6875
   -      4     -    A    02       AND2        !       0    4    0    3  :6881
   -      3     -    A    11       AND2        !       0    3    0    3  :6891
   -      6     -    A    02       AND2        !       0    2    0    1  :6910
   -      6     -    A    05       AND2                0    2    0    1  :6943
   -      2     -    A    20        OR2                0    4    0    2  :6959
   -      6     -    A    20        OR2                0    3    0    2  :6969
   -      7     -    A    20        OR2                0    3    0    2  :6979
   -      2     -    A    23       AND2                0    2    0    1  :6994
   -      6     -    A    23       AND2                0    4    0    2  :7008
   -      5     -    A    14        OR2                0    4    0    1  :7357
   -      7     -    A    14        OR2                0    3    0    1  :7364
   -      2     -    A    14        OR2                0    3    0    1  :7371
   -      7     -    A    24        OR2                0    3    0    2  :7379
   -      2     -    A    09       AND2    s           0    3    0    4  ~7404~1
   -      5     -    A    22       AND2    s           0    3    0    3  ~7404~2
   -      8     -    A    12       AND2    s           0    4    0    1  ~7491~1
   -      3     -    A    09        OR2                0    2    0    1  :7513
   -      2     -    A    17        OR2    s           0    4    0    1  ~7536~1
   -      2     -    B    05        OR2    s           0    4    0    2  ~7548~1
   -      6     -    C    15       AND2    s   !       0    3    0    1  ~7548~2
   -      7     -    C    08        OR2    s           0    4    0    1  ~7980~1
   -      5     -    C    12        OR2    s           0    4    0    1  ~7980~2
   -      1     -    C    08        OR2    s           0    3    0    1  ~7980~3
   -      2     -    C    08        OR2    s           0    3    0    1  ~7980~4
   -      8     -    C    08        OR2    s           0    3    0    1  ~7980~5
   -      2     -    B    18        OR2    s           1    2    0    2  ~8352~1
   -      2     -    C    13        OR2        !       2    0    0   17  :8372
   -      2     -    C    22        OR2                2    1    0    1  :8399
   -      6     -    B    08       AND2        !       0    3    0    1  :8459
   -      6     -    B    04       AND2        !       2    0    0    3  :8464
   -      8     -    B    21       AND2        !       0    2    0    1  :8472
   -      1     -    B    05        OR2    s   !       0    2    0    2  ~8621~1
   -      1     -    C    15       AND2    s           0    3    0    1  ~8621~2
   -      8     -    B    05       AND2    s           2    2    0    1  ~8621~3
   -      4     -    A    16        OR2                0    4    0    1  :8648
   -      2     -    B    04        OR2                2    0    0    1  :8687


Code:

s = Synthesized pin or logic cell
+ = Synchronous flipflop
/ = Slow slew-rate output
! = NOT gate push-back
r = Fitter-inserted logic cell
p = Packed register


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** FASTTRACK INTERCONNECT UTILIZATION **

Row FastTrack Interconnect:

          Global         Left Half-      Right Half-
         FastTrack       FastTrack       FastTrack 
Row     Interconnect    Interconnect    Interconnect    Input Pins     Output Pins     Bidir Pins
A:      71/ 96( 73%)    43/ 48( 89%)    38/ 48( 79%)    0/16(  0%)      4/16( 25%)    12/16( 75%)
B:      81/ 96( 84%)    40/ 48( 83%)    37/ 48( 77%)    0/16(  0%)      6/16( 37%)    10/16( 62%)
C:      78/ 96( 81%)    43/ 48( 89%)    34/ 48( 70%)    0/16(  0%)      3/16( 18%)    13/16( 81%)


Column FastTrack Interconnect:

         FastTrack                                 
Column  Interconnect    Input Pins     Output Pins     Bidir Pins
01:      4/24( 16%)     0/4(  0%)      3/4( 75%)       1/4( 25%)
02:      4/24( 16%)     0/4(  0%)      2/4( 50%)       1/4( 25%)
03:      8/24( 33%)     0/4(  0%)      2/4( 50%)       2/4( 50%)
04:      3/24( 12%)     1/4( 25%)      2/4( 50%)       0/4(  0%)
05:      4/24( 16%)     0/4(  0%)      2/4( 50%)       1/4( 25%)
06:      6/24( 25%)     0/4(  0%)      1/4( 25%)       2/4( 50%)
07:      6/24( 25%)     1/4( 25%)      1/4( 25%)       1/4( 25%)
08:      4/24( 16%)     0/4(  0%)      4/4(100%)       0/4(  0%)
09:      7/24( 29%)     0/4(  0%)      0/4(  0%)       3/4( 75%)
10:      7/24( 29%)     0/4(  0%)      0/4(  0%)       3/4( 75%)
11:      3/24( 12%)     0/4(  0%)      1/4( 25%)       2/4( 50%)
12:      3/24( 12%)     0/4(  0%)      0/4(  0%)       3/4( 75%)
13:      9/24( 37%)     0/4(  0%)      2/4( 50%)       2/4( 50%)
14:     11/24( 45%)     0/4(  0%)      1/4( 25%)       2/4( 50%)
15:     13/24( 54%)     0/4(  0%)      0/4(  0%)       3/4( 75%)
16:      8/24( 33%)     0/4(  0%)      1/4( 25%)       2/4( 50%)
17:     10/24( 41%)     0/4(  0%)      3/4( 75%)       0/4(  0%)
18:     10/24( 41%)     0/4(  0%)      3/4( 75%)       1/4( 25%)
19:      7/24( 29%)     0/4(  0%)      2/4( 50%)       1/4( 25%)
20:      7/24( 29%)     0/4(  0%)      1/4( 25%)       2/4( 50%)
21:      7/24( 29%)     0/4(  0%)      4/4(100%)       0/4(  0%)
22:      5/24( 20%)     0/4(  0%)      2/4( 50%)       1/4( 25%)
23:      6/24( 25%)     0/4(  0%)      2/4( 50%)       1/4( 25%)
24:      8/24( 33%)     0/4(  0%)      3/4( 75%)       1/4( 25%)
EA:      9/24( 37%)     0/4(  0%)      0/4(  0%)       0/4(  0%)


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** CLOCK SIGNALS **

Type     Fan-out       Name
INPUT      153         TG42
DFF         48         AY_CCC2
DFF         29         AY_CCC1
LCELL       19         :3452
DFF         17         CT2
LCELL       17         :8372
DFF         15         RXA0
DFF         13         KBD_CC
DFF         13         KB_CT2
DFF         10         CTH5
DFF         10         CTH2
DFF         10         RXA1
DFF          9         CT5
LCELL        9         LWR_PIC
DFF          9         LMC_END
DFF          8         CTV2
DFF          8         CTV8
LCELL        8         LWR_COL
DFF          8         CAS
DFF          7         CT0
DFF          7         AY_CCC8
DFF          6         CTH1
DFF          6         AY_D_WR
INPUT        6         /M1
LCELL        5         :2195
DFF          5         AY_VA3
DFF          5         CTV5
DFF          5         CTV0
DFF          4         SINC_HH
DFF          3         K_CLK
LCELL        3         :4724
LCELL        3         :8464
DFF          1         :2024
DFF          1         KB_F12
DFF          1         :2199
LCELL        1         :4686
LCELL        1         /IOWR
LCELL        1         :8459


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** CLEAR SIGNALS **

Type     Fan-out       Name
INPUT       51         /IO
INPUT       22         /RESET
LCELL       17         :8372
DFF         14         MC_END
DFF         13         KB_CT2
DFF         13         KBD_CC
DFF         10         AY_F_RES
INPUT        9         /MR
DFF          9         /IOM1
LCELL        8         BLK_R
DFF          8         BLANK
DFF          6         :2216
DFF          3         V_WE
LCELL        3         :4724
LCELL        2         CORRECT_1F
DFF          1         KB_RESET
LCELL        1         :8399
DFF          1         :2201
LCELL        1         :2198
DFF          1         :2069
DFF          1         SINC_VV
LCELL        1         :8472


Device-Specific Information:     c:\prj\sprinter\firmware\97\flex\sprint08.rpt
sprint08

** EQUATIONS **

TAPE_IN  : INPUT;
TG42     : INPUT;
/IO      : INPUT;
/MR      : INPUT;
/M1      : INPUT;
/RD      : INPUT;
/RF      : INPUT;
/WR      : INPUT;

-- Node name is 'AA0' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA0', location is LC8_A21, type is buried.
AA0      = DFFE( A0, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA1' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA1', location is LC2_B17, type is buried.
AA1      = DFFE( A1, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA2' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA2', location is LC5_B14, type is buried.
AA2      = DFFE( A2, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA3' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA3', location is LC1_C13, type is buried.
AA3      = DFFE( A3, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA4' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA4', location is LC4_C13, type is buried.
AA4      = DFFE( A4, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA5' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA5', location is LC4_B14, type is buried.
AA5      = DFFE( A5, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA6' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA6', location is LC4_B13, type is buried.
AA6      = DFFE( A6, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA7' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA7', location is LC7_C23, type is buried.
AA7      = DFFE( A7, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA8' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA8', location is LC8_C20, type is buried.
AA8      = DFFE( A8, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA9' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA9', location is LC4_C24, type is buried.
AA9      = DFFE( A9, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA10' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA10', location is LC8_C13, type is buried.
AA10     = DFFE( A10, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA11' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA11', location is LC7_C13, type is buried.
AA11     = DFFE( A11, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA12' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA12', location is LC5_B17, type is buried.
AA12     = DFFE( A12, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AA13' from file "sprint08.tdf" line 496, column 4
-- Equation name is 'AA13', location is LC3_B14, type is buried.
AA13     = DFFE( A13, !_LC2_C13,  VCC,  VCC,  VCC);

-- Node name is 'AROM16' from file "sprint08.tdf" line 314, column 2
-- Equation name is 'AROM16', location is LC4_B1, type is buried.
AROM16   = DFFE( D0,  _LC5_B3,  /RESET,  VCC,  _LC8_C15);

-- Node name is 'AR0' from file "sprint08.tdf" line 744, column 5
-- Equation name is 'AR0', location is LC5_B12, type is buried.
AR0      = LCELL( _EQ001);
  _EQ001 = !DOS &  SC_LCELL
         #  PN4 &  SC_LCELL
         # !SYS;

-- Node name is 'AR1' from file "sprint08.tdf" line 743, column 5
-- Equation name is 'AR1', location is LC3_B12, type is buried.
AR1      = LCELL( _EQ002);
  _EQ002 =  DOS &  SC_LCELL
         # !SYS;

-- Node name is 'AR2' from file "sprint08.tdf" line 742, column 5
-- Equation name is 'AR2', location is LC5_B1, type is buried.
AR2      = LCELL( _EQ003);
  _EQ003 =  AROM16 & !SYS
         #  AROM16 & !SC0;

-- Node name is 'AR3' from file "sprint08.tdf" line 741, column 11
-- Equation name is 'AR3', location is LC2_B1, type is buried.
AR3      = LCELL( _EQ004);
  _EQ004 = !SYS
         #  SC0;

-- Node name is 'AX128' from file "sprint08.tdf" line 1797, column 10
-- Equation name is 'AX128', location is LC4_A5, type is buried.
AX128    = LCELL( _EQ005);
  _EQ005 =  A15 &  PN1;

-- Node name is 'AY_AAX0' from file "sprint08.tdf" line 511, column 8
-- Equation name is 'AY_AAX0', location is LC2_A1, type is buried.
AY_AAX0  = DFFE( _EQ006,  _LC2_B16,  VCC,  VCC,  VCC);
  _EQ006 =  D0 & !D1 &  D2 &  D3;

-- Node name is 'AY_AA0' from file "sprint08.tdf" line 547, column 7
-- Equation name is 'AY_AA0', location is LC2_A19, type is buried.
AY_AA0   = DFFE( _EQ007, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ007 = !AY_ABLK &  AY_BINV &  AY_GF2 & !AY_VA0
         # !AY_ABLK & !AY_BINV &  AY_GF2 &  AY_VA0
         # !AY_ABLK &  AY_BINV & !AY_GF2 &  AY_VA0
         # !AY_ABLK & !AY_BINV & !AY_GF2 & !AY_VA0;

-- Node name is 'AY_AA1' from file "sprint08.tdf" line 547, column 7
-- Equation name is 'AY_AA1', location is LC4_A19, type is buried.
AY_AA1   = DFFE( _EQ008, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ008 = !AY_ABLK &  AY_BINV &  AY_GF2 & !AY_VA1
         # !AY_ABLK & !AY_BINV &  AY_GF2 &  AY_VA1
         # !AY_ABLK &  AY_BINV & !AY_GF2 &  AY_VA1
         # !AY_ABLK & !AY_BINV & !AY_GF2 & !AY_VA1;

-- Node name is 'AY_AA2' from file "sprint08.tdf" line 547, column 7
-- Equation name is 'AY_AA2', location is LC5_A19, type is buried.
AY_AA2   = DFFE( _EQ009, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ009 = !AY_ABLK &  AY_BINV &  AY_GF2 & !AY_VA2
         # !AY_ABLK & !AY_BINV &  AY_GF2 &  AY_VA2
         # !AY_ABLK &  AY_BINV & !AY_GF2 &  AY_VA2
         # !AY_ABLK & !AY_BINV & !AY_GF2 & !AY_VA2;

-- Node name is 'AY_AA3' from file "sprint08.tdf" line 547, column 7
-- Equation name is 'AY_AA3', location is LC6_A19, type is buried.
AY_AA3   = DFFE( _EQ010, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ010 = !AY_ABLK & !AY_BINV &  AY_GF2 &  AY_VA3
         # !AY_ABLK &  AY_BINV &  AY_GF2 & !AY_VA3
         # !AY_ABLK &  AY_BINV & !AY_GF2 &  AY_VA3
         # !AY_ABLK & !AY_BINV & !AY_GF2 & !AY_VA3;

-- Node name is 'AY_ABLK' from file "sprint08.tdf" line 3259, column 13
-- Equation name is 'AY_ABLK', location is LC3_A15, type is buried.
AY_ABLK  = DFFE(!AY_GF3, !AY_VA3,  AY_F_RES,  VCC,  VCC);

-- Node name is 'AY_ADR0' from file "sprint08.tdf" line 509, column 8
-- Equation name is 'AY_ADR0', location is LC8_A1, type is buried.
AY_ADR0  = DFFE( D0,  _LC2_B16,  VCC,  VCC,  VCC);

-- Node name is 'AY_ADR1' from file "sprint08.tdf" line 509, column 8
-- Equation name is 'AY_ADR1', location is LC6_A4, type is buried.
AY_ADR1  = DFFE( D1,  _LC2_B16,  VCC,  VCC,  VCC);

-- Node name is 'AY_ADR2' from file "sprint08.tdf" line 509, column 8
-- Equation name is 'AY_ADR2', location is LC3_A4, type is buried.
AY_ADR2  = DFFE( D2,  _LC2_B16,  VCC,  VCC,  VCC);

-- Node name is 'AY_ADR3' from file "sprint08.tdf" line 509, column 8
-- Equation name is 'AY_ADR3', location is LC2_A4, type is buried.
AY_ADR3  = DFFE( D3,  _LC2_B16,  VCC,  VCC,  VCC);

-- Node name is 'AY_AMP0' from file "sprint08.tdf" line 578, column 8
-- Equation name is 'AY_AMP0', location is LC1_A19, type is buried.
AY_AMP0  = DFFE( _EQ011, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ011 =  AY_DAT0 & !AY_DAT4
         #  AY_AA0 &  AY_DAT4
         #  AY_AA0 &  AY_DAT0;

-- Node name is 'AY_AMP1' from file "sprint08.tdf" line 578, column 8
-- Equation name is 'AY_AMP1', location is LC8_A19, type is buried.
AY_AMP1  = DFFE( _EQ012, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ012 =  AY_DAT1 & !AY_DAT4
         #  AY_AA1 &  AY_DAT4
         #  AY_AA1 &  AY_DAT1;

-- Node name is 'AY_AMP2' from file "sprint08.tdf" line 578, column 8
-- Equation name is 'AY_AMP2', location is LC3_A19, type is buried.
AY_AMP2  = DFFE( _EQ013, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ013 =  AY_DAT2 & !AY_DAT4
         #  AY_AA2 &  AY_DAT4
         #  AY_AA2 &  AY_DAT2;

-- Node name is 'AY_AMP3' from file "sprint08.tdf" line 578, column 8
-- Equation name is 'AY_AMP3', location is LC7_A19, type is buried.
AY_AMP3  = DFFE( _EQ014, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ014 =  AY_AA3 &  AY_DAT4
         #  AY_AA3 &  AY_DAT3
         #  AY_DAT3 & !AY_DAT4;

-- Node name is 'AY_AX0~1' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX0~1', location is LC6_A1, type is buried.
-- synthesized logic cell 
_LC6_A1  = LCELL( _EQ015);
  _EQ015 =  AY_ADR0 &  AY_CCC0 & !AY_CCC1
         # !AY_CCC0 & !AY_CCC1 &  AY_CCC2;

-- Node name is 'AY_AX0' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX0', location is LC1_A1, type is buried.
AY_AX0   = LCELL( _EQ016);
  _EQ016 =  AY_CCC1 &  _EC1_A
         #  _LC6_A1;

-- Node name is 'AY_AX1~1' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX1~1', location is LC8_A4, type is buried.
-- synthesized logic cell 
_LC8_A4  = LCELL( _EQ017);
  _EQ017 =  AY_ADR1 &  AY_CCC0 & !AY_CCC1
         # !AY_CCC0 & !AY_CCC1 &  AY_CCC3;

-- Node name is 'AY_AX1' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX1', location is LC5_A4, type is buried.
AY_AX1   = LCELL( _EQ018);
  _EQ018 =  AY_CCC1 &  _EC7_A
         #  _LC8_A4;

-- Node name is 'AY_AX2~1' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX2~1', location is LC1_A4, type is buried.
-- synthesized logic cell 
_LC1_A4  = LCELL( _EQ019);
  _EQ019 =  AY_ADR2 &  AY_CCC0 & !AY_CCC1
         # !AY_CCC0 & !AY_CCC1 &  AY_CCC4;

-- Node name is 'AY_AX2' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX2', location is LC1_A22, type is buried.
AY_AX2   = LCELL( _EQ020);
  _EQ020 =  AY_CCC1 &  _EC3_A
         #  _LC1_A4;

-- Node name is 'AY_AX3~1' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX3~1', location is LC4_A4, type is buried.
-- synthesized logic cell 
_LC4_A4  = LCELL( _EQ021);
  _EQ021 =  AY_ADR3 &  AY_CCC0 & !AY_CCC1
         # !AY_CCC0 & !AY_CCC1 &  AY_CCC5;

-- Node name is 'AY_AX3' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX3', location is LC1_A2, type is buried.
AY_AX3   = LCELL( _EQ022);
  _EQ022 =  AY_CCC1 &  _EC4_A
         #  _LC4_A4;

-- Node name is 'AY_AX4' from file "sprint08.tdf" line 3140, column 13
-- Equation name is 'AY_AX4', location is LC3_A24, type is buried.
AY_AX4   = LCELL( _EQ023);
  _EQ023 =  AY_CCC1 &  _EC6_A
         # !AY_CCC0 & !AY_CCC1 &  AY_CCC6;

-- Node name is 'AY_AX5' from file "sprint08.tdf" line 3132, column 13
-- Equation name is 'AY_AX5', location is LC5_A8, type is buried.
AY_AX5   = LCELL( _EQ024);
  _EQ024 = !AY_CCC0 & !AY_CCC1 &  AY_CCC7;

-- Node name is 'AY_BBLK' from file "sprint08.tdf" line 3257, column 13
-- Equation name is 'AY_BBLK', location is LC6_A15, type is buried.
AY_BBLK  = DFFE( AY_GF0, !AY_VA3,  AY_F_RES,  VCC,  VCC);

-- Node name is 'AY_BINV' from file "sprint08.tdf" line 3261, column 13
-- Equation name is 'AY_BINV', location is LC2_A15, type is buried.
AY_BINV  = DFFE( _EQ025, !AY_VA3,  AY_F_RES,  VCC,  VCC);
  _EQ025 = !AY_BINV &  AY_GF0 & !AY_GF1
         # !AY_BINV & !AY_GF0 &  AY_GF1;

-- Node name is 'AY_C' from file "sprint08.tdf" line 560, column 2
-- Equation name is 'AY_C', location is LC8_A11, type is buried.
AY_C     = DFFE( _EQ026, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ026 = !_EC5_A & !_EC8_A & !_LC3_A11;

-- Node name is 'AY_CCC0' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC0', location is LC1_B20, type is buried.
AY_CCC0  = DFFE( CT0, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC1' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC1', location is LC8_A10, type is buried.
AY_CCC1  = DFFE( AY_CCC0, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC2' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC2', location is LC7_B11, type is buried.
AY_CCC2  = DFFE( CT2, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC3' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC3', location is LC3_B21, type is buried.
AY_CCC3  = DFFE( CT3, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC4' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC4', location is LC2_B24, type is buried.
AY_CCC4  = DFFE( CT4, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC5' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC5', location is LC8_A24, type is buried.
AY_CCC5  = DFFE( CT5, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC6' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC6', location is LC1_A24, type is buried.
AY_CCC6  = DFFE( CTH0, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC7' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC7', location is LC7_A8, type is buried.
AY_CCC7  = DFFE( CTH1, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CCC8' from file "sprint08.tdf" line 556, column 8
-- Equation name is 'AY_CCC8', location is LC6_A24, type is buried.
AY_CCC8  = DFFE( CTH2, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'AY_CX' from file "sprint08.tdf" line 561, column 2
-- Equation name is 'AY_CX', location is LC6_A9, type is buried.
!AY_CX   = AY_CX~NOT;
AY_CX~NOT = DFFE(!_LC7_A9, GLOBAL( TG42), !_LC4_A9,  VCC,  _LC1_A9);

-- Node name is 'AY_DAT_WR' from file "sprint08.tdf" line 571, column 2
-- Equation name is 'AY_DAT_WR', location is LC1_A3, type is buried.
AY_DAT_WR = DFFE( _EC5_A, GLOBAL( TG42),  VCC,  VCC,  AY_CCC1);

-- Node name is 'AY_DAT0' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT0', location is LC7_A10, type is buried.
AY_DAT0  = DFFE( _EQ027, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ027 =  _EC1_A & !_LC5_A10
         # !_EC1_A &  _LC5_A10;

-- Node name is 'AY_DAT1' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT1', location is LC8_A2, type is buried.
AY_DAT1  = DFFE( _EQ028, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ028 = !_EC7_A & !_LC6_A10
         #  _EC7_A &  _LC6_A10;

-- Node name is 'AY_DAT2' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT2', location is LC5_A2, type is buried.
AY_DAT2  = DFFE( _EQ029, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ029 = !_EC3_A & !_EC7_A & !_LC6_A10
         #  _EC3_A &  _EC7_A
         #  _EC3_A &  _LC6_A10;

-- Node name is 'AY_DAT3' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT3', location is LC7_A2, type is buried.
AY_DAT3  = DFFE( _EQ030, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ030 = !_EC4_A & !_LC3_A2
         #  _EC4_A &  _LC3_A2;

-- Node name is 'AY_DAT4' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT4', location is LC4_A11, type is buried.
AY_DAT4  = DFFE( _EQ031, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ031 = !_EC6_A & !_LC4_A2
         #  _EC6_A &  _LC4_A2;

-- Node name is 'AY_DAT5' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT5', location is LC7_A11, type is buried.
AY_DAT5  = DFFE( _EQ032, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ032 = !_EC2_A & !_EC6_A & !_LC4_A2
         #  _EC2_A &  _EC6_A
         #  _EC2_A &  _LC4_A2;

-- Node name is 'AY_DAT6' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT6', location is LC5_A11, type is buried.
AY_DAT6  = DFFE( _EQ033, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ033 = !_EC5_A & !_LC3_A11
         #  _EC5_A &  _LC3_A11;

-- Node name is 'AY_DAT7' from file "sprint08.tdf" line 572, column 8
-- Equation name is 'AY_DAT7', location is LC6_A11, type is buried.
AY_DAT7  = DFFE( _EQ034, GLOBAL( TG42),  VCC,  VCC,  _LC7_A3);
  _EQ034 = !_EC5_A & !_EC8_A & !_LC3_A11
         #  _EC5_A &  _EC8_A
         #  _EC8_A &  _LC3_A11;

-- Node name is 'AY_DD0' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD0', location is LC5_C23, type is buried.
AY_DD0   = DFFE( _EC1_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD1' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD1', location is LC5_C20, type is buried.
AY_DD1   = DFFE( _EC7_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD2' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD2', location is LC7_C24, type is buried.
AY_DD2   = DFFE( _EC3_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD3' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD3', location is LC8_C4, type is buried.
AY_DD3   = DFFE( _EC4_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD4' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD4', location is LC8_A8, type is buried.
AY_DD4   = DFFE( _EC6_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD5' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD5', location is LC7_B3, type is buried.
AY_DD5   = DFFE( _EC2_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD6' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD6', location is LC6_B2, type is buried.
AY_DD6   = DFFE( _EC5_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DD7' from file "sprint08.tdf" line 580, column 7
-- Equation name is 'AY_DD7', location is LC7_C7, type is buried.
AY_DD7   = DFFE( _EC8_A, GLOBAL( TG42),  VCC,  VCC, !_LC2_A8);

-- Node name is 'AY_DI0' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI0', location is LC2_A10, type is buried.
AY_DI0   = LCELL( _EQ035);
  _EQ035 =  AY_CCC0 & !AY_CCC1 &  MXVD0
         #  AY_CCC1 &  AY_DAT0
         # !AY_CCC0 &  AY_DAT0;

-- Node name is 'AY_DI1' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI1', location is LC2_A24, type is buried.
AY_DI1   = LCELL( _EQ036);
  _EQ036 =  AY_CCC0 & !AY_CCC1 &  MXVD1
         #  AY_CCC1 &  AY_DAT1
         # !AY_CCC0 &  AY_DAT1;

-- Node name is 'AY_DI2' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI2', location is LC6_A12, type is buried.
AY_DI2   = LCELL( _EQ037);
  _EQ037 =  AY_CCC0 & !AY_CCC1 &  MXVD2
         #  AY_CCC1 &  AY_DAT2
         # !AY_CCC0 &  AY_DAT2;

-- Node name is 'AY_DI3' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI3', location is LC2_A2, type is buried.
AY_DI3   = LCELL( _EQ038);
  _EQ038 =  AY_CCC0 & !AY_CCC1 &  MXVD3
         #  AY_CCC1 &  AY_DAT3
         # !AY_CCC0 &  AY_DAT3;

-- Node name is 'AY_DI4' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI4', location is LC4_A1, type is buried.
AY_DI4   = LCELL( _EQ039);
  _EQ039 =  AY_CCC0 & !AY_CCC1 &  MXVD4
         #  AY_CCC1 &  AY_DAT4
         # !AY_CCC0 &  AY_DAT4;

-- Node name is 'AY_DI5' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI5', location is LC2_A12, type is buried.
AY_DI5   = LCELL( _EQ040);
  _EQ040 =  AY_CCC0 & !AY_CCC1 &  MXVD5
         #  AY_CCC1 &  AY_DAT5
         # !AY_CCC0 &  AY_DAT5;

-- Node name is 'AY_DI6' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI6', location is LC3_A1, type is buried.
AY_DI6   = LCELL( _EQ041);
  _EQ041 =  AY_CCC0 & !AY_CCC1 &  MXVD6
         #  AY_CCC1 &  AY_DAT6
         # !AY_CCC0 &  AY_DAT6;

-- Node name is 'AY_DI7' from file "sprint08.tdf" line 3143, column 13
-- Equation name is 'AY_DI7', location is LC1_A11, type is buried.
AY_DI7   = LCELL( _EQ042);
  _EQ042 =  AY_CCC0 & !AY_CCC1 &  MXVD7
         #  AY_CCC1 &  AY_DAT7
         # !AY_CCC0 &  AY_DAT7;

-- Node name is 'AY_D_WR' from file "sprint08.tdf" line 3114, column 13
-- Equation name is 'AY_D_WR', location is LC7_B16, type is buried.
!AY_D_WR = AY_D_WR~NOT;
AY_D_WR~NOT = DFFE( _EQ043, !/IOWR, GLOBAL(!/IO),  VCC,  VCC);
  _EQ043 =  DD0 & !DD1 & !DD2 & !_LC2_B5;

-- Node name is 'AY_F_RES' from file "sprint08.tdf" line 3116, column 13
-- Equation name is 'AY_F_RES', location is LC7_A17, type is buried.
AY_F_RES = DFFE( VCC,  _LC3_A17,  _LC5_A1,  VCC,  VCC);

-- Node name is 'AY_GF0' from file "sprint08.tdf" line 530, column 7
-- Equation name is 'AY_GF0', location is LC7_A15, type is buried.
AY_GF0   = DFFE( _EQ044,  AY_D_WR,  /RESET,  VCC,  VCC);
  _EQ044 =  D0 & !_LC7_A4
         #  AY_GF0 &  _LC7_A4;

-- Node name is 'AY_GF1' from file "sprint08.tdf" line 530, column 7
-- Equation name is 'AY_GF1', location is LC4_A15, type is buried.
AY_GF1   = DFFE( _EQ045,  AY_D_WR,  /RESET,  VCC,  VCC);
  _EQ045 =  D1 & !_LC7_A4
         #  AY_GF1 &  _LC7_A4;

-- Node name is 'AY_GF2' from file "sprint08.tdf" line 530, column 7
-- Equation name is 'AY_GF2', location is LC1_A15, type is buried.
AY_GF2   = DFFE( _EQ046,  AY_D_WR,  /RESET,  VCC,  VCC);
  _EQ046 =  D2 & !_LC7_A4
         #  AY_GF2 &  _LC7_A4;

-- Node name is 'AY_GF3' from file "sprint08.tdf" line 530, column 7
-- Equation name is 'AY_GF3', location is LC8_A15, type is buried.
AY_GF3   = DFFE( _EQ047,  AY_D_WR,  /RESET,  VCC,  VCC);
  _EQ047 =  D3 & !_LC7_A4
         #  AY_GF3 &  _LC7_A4;

-- Node name is 'AY_OUTS1' from file "sprint08.tdf" line 3180, column 13
-- Equation name is 'AY_OUTS1', location is LC4_A22, type is buried.
AY_OUTS1 = DFFE( _EQ048, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ048 = !_EC3_A & !_EC7_A &  _LC2_A9 &  _LC6_A22;

-- Node name is 'AY_OUTS2' from file "sprint08.tdf" line 3181, column 13
-- Equation name is 'AY_OUTS2', location is LC7_A7, type is buried.
AY_OUTS2 = DFFE( _EQ049, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ049 = !_EC1_A & !_EC3_A &  _LC2_A9 &  _LC5_A7;

-- Node name is 'AY_OUTS3' from file "sprint08.tdf" line 3182, column 13
-- Equation name is 'AY_OUTS3', location is LC6_A7, type is buried.
AY_OUTS3 = DFFE( _EQ050, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ050 =  _EC1_A & !_EC3_A &  _LC2_A9 &  _LC5_A7;

-- Node name is 'AY_OUT1' from file "sprint08.tdf" line 537, column 8
-- Equation name is 'AY_OUT1', location is LC3_A5, type is buried.
AY_OUT1  = DFFE( _EQ051, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ051 = !AY_CX &  AY_OUT1
         #  AY_CX &  AY_OUTS1 & !AY_OUT1
         # !AY_OUTS1 &  AY_OUT1;

-- Node name is 'AY_OUT2' from file "sprint08.tdf" line 537, column 8
-- Equation name is 'AY_OUT2', location is LC2_A7, type is buried.
AY_OUT2  = DFFE( _EQ052, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ052 = !AY_CX &  AY_OUT2
         #  AY_CX &  AY_OUTS2 & !AY_OUT2
         # !AY_OUTS2 &  AY_OUT2;

-- Node name is 'AY_OUT3' from file "sprint08.tdf" line 537, column 8
-- Equation name is 'AY_OUT3', location is LC1_A12, type is buried.
AY_OUT3  = DFFE( _EQ053, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ053 = !AY_CX &  AY_OUT3
         #  AY_CX &  AY_OUTS3 & !AY_OUT3
         # !AY_OUTS3 &  AY_OUT3;

-- Node name is 'AY_Q' from file "sprint08.tdf" line 3205, column 67
-- Equation name is 'AY_Q', location is LC5_A5, type is buried.
AY_Q     = LCELL( _EQ054);
  _EQ054 =  _LC8_A7
         #  AY_OUTS1 &  _LC1_A5;

-- Node name is 'AY_Q~1' from file "sprint08.tdf" line 3205, column 67
-- Equation name is 'AY_Q~1', location is LC8_A7, type is buried.
-- synthesized logic cell 
_LC8_A7  = LCELL( _EQ055);
  _EQ055 =  AY_OUTS2 &  _LC1_A7
         #  AY_OUTS3 &  _LC3_A12;

-- Node name is 'AY_SHR' from file "sprint08.tdf" line 546, column 2
-- Equation name is 'AY_SHR', location is LC3_A21, type is buried.
AY_SHR   = DFFE( _LC1_A21, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH0' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH0', location is LC1_A17, type is buried.
AY_SH0   = DFFE( AY_SH1, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH1' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH1', location is LC8_A17, type is buried.
AY_SH1   = DFFE( AY_SH2, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH2' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH2', location is LC5_A17, type is buried.
AY_SH2   = DFFE( AY_SH3, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH3' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH3', location is LC4_A17, type is buried.
AY_SH3   = DFFE( AY_SH4, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH4' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH4', location is LC6_A17, type is buried.
AY_SH4   = DFFE( AY_SH5, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH5' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH5', location is LC6_A21, type is buried.
AY_SH5   = DFFE( AY_SH6, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH6' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH6', location is LC7_A21, type is buried.
AY_SH6   = DFFE( AY_SH7, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_SH7' from file "sprint08.tdf" line 545, column 7
-- Equation name is 'AY_SH7', location is LC4_A21, type is buried.
AY_SH7   = DFFE( AY_SHR, GLOBAL( TG42),  VCC,  VCC,  _LC7_A22);

-- Node name is 'AY_VAR' from file "sprint08.tdf" line 567, column 2
-- Equation name is 'AY_VAR', location is LC3_A23, type is buried.
AY_VAR   = DFFE( _EQ056, GLOBAL( TG42),  AY_F_RES,  VCC,  _LC3_A22);
  _EQ056 = !AY_CX &  AY_VAR
         #  AY_CX & !AY_VAR;

-- Node name is 'AY_VA0' from file "sprint08.tdf" line 566, column 7
-- Equation name is 'AY_VA0', location is LC8_A23, type is buried.
AY_VA0   = DFFE( _EQ057, GLOBAL( TG42),  AY_F_RES,  VCC,  _LC3_A22);
  _EQ057 = !AY_CX &  AY_VA0
         # !AY_VAR &  AY_VA0
         #  AY_CX &  AY_VAR & !AY_VA0;

-- Node name is 'AY_VA1' from file "sprint08.tdf" line 566, column 7
-- Equation name is 'AY_VA1', location is LC1_A23, type is buried.
AY_VA1   = DFFE( _EQ058, GLOBAL( TG42),  AY_F_RES,  VCC,  _LC3_A22);
  _EQ058 =  AY_VA1 & !_LC2_A23
         # !AY_VA0 &  AY_VA1
         #  AY_VA0 & !AY_VA1 &  _LC2_A23;

-- Node name is 'AY_VA2' from file "sprint08.tdf" line 566, column 7
-- Equation name is 'AY_VA2', location is LC7_A23, type is buried.
AY_VA2   = DFFE( _EQ059, GLOBAL( TG42),  AY_F_RES,  VCC,  _LC3_A22);
  _EQ059 =  AY_VA2 & !_LC6_A23
         # !AY_VA2 &  _LC6_A23;

-- Node name is 'AY_VA3' from file "sprint08.tdf" line 566, column 7
-- Equation name is 'AY_VA3', location is LC5_A23, type is buried.
AY_VA3   = DFFE( _EQ060, GLOBAL( TG42),  AY_F_RES,  VCC,  _LC3_A22);
  _EQ060 = !AY_VA2 &  AY_VA3
         #  AY_VA3 & !_LC6_A23
         #  AY_VA2 & !AY_VA3 &  _LC6_A23;

-- Node name is 'AY_WR' from file "sprint08.tdf" line 3141, column 11
-- Equation name is 'AY_WR', location is LC1_A10, type is buried.
AY_WR    = LCELL( _EQ061);
  _EQ061 =  AY_CCC1 & !_LC8_A9
         #  AY_CCC0 & !AY_CCC1 & !AY_D_WR;

-- Node name is 'AY_XXM0' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM0', location is LC3_A14, type is buried.
AY_XXM0  = DFFE( AY_XX0, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XXM1' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM1', location is LC4_A14, type is buried.
AY_XXM1  = DFFE( AY_XX1, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XXM2' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM2', location is LC6_A14, type is buried.
AY_XXM2  = DFFE( AY_XX2, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XXM3' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM3', location is LC8_A14, type is buried.
AY_XXM3  = DFFE( AY_XX3, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XXM4' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM4', location is LC4_A24, type is buried.
AY_XXM4  = DFFE( AY_XX4, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XXM5' from file "sprint08.tdf" line 569, column 8
-- Equation name is 'AY_XXM5', location is LC1_A14, type is buried.
AY_XXM5  = DFFE( AY_XX5, !AY_CCC8,  VCC,  VCC,  VCC);

-- Node name is 'AY_XX0' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX0', location is LC2_A5, type is buried.
AY_XX0   = DFFE( _EQ062, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ062 = !AY_AMP0 &  AY_XX0
         #  AY_AMP0 & !AY_XX0;

-- Node name is 'AY_XX1' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX1', location is LC3_A20, type is buried.
AY_XX1   = DFFE( _EQ063, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ063 = !AY_AMP1 & !AY_XX1 &  _LC6_A5
         #  AY_AMP1 &  AY_XX1 &  _LC6_A5
         #  AY_AMP1 & !AY_XX1 & !_LC6_A5
         # !AY_AMP1 &  AY_XX1 & !_LC6_A5;

-- Node name is 'AY_XX2' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX2', location is LC8_A20, type is buried.
AY_XX2   = DFFE( _EQ064, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ064 = !AY_AMP2 & !AY_XX2 &  _LC2_A20
         #  AY_AMP2 &  AY_XX2 &  _LC2_A20
         #  AY_AMP2 & !AY_XX2 & !_LC2_A20
         # !AY_AMP2 &  AY_XX2 & !_LC2_A20;

-- Node name is 'AY_XX3' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX3', location is LC5_A20, type is buried.
AY_XX3   = DFFE( _EQ065, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ065 = !AY_AMP3 & !AY_XX3 &  _LC6_A20
         #  AY_AMP3 &  AY_XX3 &  _LC6_A20
         #  AY_AMP3 & !AY_XX3 & !_LC6_A20
         # !AY_AMP3 &  AY_XX3 & !_LC6_A20;

-- Node name is 'AY_XX4' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX4', location is LC1_A20, type is buried.
AY_XX4   = DFFE( _EQ066, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ066 =  AY_XX4 & !_LC7_A20
         # !AY_XX4 &  _LC7_A20;

-- Node name is 'AY_XX5' from file "sprint08.tdf" line 568, column 7
-- Equation name is 'AY_XX5', location is LC4_A20, type is buried.
AY_XX5   = DFFE( _EQ067, GLOBAL( TG42),  _LC5_A24,  VCC,  AY_Q);
  _EQ067 = !AY_XX4 &  AY_XX5
         #  AY_XX5 & !_LC7_A20
         #  AY_XX4 & !AY_XX5 &  _LC7_A20;

-- Node name is 'AY_X_0' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_0', location is LC8_A5, type is buried.
AY_X_0   = DFFE( AY_DAT0, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'AY_X_1' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_1', location is LC4_A7, type is buried.
AY_X_1   = DFFE( AY_DAT1, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'AY_X_2' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_2', location is LC7_A12, type is buried.
AY_X_2   = DFFE( AY_DAT2, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'AY_X_3' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_3', location is LC7_A5, type is buried.
AY_X_3   = DFFE( AY_DAT3, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'AY_X_4' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_4', location is LC3_A7, type is buried.
AY_X_4   = DFFE( AY_DAT4, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'AY_X_5' from file "sprint08.tdf" line 516, column 7
-- Equation name is 'AY_X_5', location is LC5_A12, type is buried.
AY_X_5   = DFFE( AY_DAT5, GLOBAL( TG42),  VCC,  VCC,  _LC2_A22);

-- Node name is 'A0' from file "sprint08.tdf" line 700, column 29
-- Equation name is 'A0', type is bidir 
A0       = TRI(GND,  GND);

-- Node name is 'A1' from file "sprint08.tdf" line 700, column 29
-- Equation name is 'A1', type is bidir 
A1       = TRI(GND,  GND);

-- Node name is 'A2' from file "sprint08.tdf" line 700, column 29
-- Equation name is 'A2', type is bidir 
A2       = TRI(GND,  GND);

-- Node name is 'A3' from file "sprint08.tdf" line 700, column 29
-- Equation name is 'A3', type is bidir 
A3       = TRI(GND,  GND);

-- Node name is 'A4' from file "sprint08.tdf" line 702, column 3
-- Equation name is 'A4', type is bidir 
A4       = TRI(GND,  GND);

-- Node name is 'A5' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A5', type is bidir 
A5       = TRI(GND,  GND);

-- Node name is 'A6' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A6', type is bidir 
A6       = TRI(GND,  GND);

-- Node name is 'A7' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A7', type is bidir 
A7       = TRI(GND,  GND);

-- Node name is 'A8' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A8', type is bidir 
A8       = TRI(GND,  GND);

-- Node name is 'A9' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A9', type is bidir 
A9       = TRI(GND,  GND);

-- Node name is 'A10' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A10', type is bidir 
A10      = TRI(GND,  GND);

-- Node name is 'A11' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A11', type is bidir 
A11      = TRI(GND,  GND);

-- Node name is 'A12' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A12', type is bidir 
A12      = TRI(GND,  GND);

-- Node name is 'A13' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A13', type is bidir 
A13      = TRI(GND,  GND);

-- Node name is 'A14' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A14', type is bidir 
A14      = TRI(GND,  GND);

-- Node name is 'A15' from file "sprint08.tdf" line 701, column 29
-- Equation name is 'A15', type is bidir 
A15      = TRI(GND,  GND);

-- Node name is 'BEEPER' from file "sprint08.tdf" line 1456, column 17
-- Equation name is 'BEEPER', type is output 
BEEPER   =  _LC5_B24;

-- Node name is 'BLANK' from file "sprint08.tdf" line 1727, column 10
-- Equation name is 'BLANK', location is LC8_C16, type is buried.
!BLANK   = BLANK~NOT;
BLANK~NOT = DFFE( _EQ068,  CTH2, !SINC_VV,  VCC,  VCC);
  _EQ068 =  CTH4
         # !CTH5;

-- Node name is 'BLK_R' from file "sprint08.tdf" line 767, column 10
-- Equation name is 'BLK_R', location is LC2_B10, type is buried.
BLK_R    = LCELL( _EQ069);
  _EQ069 =  _LC7_B10 & !/MR &  /RF;

-- Node name is 'BORD' from file "sprint08.tdf" line 1732, column 9
-- Equation name is 'BORD', location is LC6_C18, type is buried.
BORD     = DFFE( _EQ070,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ070 =  CTV6 &  CTV7
         #  CTH5
         #  CTV8;

-- Node name is 'BRD0' from file "sprint08.tdf" line 316, column 5
-- Equation name is 'BRD0', location is LC2_B22, type is buried.
BRD0     = DFFE( D0,  _LC5_B3,  VCC,  VCC, !_LC3_B22);

-- Node name is 'BRD1' from file "sprint08.tdf" line 316, column 5
-- Equation name is 'BRD1', location is LC5_B22, type is buried.
BRD1     = DFFE( D1,  _LC5_B3,  VCC,  VCC, !_LC3_B22);

-- Node name is 'BRD2' from file "sprint08.tdf" line 316, column 5
-- Equation name is 'BRD2', location is LC1_B22, type is buried.
BRD2     = DFFE( D2,  _LC5_B3,  VCC,  VCC, !_LC3_B22);

-- Node name is 'BRD3' from file "sprint08.tdf" line 316, column 5
-- Equation name is 'BRD3', location is LC6_B22, type is buried.
BRD3     = DFFE( D3,  _LC5_B3,  VCC,  VCC, !_LC3_B22);

-- Node name is 'BRD4' from file "sprint08.tdf" line 316, column 5
-- Equation name is 'BRD4', location is LC7_B24, type is buried.
BRD4     = DFFE( D4,  _LC5_B3,  VCC,  VCC, !_LC3_B22);

-- Node name is 'CAS' from file "sprint08.tdf" line 1577, column 8
-- Equation name is 'CAS', location is LC2_B14, type is buried.
CAS      = DFFE( _EQ071, GLOBAL(!TG42),  VCC,  VCC,  VCC);
  _EQ071 = !AY_CCC0 & !CT2
         #  AY_CCC0 &  CT2;

-- Node name is 'CAS_0' from file "sprint08.tdf" line 1612, column 2
-- Equation name is 'CAS_0', type is output 
CAS_0    =  _LC5_B18;

-- Node name is 'CAS_1' from file "sprint08.tdf" line 1613, column 2
-- Equation name is 'CAS_1', type is output 
CAS_1    =  _LC4_B18;

-- Node name is 'CAS_2' from file "sprint08.tdf" line 1614, column 2
-- Equation name is 'CAS_2', type is output 
CAS_2    =  _LC2_B8;

-- Node name is 'CAS_3' from file "sprint08.tdf" line 1615, column 2
-- Equation name is 'CAS_3', type is output 
CAS_3    =  _LC7_B18;

-- Node name is 'CLK_PIX' from file "sprint08.tdf" line 1450, column 2
-- Equation name is 'CLK_PIX', type is output 
CLK_PIX  =  _LC7_B23;

-- Node name is 'CLKZ1' from file "sprint08.tdf" line 1529, column 2
-- Equation name is 'CLKZ1', type is output 
CLKZ1    =  _LC7_B20;

-- Node name is 'CNF3' from file "sprint08.tdf" line 418, column 5
-- Equation name is 'CNF3', location is LC3_B13, type is buried.
CNF3     = DFFE( D3,  _LC5_B3,  /RESET,  VCC,  _LC7_B13);

-- Node name is 'CNF4' from file "sprint08.tdf" line 418, column 5
-- Equation name is 'CNF4', location is LC8_B13, type is buried.
CNF4     = DFFE( D4,  _LC5_B3,  /RESET,  VCC,  _LC7_B13);

-- Node name is 'CORRECT_1F' from file "sprint08.tdf" line 859, column 16
-- Equation name is 'CORRECT_1F', location is LC7_B5, type is buried.
CORRECT_1F = LCELL( _EQ072);
  _EQ072 =  _LC1_B5 &  _LC1_C15 & !_LC5_B5 &  _LC8_B5;

-- Node name is 'CTF0' from file "sprint08.tdf" line 323, column 5
-- Equation name is 'CTF0', location is LC2_C19, type is buried.
CTF0     = DFFE(!CTF0, !CTV8,  VCC,  VCC,  VCC);

-- Node name is 'CTF1' from file "sprint08.tdf" line 323, column 5
-- Equation name is 'CTF1', location is LC1_C19, type is buried.
CTF1     = DFFE( _EQ073, !CTV8,  VCC,  VCC,  VCC);
  _EQ073 =  CTF0 & !CTF1
         # !CTF0 &  CTF1;

-- Node name is 'CTF2' from file "sprint08.tdf" line 323, column 5
-- Equation name is 'CTF2', location is LC4_C19, type is buried.
CTF2     = DFFE( _EQ074, !CTV8,  VCC,  VCC,  VCC);
  _EQ074 =  CTF2 & !_LC3_C19
         # !CTF2 &  _LC3_C19;

-- Node name is 'CTF3' from file "sprint08.tdf" line 323, column 5
-- Equation name is 'CTF3', location is LC6_C19, type is buried.
CTF3     = DFFE( _EQ075, !CTV8,  VCC,  VCC,  VCC);
  _EQ075 = !CTF2 &  CTF3
         #  CTF3 & !_LC3_C19
         #  CTF2 & !CTF3 &  _LC3_C19;

-- Node name is 'CTF4' from file "sprint08.tdf" line 323, column 5
-- Equation name is 'CTF4', location is LC7_C19, type is buried.
CTF4     = DFFE( _EQ076, !CTV8,  VCC,  VCC,  VCC);
  _EQ076 = !CTF2 &  CTF4
         #  CTF4 & !_LC3_C19
         # !CTF3 &  CTF4
         #  CTF2 &  CTF3 & !CTF4 &  _LC3_C19;

-- Node name is 'CTH0' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH0', location is LC4_A18, type is buried.
CTH0     = DFFE(!CTH0, !CT5,  VCC,  VCC,  VCC);

-- Node name is 'CTH1' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH1', location is LC6_A18, type is buried.
CTH1     = DFFE( _EQ077, !CT5,  VCC,  VCC,  VCC);
  _EQ077 = !CTH0 &  CTH1
         #  CTH0 & !CTH1;

-- Node name is 'CTH2' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH2', location is LC2_A18, type is buried.
CTH2     = DFFE( _EQ078, !CT5,  VCC,  VCC,  VCC);
  _EQ078 = !CTH1 &  CTH2
         # !CTH0 &  CTH2
         #  CTH0 &  CTH1 & !CTH2;

-- Node name is 'CTH3' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH3', location is LC3_C17, type is buried.
CTH3     = DFFE( _EQ079, !CTH2,  VCC,  VCC,  VCC);
  _EQ079 = !CTH3 & !CTH4
         # !CTH3 & !CTH5;

-- Node name is 'CTH4' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH4', location is LC5_C17, type is buried.
CTH4     = DFFE( _EQ080, !CTH2,  VCC,  VCC,  VCC);
  _EQ080 =  CTH3 & !CTH4
         # !CTH3 &  CTH4 & !CTH5;

-- Node name is 'CTH5' from file "sprint08.tdf" line 321, column 5
-- Equation name is 'CTH5', location is LC6_C17, type is buried.
CTH5     = DFFE( _EQ081, !CTH2,  VCC,  VCC,  VCC);
  _EQ081 = !CTH4 &  CTH5
         #  CTH3 &  CTH4 & !CTH5;

-- Node name is 'CTV0' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV0', location is LC5_C15, type is buried.
CTV0     = DFFE(!CTV0,  SINC_HH,  VCC,  VCC,  VCC);

-- Node name is 'CTV1' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV1', location is LC2_C15, type is buried.
CTV1     = DFFE( _EQ082,  SINC_HH,  VCC,  VCC,  VCC);
  _EQ082 =  CTV0 & !CTV1
         # !CTV0 &  CTV1;

-- Node name is 'CTV2' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV2', location is LC3_C15, type is buried.
CTV2     = DFFE( _EQ083,  SINC_HH,  VCC,  VCC,  VCC);
  _EQ083 = !CTV0 &  CTV2
         # !CTV1 &  CTV2
         #  CTV0 &  CTV1 & !CTV2;

-- Node name is 'CTV3' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV3', location is LC1_C21, type is buried.
CTV3     = DFFE(!CTV3, !CTV2,  VCC,  VCC,  VCC);

-- Node name is 'CTV4' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV4', location is LC4_C21, type is buried.
CTV4     = DFFE( _EQ084, !CTV2,  VCC,  VCC,  VCC);
  _EQ084 = !CTV3 &  CTV4 &  _LC3_C18
         #  CTV3 & !CTV4 &  _LC3_C18;

-- Node name is 'CTV5' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV5', location is LC2_C21, type is buried.
CTV5     = DFFE( _EQ085, !CTV2,  VCC,  VCC,  VCC);
  _EQ085 = !CTV4 &  CTV5 &  _LC3_C18
         # !CTV3 &  CTV5 &  _LC3_C18
         #  CTV3 &  CTV4 & !CTV5 &  _LC3_C18;

-- Node name is 'CTV6' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV6', location is LC2_C18, type is buried.
CTV6     = DFFE( _EQ086, !CTV2,  VCC,  VCC,  VCC);
  _EQ086 =  CTV6 &  _LC3_C18 & !_LC3_C21
         # !CTV6 &  _LC3_C18 &  _LC3_C21;

-- Node name is 'CTV7' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV7', location is LC1_C18, type is buried.
CTV7     = DFFE( _EQ087, !CTV2,  VCC,  VCC,  VCC);
  _EQ087 = !CTV6 &  CTV7 &  _LC3_C18
         #  CTV7 &  _LC3_C18 & !_LC3_C21
         #  CTV6 & !CTV7 &  _LC3_C18 &  _LC3_C21;

-- Node name is 'CTV8' from file "sprint08.tdf" line 322, column 5
-- Equation name is 'CTV8', location is LC5_C18, type is buried.
CTV8     = DFFE( _EQ088, !CTV2,  VCC,  VCC,  VCC);
  _EQ088 =  CTV8 & !_LC3_C21
         #  CTV6 &  CTV7 & !CTV8 &  _LC3_C21;

-- Node name is 'CT0' from file "sprint08.tdf" line 296, column 4
-- Equation name is 'CT0', location is LC8_B20, type is buried.
CT0      = DFFE( _EQ089, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ089 = !AY_CCC0 & !CT0;

-- Node name is 'CT2' from file "sprint08.tdf" line 296, column 4
-- Equation name is 'CT2', location is LC3_B20, type is buried.
CT2      = DFFE( _EQ090, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ090 =  AY_CCC0 & !CT2
         # !AY_CCC0 &  CT2;

-- Node name is 'CT3' from file "sprint08.tdf" line 296, column 4
-- Equation name is 'CT3', location is LC3_B24, type is buried.
CT3      = DFFE( _EQ091, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ091 =  AY_CCC0 &  CT2 & !CT3
         # !CT2 &  CT3
         # !AY_CCC0 &  CT3;

-- Node name is 'CT4' from file "sprint08.tdf" line 296, column 4
-- Equation name is 'CT4', location is LC1_B24, type is buried.
CT4      = DFFE( _EQ092, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ092 = !CT2 &  CT4
         # !CT3 &  CT4
         #  AY_CCC0 &  CT2 &  CT3 & !CT4
         # !AY_CCC0 &  CT4;

-- Node name is 'CT5' from file "sprint08.tdf" line 296, column 4
-- Equation name is 'CT5', location is LC8_B24, type is buried.
CT5      = DFFE( _EQ093, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ093 =  CT5 & !_LC4_B24
         # !CT4 &  CT5
         #  AY_CCC0 &  CT4 & !CT5 &  _LC4_B24
         # !AY_CCC0 &  CT5;

-- Node name is 'DCOL0' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL0', location is LC6_B19, type is buried.
DCOL0    = DFFE( _EQ094,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ094 =  BORD &  BRD0
         # !BORD &  VD00;

-- Node name is 'DCOL1' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL1', location is LC1_B19, type is buried.
DCOL1    = DFFE( _EQ095,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ095 =  BORD &  BRD1
         # !BORD &  VD01;

-- Node name is 'DCOL2' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL2', location is LC4_B22, type is buried.
DCOL2    = DFFE( _EQ096,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ096 =  BORD &  BRD2
         # !BORD &  VD02;

-- Node name is 'DCOL3' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL3', location is LC2_B19, type is buried.
DCOL3    = DFFE( _EQ097,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ097 = !BORD &  VD03
         #  BORD &  BRD0;

-- Node name is 'DCOL4' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL4', location is LC5_B19, type is buried.
DCOL4    = DFFE( _EQ098,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ098 = !BORD &  VD04
         #  BORD &  BRD1;

-- Node name is 'DCOL5' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL5', location is LC8_B22, type is buried.
DCOL5    = DFFE( _EQ099,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ099 = !BORD &  VD05
         #  BORD &  BRD2;

-- Node name is 'DCOL6' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL6', location is LC8_B19, type is buried.
DCOL6    = DFFE( _EQ100,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ100 = !BORD &  VD06;

-- Node name is 'DCOL7' from file "sprint08.tdf" line 351, column 6
-- Equation name is 'DCOL7', location is LC7_B19, type is buried.
DCOL7    = DFFE( _EQ101,  LWR_COL, !BLANK,  VCC,  VCC);
  _EQ101 = !BORD &  VD07;

-- Node name is 'DCP_CX' from file "sprint08.tdf" line 1302, column 11
-- Equation name is 'DCP_CX', location is LC1_B3, type is buried.
DCP_CX   = LCELL( _EQ102);
  _EQ102 = !DCP4 & !DCP5 &  DD6 &  DD7;

-- Node name is 'DCP3' from file "sprint08.tdf" line 298, column 5
-- Equation name is 'DCP3', location is LC6_B5, type is buried.
DCP3     = DFFE( _EQ103,  LMC_END, !CORRECT_1F,  VCC,  VCC);
  _EQ103 = !/IO &  _LC5_B9 &  SC4
         #  /IO &  MD3
         # !_LC5_B9 &  MD3;

-- Node name is 'DCP4' from file "sprint08.tdf" line 298, column 5
-- Equation name is 'DCP4', location is LC1_B9, type is buried.
DCP4     = DFFE( _EQ104,  LMC_END, !CORRECT_1F,  VCC,  VCC);
  _EQ104 = !/IO &  _LC5_B9
         #  MD4;

-- Node name is 'DCP5' from file "sprint08.tdf" line 298, column 5
-- Equation name is 'DCP5', location is LC7_B9, type is buried.
DCP5     = DFFE( _EQ105,  LMC_END,  VCC,  VCC,  VCC);
  _EQ105 = !/IO &  _LC5_B9
         #  MD5;

-- Node name is 'DD0' from file "sprint08.tdf" line 299, column 4
-- Equation name is 'DD0', location is LC8_B9, type is buried.
DD0      = DFFE( _EQ106,  LMC_END,  VCC,  VCC,  VCC);
  _EQ106 = !/IO &  _LC5_B9 &  PN0
         #  /IO &  MD0
         # !_LC5_B9 &  MD0;

-- Node name is 'DD1' from file "sprint08.tdf" line 299, column 4
-- Equation name is 'DD1', location is LC4_B9, type is buried.
DD1      = DFFE( _EQ107,  LMC_END,  VCC,  VCC,  VCC);
  _EQ107 = !/IO &  _LC5_B9 &  PN1
         #  /IO &  MD1
         # !_LC5_B9 &  MD1;

-- Node name is 'DD2' from file "sprint08.tdf" line 299, column 4
-- Equation name is 'DD2', location is LC2_B9, type is buried.
DD2      = DFFE( _EQ108,  LMC_END,  VCC,  VCC,  VCC);
  _EQ108 = !/IO &  _LC5_B9 &  PN2
         #  /IO &  MD2
         # !_LC5_B9 &  MD2;

-- Node name is 'DD6' from file "sprint08.tdf" line 299, column 4
-- Equation name is 'DD6', location is LC3_B9, type is buried.
DD6      = DFFE( _EQ109,  LMC_END,  VCC,  VCC,  VCC);
  _EQ109 = !/IO &  _LC5_B9
         #  MD6;

-- Node name is 'DD7' from file "sprint08.tdf" line 299, column 4
-- Equation name is 'DD7', location is LC6_B9, type is buried.
DD7      = DFFE( _EQ110,  LMC_END,  VCC,  VCC,  VCC);
  _EQ110 = !/IO &  _LC5_B9
         #  MD7;

-- Node name is 'DOS' from file "sprint08.tdf" line 1378, column 10
-- Equation name is 'DOS', location is LC5_C8, type is buried.
!DOS     = DOS~NOT;
DOS~NOT  = DFFE( _EQ111, !_LC6_B4,  /RESET,  VCC,  VCC);
  _EQ111 = !A14 & !A15 & !DOS
         # !A14 & !A15 &  _LC6_C8;

-- Node name is 'DOS_ON_' from file "sprint08.tdf" line 1379, column 13
-- Equation name is 'DOS_ON_', location is LC4_B11, type is buried.
DOS_ON_  = DFFE( _EQ112,  AY_CCC2,  VCC,  VCC,  VCC);
  _EQ112 = !_LC3_B11
         #  DOS;

-- Node name is 'DPIC' from file "sprint08.tdf" line 350, column 2
-- Equation name is 'DPIC', location is LC1_C2, type is buried.
DPIC     = DFFE( D_PIC07, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'D_PIC00' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC00', location is LC2_B15, type is buried.
D_PIC00  = DFFE( VD00,  LWR_PIC,  VCC,  VCC,  VCC);

-- Node name is 'D_PIC01' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC01', location is LC3_B15, type is buried.
D_PIC01  = DFFE( _EQ113,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ113 =  LD_PIC &  VD01
         #  D_PIC00 & !LD_PIC;

-- Node name is 'D_PIC02' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC02', location is LC4_B15, type is buried.
D_PIC02  = DFFE( _EQ114,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ114 =  LD_PIC &  VD02
         #  D_PIC01 & !LD_PIC;

-- Node name is 'D_PIC03' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC03', location is LC5_B15, type is buried.
D_PIC03  = DFFE( _EQ115,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ115 =  LD_PIC &  VD03
         #  D_PIC02 & !LD_PIC;

-- Node name is 'D_PIC04' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC04', location is LC6_B15, type is buried.
D_PIC04  = DFFE( _EQ116,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ116 =  LD_PIC &  VD04
         #  D_PIC03 & !LD_PIC;

-- Node name is 'D_PIC05' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC05', location is LC7_B15, type is buried.
D_PIC05  = DFFE( _EQ117,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ117 =  LD_PIC &  VD05
         #  D_PIC04 & !LD_PIC;

-- Node name is 'D_PIC06' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC06', location is LC8_B15, type is buried.
D_PIC06  = DFFE( _EQ118,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ118 =  LD_PIC &  VD06
         #  D_PIC05 & !LD_PIC;

-- Node name is 'D_PIC07' from file "sprint08.tdf" line 353, column 8
-- Equation name is 'D_PIC07', location is LC1_B15, type is buried.
D_PIC07  = DFFE( _EQ119,  LWR_PIC,  VCC,  VCC,  VCC);
  _EQ119 =  LD_PIC &  VD07
         #  D_PIC06 & !LD_PIC;

-- Node name is 'D_RD' from file "sprint08.tdf" line 1415, column 38
-- Equation name is 'D_RD', location is LC1_B4, type is buried.
D_RD     = LCELL( _EQ120);
  _EQ120 = !_LC5_B4
         # !/IOM1 &  _LC5_B5 & !/RD;

-- Node name is 'D0' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D0', type is bidir 
D0       = TRI(SD0,  D_RD);

-- Node name is 'D1' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D1', type is bidir 
D1       = TRI(SD1,  D_RD);

-- Node name is 'D2' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D2', type is bidir 
D2       = TRI(SD2,  D_RD);

-- Node name is 'D3' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D3', type is bidir 
D3       = TRI(SD3,  D_RD);

-- Node name is 'D4' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D4', type is bidir 
D4       = TRI(SD4,  D_RD);

-- Node name is 'D5' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D5', type is bidir 
D5       = TRI(SD5,  D_RD);

-- Node name is 'D6' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D6', type is bidir 
D6       = TRI(SD6,  D_RD);

-- Node name is 'D7' from file "sprint08.tdf" line 1418, column 4
-- Equation name is 'D7', type is bidir 
D7       = TRI(SD7,  D_RD);

-- Node name is 'E_CAS_0' from file "sprint08.tdf" line 1600, column 12
-- Equation name is 'E_CAS_0', location is LC3_B18, type is buried.
E_CAS_0  = DFFE( _EQ121, !AY_CCC2,  VCC,  VCC,  VCC);
  _EQ121 =  _LC2_B18
         #  AA10 &  /IO
         #  DOS & !/IO;

-- Node name is 'E_CAS_1' from file "sprint08.tdf" line 1601, column 12
-- Equation name is 'E_CAS_1', location is LC6_B18, type is buried.
E_CAS_1  = DFFE( _EQ122, !AY_CCC2,  VCC,  VCC,  VCC);
  _EQ122 = !AA10 &  /IO
         # !AA10 & !DOS
         # !DOS & !/IO
         #  _LC2_B18;

-- Node name is 'E_CAS_2' from file "sprint08.tdf" line 1602, column 12
-- Equation name is 'E_CAS_2', location is LC1_B18, type is buried.
E_CAS_2  = DFFE( _EQ123, !AY_CCC2,  VCC,  VCC,  VCC);
  _EQ123 = !AA11
         # !/IO
         #  BLK_R
         # !AA10;

-- Node name is 'E_CAS_3' from file "sprint08.tdf" line 1603, column 12
-- Equation name is 'E_CAS_3', location is LC8_B18, type is buried.
E_CAS_3  = DFFE( _EQ124, !AY_CCC2,  VCC,  VCC,  VCC);
  _EQ124 = !AA11
         # !/IO
         #  BLK_R
         #  AA10;

-- Node name is 'IN_OUT_CMD' from file "sprint08.tdf" line 504, column 2
-- Equation name is 'IN_OUT_CMD', location is LC2_A6, type is buried.
IN_OUT_CMD = DFFE( _EQ125,  _LC6_B4, GLOBAL( /IO),  VCC,  VCC);
  _EQ125 = !D5 &  _LC3_A6 &  _LC5_A15 & !PRF_CMD;

-- Node name is 'INTT' from file "sprint08.tdf" line 1495, column 9
-- Equation name is 'INTT', location is LC1_C22, type is buried.
!INTT    = INTT~NOT;
INTT~NOT = DFFE( VCC,  _LC5_C22,  _LC2_C22,  VCC,  VCC);

-- Node name is 'IO_WAIT~1' from file "sprint08.tdf" line 1559, column 48
-- Equation name is 'IO_WAIT~1', location is LC2_B7, type is buried.
-- synthesized logic cell 
_LC2_B7  = LCELL( _EQ126);
  _EQ126 =  _LC6_B7 &  LMC_END
         # !/M1
         #  /IO;

-- Node name is 'KA8' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA8', location is LC3_C9, type is buried.
KA8      = LCELL( _EQ127);
  _EQ127 =  KB_D1 &  _LC5_C9
         #  KDD6 & !_LC5_C9
         # !_LC4_C6;

-- Node name is 'KA9' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA9', location is LC7_C9, type is buried.
KA9      = LCELL( _EQ128);
  _EQ128 =  KB_D2 &  _LC5_C9
         #  KDD7 & !_LC5_C9
         # !_LC4_C6;

-- Node name is 'KA10' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA10', location is LC4_C4, type is buried.
KA10     = LCELL( _EQ129);
  _EQ129 =  KDCA0 & !_LC4_C6
         #  KB_D3 &  _LC4_C6 &  _LC5_C9;

-- Node name is 'KA11' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA11', location is LC2_C12, type is buried.
KA11     = LCELL( _EQ130);
  _EQ130 =  KDCA1 & !_LC4_C6
         #  KB_D4 &  _LC4_C6 &  _LC5_C9;

-- Node name is 'KA12' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA12', location is LC1_C7, type is buried.
KA12     = LCELL( _EQ131);
  _EQ131 =  KDCA2 & !_LC4_C6
         #  KB_D5 &  _LC4_C6 &  _LC5_C9;

-- Node name is 'KA13' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA13', location is LC1_C9, type is buried.
KA13     = LCELL( _EQ132);
  _EQ132 =  KB_D6 &  _LC5_C9
         # !_LC4_C6;

-- Node name is 'KA14' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA14', location is LC2_C9, type is buried.
KA14     = LCELL( _EQ133);
  _EQ133 =  _LC4_C6 & !_LC5_C9
         #  KB_D7 &  _LC4_C6;

-- Node name is 'KA15' from file "sprint08.tdf" line 2516, column 27
-- Equation name is 'KA15', location is LC8_C9, type is buried.
KA15     = LCELL( _EQ134);
  _EQ134 =  KB_D8
         # !_LC5_C9
         # !_LC4_C6;

-- Node name is 'KB_ALT' from file "sprint08.tdf" line 409, column 2
-- Equation name is 'KB_ALT', location is LC2_C5, type is buried.
KB_ALT   = DFFE( _EQ135, !KB_CT2,  VCC,  VCC,  VCC);
  _EQ135 =  KB_ALT & !KB_ALT_X
         #  KB_ALT & !KB_XXX
         #  KB_ALT_X & !KB_OFF &  KB_XXX;

-- Node name is 'KB_ALT_X' from file "sprint08.tdf" line 2460, column 13
-- Equation name is 'KB_ALT_X', location is LC5_C1, type is buried.
KB_ALT_X = LCELL( _EQ136);
  _EQ136 =  KB_D1 & !KB_D2 & !KB_D3 &  KB_D5;

-- Node name is 'KB_CTRL' from file "sprint08.tdf" line 408, column 2
-- Equation name is 'KB_CTRL', location is LC3_C5, type is buried.
KB_CTRL  = DFFE( _EQ137, !KB_CT2,  VCC,  VCC,  VCC);
  _EQ137 =  KB_CTRL & !KB_CTRL_X
         #  KB_CTRL & !KB_XXX
         #  KB_CTRL_X & !KB_OFF &  KB_XXX;

-- Node name is 'KB_CTRL_X' from file "sprint08.tdf" line 2459, column 14
-- Equation name is 'KB_CTRL_X', location is LC6_C1, type is buried.
KB_CTRL_X = LCELL( _EQ138);
  _EQ138 = !KB_D1 & !KB_D2 &  KB_D3 &  KB_D5;

-- Node name is 'KB_CT0' from file "sprint08.tdf" line 407, column 7
-- Equation name is 'KB_CT0', location is LC8_C3, type is buried.
!KB_CT0  = KB_CT0~NOT;
KB_CT0~NOT = DFFE( _EQ139,  CTH5,  KBD_CC,  VCC,  VCC);
  _EQ139 =  KB_CT0
         # !KB_CT1 & !KB_CT2;

-- Node name is 'KB_CT1' from file "sprint08.tdf" line 407, column 7
-- Equation name is 'KB_CT1', location is LC6_C3, type is buried.
!KB_CT1  = KB_CT1~NOT;
KB_CT1~NOT = DFFE( _EQ140,  CTH5,  KBD_CC,  VCC,  VCC);
  _EQ140 = !KB_CT1 & !KB_CT2
         #  KB_CT0 & !KB_CT1
         # !KB_CT0 &  KB_CT1;

-- Node name is 'KB_CT2' from file "sprint08.tdf" line 407, column 7
-- Equation name is 'KB_CT2', location is LC3_C3, type is buried.
!KB_CT2  = KB_CT2~NOT;
KB_CT2~NOT = DFFE( _EQ141,  CTH5,  KBD_CC,  VCC,  VCC);
  _EQ141 = !KB_CT2
         # !KB_CT0 & !KB_CT1;

-- Node name is 'KBD_CC' from file "sprint08.tdf" line 1474, column 11
-- Equation name is 'KBD_CC', location is LC2_C16, type is buried.
KBD_CC   = DFFE( KBD_CLK,  CTH2,  VCC,  VCC,  VCC);

-- Node name is 'KBD_CLK' from file "sprint08.tdf" line 1477, column 2
-- Equation name is 'KBD_CLK', type is bidir 
KBD_CLK  = TRI(VCC,  GND);

-- Node name is 'KBD_DAT' from file "sprint08.tdf" line 1478, column 2
-- Equation name is 'KBD_DAT', type is bidir 
KBD_DAT  = TRI(VCC,  GND);

-- Node name is 'KBD_DD' from file "sprint08.tdf" line 1475, column 11
-- Equation name is 'KBD_DD', location is LC7_C16, type is buried.
KBD_DD   = DFFE( KBD_DAT,  CTH2,  VCC,  VCC,  VCC);

-- Node name is 'KBD0' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD0', location is LC4_C23, type is buried.
!KBD0    = KBD0~NOT;
KBD0~NOT = DFFE( _EQ142, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ142 = !KBD0
         # !_EC3_C & !KB_MXA;

-- Node name is 'KBD1' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD1', location is LC3_C20, type is buried.
!KBD1    = KBD1~NOT;
KBD1~NOT = DFFE( _EQ143, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ143 = !KBD1
         # !_EC7_C & !KB_MXA;

-- Node name is 'KB_D1' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D1', location is LC1_C1, type is buried.
KB_D1    = DFFE( KB_D2,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KBD2' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD2', location is LC6_C24, type is buried.
!KBD2    = KBD2~NOT;
KBD2~NOT = DFFE( _EQ144, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ144 = !KBD2
         # !_EC6_C & !KB_MXA;

-- Node name is 'KB_D2' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D2', location is LC2_C1, type is buried.
KB_D2    = DFFE( KB_D3,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KBD3' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD3', location is LC7_C4, type is buried.
!KBD3    = KBD3~NOT;
KBD3~NOT = DFFE( _EQ145, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ145 = !KBD3
         # !_EC1_C & !KB_MXA;

-- Node name is 'KB_D3' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D3', location is LC7_C14, type is buried.
KB_D3    = DFFE( KB_D4,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KBD4' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD4', location is LC7_C12, type is buried.
!KBD4    = KBD4~NOT;
KBD4~NOT = DFFE( _EQ146, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ146 = !KBD4
         # !_EC5_C & !KB_MXA;

-- Node name is 'KB_D4' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D4', location is LC5_C14, type is buried.
KB_D4    = DFFE( KB_D5,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KBD5' from file "sprint08.tdf" line 421, column 5
-- Equation name is 'KBD5', location is LC5_C7, type is buried.
!KBD5    = KBD5~NOT;
KBD5~NOT = DFFE( _EQ147, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ147 = !KBD5
         # !_EC4_C & !KB_MXA;

-- Node name is 'KB_D5' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D5', location is LC1_C14, type is buried.
KB_D5    = DFFE( KB_D6,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_D6' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D6', location is LC6_C14, type is buried.
KB_D6    = DFFE( KB_D7,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_D7' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D7', location is LC2_C14, type is buried.
KB_D7    = DFFE( KB_D8,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_D8' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D8', location is LC4_C14, type is buried.
KB_D8    = DFFE( KB_D9,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_D9' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D9', location is LC8_C14, type is buried.
KB_D9    = DFFE( KB_D10,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_D10' from file "sprint08.tdf" line 405, column 6
-- Equation name is 'KB_D10', location is LC3_C14, type is buried.
KB_D10   = DFFE( KBD_DD,  KBD_CC,  VCC,  VCC,  VCC);

-- Node name is 'KB_EXT' from file "sprint08.tdf" line 411, column 2
-- Equation name is 'KB_EXT', location is LC4_C1, type is buried.
KB_EXT   = DFFE( _EQ148, !_LC2_C3,  VCC,  VCC,  VCC);
  _EQ148 = !KB_D5 &  _LC3_C1;

-- Node name is 'KB_F12' from file "sprint08.tdf" line 2479, column 12
-- Equation name is 'KB_F12', location is LC4_C5, type is buried.
!KB_F12  = KB_F12~NOT;
KB_F12~NOT = DFFE( _EQ149, !KB_CT2,  _LC2_C3,  VCC,  VCC);
  _EQ149 = !KB_OFF &  KB_XXX &  _LC8_C1;

-- Node name is 'KB_MA0' from file "sprint08.tdf" line 583, column 7
-- Equation name is 'KB_MA0', location is LC4_C8, type is buried.
KB_MA0   = DFFE(!KB_MA0, GLOBAL( TG42), GLOBAL(!/IO),  VCC,  VCC);

-- Node name is 'KB_MA1' from file "sprint08.tdf" line 583, column 7
-- Equation name is 'KB_MA1', location is LC1_C12, type is buried.
KB_MA1   = DFFE( _EQ150, GLOBAL( TG42), GLOBAL(!/IO),  VCC,  VCC);
  _EQ150 = !KB_MA0 &  KB_MA1
         #  KB_MA0 & !KB_MA1;

-- Node name is 'KB_MA2' from file "sprint08.tdf" line 583, column 7
-- Equation name is 'KB_MA2', location is LC8_C12, type is buried.
KB_MA2   = DFFE( _EQ151, GLOBAL( TG42), GLOBAL(!/IO),  VCC,  VCC);
  _EQ151 = !KB_MA1 &  KB_MA2
         # !KB_MA0 &  KB_MA2
         #  KB_MA0 &  KB_MA1 & !KB_MA2;

-- Node name is 'KB_MXA' from file "sprint08.tdf" line 2523, column 11
-- Equation name is 'KB_MXA', location is LC6_C12, type is buried.
KB_MXA   = DFFE( _EQ152, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ152 =  KB_MA1 &  _LC7_C8
         #  KB_MA1 &  _LC5_C12
         # !KB_MA1 &  _LC8_C8;

-- Node name is 'KB_OFF' from file "sprint08.tdf" line 406, column 2
-- Equation name is 'KB_OFF', location is LC5_C3, type is buried.
KB_OFF   = DFFE( _EQ153, !_LC4_C3,  VCC,  VCC,  VCC);
  _EQ153 =  KB_D5 & !KB_EXT &  _LC3_C1
         #  KB_EXT &  KB_OFF;

-- Node name is 'KB_RESET' from file "sprint08.tdf" line 412, column 2
-- Equation name is 'KB_RESET', location is LC6_C5, type is buried.
!KB_RESET = KB_RESET~NOT;
KB_RESET~NOT = DFFE( _EQ154, !KB_CT2,  _LC2_C3,  VCC,  VCC);
  _EQ154 =  KB_ALT_X &  KB_D6 &  KB_D7 &  _LC8_C5;

-- Node name is 'KB_XXX' from file "sprint08.tdf" line 2465, column 12
-- Equation name is 'KB_XXX', location is LC1_C5, type is buried.
KB_XXX   = LCELL( _EQ155);
  _EQ155 = !KB_D4 & !KB_D6 & !KB_D7 & !KB_D8;

-- Node name is 'K_CLK' from file "sprint08.tdf" line 2490, column 11
-- Equation name is 'K_CLK', location is LC3_B10, type is buried.
K_CLK    = DFFE( /RF, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'KDCA0' from file "sprint08.tdf" line 2537, column 10
-- Equation name is 'KDCA0', location is LC6_C4, type is buried.
KDCA0    = LCELL( _EQ156);
  _EQ156 =  /IO &  KDD3
         # !/IO &  KB_MA0;

-- Node name is 'KDCA1' from file "sprint08.tdf" line 2537, column 10
-- Equation name is 'KDCA1', location is LC4_C12, type is buried.
KDCA1    = LCELL( _EQ157);
  _EQ157 =  /IO &  KDD4
         # !/IO &  KB_MA1;

-- Node name is 'KDCA2' from file "sprint08.tdf" line 2537, column 10
-- Equation name is 'KDCA2', location is LC4_C7, type is buried.
KDCA2    = LCELL( _EQ158);
  _EQ158 =  /IO &  KDD5
         # !/IO &  KB_MA2;

-- Node name is 'KDD3' from file "sprint08.tdf" line 423, column 5
-- Equation name is 'KDD3', location is LC5_C4, type is buried.
KDD3     = DFFE( _EC1_C,  RXA0,  VCC,  VCC,  VCC);

-- Node name is 'KDD4' from file "sprint08.tdf" line 423, column 5
-- Equation name is 'KDD4', location is LC3_C12, type is buried.
KDD4     = DFFE( _EC5_C,  RXA0,  VCC,  VCC,  VCC);

-- Node name is 'KDD5' from file "sprint08.tdf" line 423, column 5
-- Equation name is 'KDD5', location is LC2_C7, type is buried.
KDD5     = DFFE( _EC4_C,  RXA0,  VCC,  VCC,  VCC);

-- Node name is 'KDD6' from file "sprint08.tdf" line 423, column 5
-- Equation name is 'KDD6', location is LC6_C9, type is buried.
!KDD6    = KDD6~NOT;
KDD6~NOT = DFFE(!_EC8_C,  RXA0, !KB_CT2,  VCC,  VCC);

-- Node name is 'KDD7' from file "sprint08.tdf" line 423, column 5
-- Equation name is 'KDD7', location is LC4_C9, type is buried.
!KDD7    = KDD7~NOT;
KDD7~NOT = DFFE(!_EC2_C,  RXA0, !KB_CT2,  VCC,  VCC);

-- Node name is 'KDXX0' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX0', location is LC2_C11, type is buried.
KDXX0    = DFFE( _EQ159,  RXA0,  VCC,  VCC,  VCC);
  _EQ159 =  _EC6_C
         #  _EC7_C
         #  _EC3_C;

-- Node name is 'KDXX1' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX1', location is LC3_C11, type is buried.
KDXX1    = DFFE( _EQ160,  RXA0,  VCC,  VCC,  VCC);
  _EQ160 =  _EC6_C
         #  _EC7_C
         # !_EC3_C;

-- Node name is 'KDXX2' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX2', location is LC5_C11, type is buried.
KDXX2    = DFFE( _EQ161,  RXA0,  VCC,  VCC,  VCC);
  _EQ161 =  _EC6_C
         # !_EC7_C
         #  _EC3_C;

-- Node name is 'KDXX3' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX3', location is LC7_C11, type is buried.
KDXX3    = DFFE( _EQ162,  RXA0,  VCC,  VCC,  VCC);
  _EQ162 =  _EC6_C
         # !_EC7_C
         # !_EC3_C;

-- Node name is 'KDXX4' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX4', location is LC1_C11, type is buried.
KDXX4    = DFFE( _EQ163,  RXA0,  VCC,  VCC,  VCC);
  _EQ163 = !_EC6_C
         #  _EC7_C
         #  _EC3_C;

-- Node name is 'KDXX5' from file "sprint08.tdf" line 627, column 6
-- Equation name is 'KDXX5', location is LC8_C11, type is buried.
KDXX5    = DFFE( _EQ164,  RXA0,  VCC,  VCC,  VCC);
  _EQ164 =  _EC7_C
         # !_EC3_C
         # !_EC6_C;

-- Node name is 'KDX0' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX0', location is LC6_C11, type is buried.
KDX0     = DFFE( _EQ165,  RXA1,  VCC,  VCC,  VCC);
  _EQ165 =  _EC3_C &  KDXX0
         #  KB_OFF & !KDXX0;

-- Node name is 'KDX1' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX1', location is LC4_C11, type is buried.
KDX1     = DFFE( _EQ166,  RXA1,  VCC,  VCC,  VCC);
  _EQ166 =  _EC7_C &  KDXX1
         #  KB_OFF & !KDXX1;

-- Node name is 'KDX2' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX2', location is LC8_C6, type is buried.
KDX2     = DFFE( _EQ167,  RXA1,  VCC,  VCC,  VCC);
  _EQ167 =  _EC6_C &  KDXX2
         #  KB_OFF & !KDXX2;

-- Node name is 'KDX3' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX3', location is LC7_C6, type is buried.
KDX3     = DFFE( _EQ168,  RXA1,  VCC,  VCC,  VCC);
  _EQ168 =  _EC1_C &  KDXX3
         #  KB_OFF & !KDXX3;

-- Node name is 'KDX4' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX4', location is LC5_C6, type is buried.
KDX4     = DFFE( _EQ169,  RXA1,  VCC,  VCC,  VCC);
  _EQ169 =  _EC5_C &  KDXX4
         #  KB_OFF & !KDXX4;

-- Node name is 'KDX5' from file "sprint08.tdf" line 424, column 5
-- Equation name is 'KDX5', location is LC3_C6, type is buried.
KDX5     = DFFE( _EQ170,  RXA1,  VCC,  VCC,  VCC);
  _EQ170 =  _EC4_C &  KDXX5
         #  KB_OFF & !KDXX5;

-- Node name is 'LD_PIC' from file "sprint08.tdf" line 1842, column 12
-- Equation name is 'LD_PIC', location is LC6_B24, type is buried.
LD_PIC   = LCELL( _EQ171);
  _EQ171 = !CT3 & !CT4 & !CT5;

-- Node name is 'LMC_END' from file "sprint08.tdf" line 1619, column 13
-- Equation name is 'LMC_END', location is LC7_B17, type is buried.
LMC_END  = DFFE( MC_END, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is 'LWR_COL' from file "sprint08.tdf" line 1830, column 13
-- Equation name is 'LWR_COL', location is LC1_B21, type is buried.
LWR_COL  = LCELL( WR_COL);

-- Node name is 'LWR_PIC' from file "sprint08.tdf" line 1829, column 13
-- Equation name is 'LWR_PIC', location is LC8_C18, type is buried.
LWR_PIC  = LCELL( WR_PIC);

-- Node name is 'MA0' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA0', location is LC2_A21, type is buried.
MA0      = LCELL( _EQ172);
  _EQ172 =  _EC7_B & !_LC7_B21
         #  AA0 &  _LC7_B21;

-- Node name is 'MA1' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA1', location is LC3_B17, type is buried.
MA1      = LCELL( _EQ173);
  _EQ173 = !_LC7_B21 &  RA12
         #  AA1 &  _LC7_B21;

-- Node name is 'MA2' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA2', location is LC6_B14, type is buried.
MA2      = LCELL( _EQ174);
  _EQ174 = !_LC7_B21 &  RA13
         #  AA2 &  _LC7_B21;

-- Node name is 'MA3' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA3', location is LC4_C17, type is buried.
MA3      = LCELL( _EQ175);
  _EQ175 =  _EC1_B & !_LC7_B21
         #  _LC7_B21 &  RA3;

-- Node name is 'MA4' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA4', location is LC5_C16, type is buried.
MA4      = LCELL( _EQ176);
  _EQ176 =  _EC3_B & !_LC7_B21
         #  _LC7_B21 &  RA4;

-- Node name is 'MA5' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA5', location is LC8_B14, type is buried.
MA5      = LCELL( _EQ177);
  _EQ177 =  _EC8_B & !_LC7_B21
         #  AA5 &  _LC7_B21;

-- Node name is 'MA6' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA6', location is LC1_B13, type is buried.
MA6      = LCELL( _EQ178);
  _EQ178 =  _EC5_B & !_LC7_B21
         #  AA6 &  _LC7_B21;

-- Node name is 'MA7' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA7', location is LC3_C23, type is buried.
MA7      = LCELL( _EQ179);
  _EQ179 =  _EC4_B & !_LC7_B21
         #  _LC7_B21 &  RA7;

-- Node name is 'MA8' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA8', location is LC6_C20, type is buried.
MA8      = LCELL( _EQ180);
  _EQ180 =  _EC2_B & !_LC7_B21
         #  _LC7_B21 &  RA8;

-- Node name is 'MA9' from file "sprint08.tdf" line 1277, column 8
-- Equation name is 'MA9', location is LC2_C24, type is buried.
MA9      = LCELL( _EQ181);
  _EQ181 =  _EC6_B & !_LC7_B21
         #  _LC7_B21 &  RA9;

-- Node name is 'MC_END' from file "sprint08.tdf" line 1554, column 11
-- Equation name is 'MC_END', location is LC8_B8, type is buried.
MC_END   = DFFE( _EQ182,  CAS, !_LC2_C13,  VCC,  VCC);
  _EQ182 =  MC_END
         #  DOS_ON_ & !MC_START;

-- Node name is 'MC_START' from file "sprint08.tdf" line 430, column 2
-- Equation name is 'MC_START', location is LC3_B8, type is buried.
!MC_START = MC_START~NOT;
MC_START~NOT = DFFE(!MC1, !CT2, !_LC2_C13,  VCC,  VCC);

-- Node name is 'MC_SYCLE' from file "sprint08.tdf" line 1569, column 13
-- Equation name is 'MC_SYCLE', location is LC7_B8, type is buried.
MC_SYCLE = DFFE( _EQ183, !CT2,  VCC,  VCC,  VCC);
  _EQ183 =  BLK_R
         #  MC1;

-- Node name is 'MC1' from file "sprint08.tdf" line 1552, column 9
-- Equation name is 'MC1', location is LC3_B4, type is buried.
!MC1     = MC1~NOT;
MC1~NOT  = DFFE( _EQ184, GLOBAL(!TG42), !MC_END,  VCC,  VCC);
  _EQ184 = !/MR & !/WR
         # !/IOM & !/WR
         # !/MR & !/RD
         # !/IOM & !/RD;

-- Node name is 'MD0' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD0', type is bidir 
MD0      = TRI(_LC1_C16, !/WE1);

-- Node name is 'MD1' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD1', type is bidir 
MD1      = TRI(_LC7_A13, !/WE1);

-- Node name is 'MD2' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD2', type is bidir 
MD2      = TRI(_LC7_B22, !/WE1);

-- Node name is 'MD3' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD3', type is bidir 
MD3      = TRI(_LC2_C10, !/WE1);

-- Node name is 'MD4' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD4', type is bidir 
MD4      = TRI(_LC2_A3, !/WE1);

-- Node name is 'MD5' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD5', type is bidir 
MD5      = TRI(_LC3_C13, !/WE1);

-- Node name is 'MD6' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD6', type is bidir 
MD6      = TRI(_LC1_B11, !/WE1);

-- Node name is 'MD7' from file "sprint08.tdf" line 1419, column 5
-- Equation name is 'MD7', type is bidir 
MD7      = TRI(_LC2_C4, !/WE1);

-- Node name is 'MPGS0' from file "sprint08.tdf" line 734, column 24
-- Equation name is 'MPGS0', location is LC8_B12, type is buried.
MPGS0    = LCELL( _EQ185);
  _EQ185 =  AR0 & !A15
         #  A14 &  PN0
         #  A14 & !A15;

-- Node name is 'MPGS1' from file "sprint08.tdf" line 734, column 24
-- Equation name is 'MPGS1', location is LC4_B12, type is buried.
MPGS1    = LCELL( _EQ186);
  _EQ186 =  AR1 & !A14
         #  A15 &  PN1
         # !A14 &  A15;

-- Node name is 'MPGS2' from file "sprint08.tdf" line 734, column 24
-- Equation name is 'MPGS2', location is LC6_B1, type is buried.
MPGS2    = LCELL( _EQ187);
  _EQ187 =  AR2 & !A14 & !A15
         #  A14 &  A15 &  PN2;

-- Node name is 'MPGS3' from file "sprint08.tdf" line 734, column 24
-- Equation name is 'MPGS3', location is LC3_B1, type is buried.
MPGS3    = LCELL( _EQ188);
  _EQ188 = !A14 &  A15
         #  A14 & !A15
         #  AR3 & !A14
         #  A15 &  SC4;

-- Node name is 'MXA0' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA0', type is output 
MXA0     =  MA0;

-- Node name is 'MXA1' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA1', type is output 
MXA1     =  MA1;

-- Node name is 'MXA2' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA2', type is output 
MXA2     =  MA2;

-- Node name is 'MXA3' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA3', type is output 
MXA3     =  MA3;

-- Node name is 'MXA4' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA4', type is output 
MXA4     =  MA4;

-- Node name is 'MXA5' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA5', type is output 
MXA5     =  MA5;

-- Node name is 'MXA6' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA6', type is output 
MXA6     =  MA6;

-- Node name is 'MXA7' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA7', type is output 
MXA7     =  MA7;

-- Node name is 'MXA8' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA8', type is output 
MXA8     =  MA8;

-- Node name is 'MXA9' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA9', type is output 
MXA9     =  MA9;

-- Node name is 'MXA10' from file "sprint08.tdf" line 1444, column 5
-- Equation name is 'MXA10', type is output 
MXA10    =  _EC7_B;

-- Node name is 'MXVD0~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD0~1', location is LC8_C10, type is buried.
-- synthesized logic cell 
_LC8_C10 = DFFE( D0,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD0~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD0~2', location is LC4_C10, type is buried.
-- synthesized logic cell 
_LC4_C10 = DFFE( D0,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD0~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD0~3', location is LC3_B5, type is buried.
-- synthesized logic cell 
_LC3_B5  = DFFE( D0,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD0' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD0', location is LC1_C10, type is buried.
MXVD0    = DFFE( D0,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD1~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD1~1', location is LC2_A13, type is buried.
-- synthesized logic cell 
_LC2_A13 = DFFE( D1,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD1~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD1~2', location is LC4_A13, type is buried.
-- synthesized logic cell 
_LC4_A13 = DFFE( D1,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD1~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD1~3', location is LC5_A13, type is buried.
-- synthesized logic cell 
_LC5_A13 = DFFE( D1,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD1', location is LC1_A13, type is buried.
MXVD1    = DFFE( D1,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD2~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD2~1', location is LC1_A16, type is buried.
-- synthesized logic cell 
_LC1_A16 = DFFE( D2,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD2~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD2~2', location is LC8_A16, type is buried.
-- synthesized logic cell 
_LC8_A16 = DFFE( D2,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD2~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD2~3', location is LC7_A16, type is buried.
-- synthesized logic cell 
_LC7_A16 = DFFE( D2,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD2', location is LC4_A12, type is buried.
MXVD2    = DFFE( D2,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD3~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD3~1', location is LC6_C10, type is buried.
-- synthesized logic cell 
_LC6_C10 = DFFE( D3,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD3~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD3~2', location is LC5_C10, type is buried.
-- synthesized logic cell 
_LC5_C10 = DFFE( D3,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD3~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD3~3', location is LC7_C10, type is buried.
-- synthesized logic cell 
_LC7_C10 = DFFE( D3,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD3', location is LC3_C10, type is buried.
MXVD3    = DFFE( D3,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD4~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD4~1', location is LC3_A13, type is buried.
-- synthesized logic cell 
_LC3_A13 = DFFE( D4,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD4~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD4~2', location is LC6_A13, type is buried.
-- synthesized logic cell 
_LC6_A13 = DFFE( D4,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD4~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD4~3', location is LC8_A13, type is buried.
-- synthesized logic cell 
_LC8_A13 = DFFE( D4,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD4' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD4', location is LC7_A1, type is buried.
MXVD4    = DFFE( D4,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD5~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD5~1', location is LC6_A16, type is buried.
-- synthesized logic cell 
_LC6_A16 = DFFE( D5,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD5~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD5~2', location is LC2_A16, type is buried.
-- synthesized logic cell 
_LC2_A16 = DFFE( D5,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD5~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD5~3', location is LC3_A16, type is buried.
-- synthesized logic cell 
_LC3_A16 = DFFE( D5,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD5' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD5', location is LC5_A16, type is buried.
MXVD5    = DFFE( D5,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD6~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD6~1', location is LC8_B11, type is buried.
-- synthesized logic cell 
_LC8_B11 = DFFE( D6,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD6~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD6~2', location is LC2_B11, type is buried.
-- synthesized logic cell 
_LC2_B11 = DFFE( D6,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD6~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD6~3', location is LC5_B11, type is buried.
-- synthesized logic cell 
_LC5_B11 = DFFE( D6,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD6' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD6', location is LC6_B11, type is buried.
MXVD6    = DFFE( D6,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD7~1' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD7~1', location is LC5_A6, type is buried.
-- synthesized logic cell 
_LC5_A6  = DFFE( D7,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD7~2' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD7~2', location is LC1_A6, type is buried.
-- synthesized logic cell 
_LC1_A6  = DFFE( D7,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD7~3' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD7~3', location is LC4_A6, type is buried.
-- synthesized logic cell 
_LC4_A6  = DFFE( D7,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXVD7' from file "sprint08.tdf" line 397, column 6
-- Equation name is 'MXVD7', location is LC7_A6, type is buried.
MXVD7    = DFFE( D7,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is 'MXWE' from file "sprint08.tdf" line 1756, column 9
-- Equation name is 'MXWE', location is LC3_B23, type is buried.
!MXWE    = MXWE~NOT;
MXWE~NOT = DFFE( _EQ189,  AY_CCC2,  V_WE,  VCC,  VCC);
  _EQ189 = !A13 &  A14 & !_LC7_B1 & !/WE1;

-- Node name is 'PGS0' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS0', location is LC6_B12, type is buried.
PGS0     = LCELL( _EQ190);
  _EQ190 =  _LC4_B10 &  MPGS0
         #  DD0 & !_LC4_B10 &  MC_END;

-- Node name is 'PGS1' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS1', location is LC7_B12, type is buried.
PGS1     = LCELL( _EQ191);
  _EQ191 =  _LC4_B10 &  MPGS1
         #  DD1 & !_LC4_B10 &  MC_END;

-- Node name is 'PGS2' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS2', location is LC8_B1, type is buried.
PGS2     = LCELL( _EQ192);
  _EQ192 =  _LC4_B10 &  MPGS2
         #  DD2 & !_LC4_B10 &  MC_END;

-- Node name is 'PGS3' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS3', location is LC1_B1, type is buried.
PGS3     = LCELL( _EQ193);
  _EQ193 =  _LC4_B10 &  MPGS3
         #  DCP3 & !_LC4_B10 &  MC_END;

-- Node name is 'PGS4' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS4', location is LC6_B10, type is buried.
PGS4     = LCELL( _EQ194);
  _EQ194 =  DCP4 & !_LC4_B10 &  MC_END
         # !_LC1_B10 &  _LC4_B10;

-- Node name is 'PGS5' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS5', location is LC2_B2, type is buried.
PGS5     = LCELL( _EQ195);
  _EQ195 =  DCP5 & !_LC4_B10 &  MC_END
         #  _LC8_B2;

-- Node name is 'PGS6' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS6', location is LC1_B2, type is buried.
PGS6     = LCELL( _EQ196);
  _EQ196 =  _LC8_B2
         #  DD6 & !_LC4_B10 &  MC_END;

-- Node name is 'PGS7' from file "sprint08.tdf" line 750, column 23
-- Equation name is 'PGS7', location is LC3_B2, type is buried.
PGS7     = LCELL( _EQ197);
  _EQ197 =  DD7 &  MC_END
         #  _LC4_B10;

-- Node name is 'PN0' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN0', location is LC8_B6, type is buried.
PN0      = DFFE( D0,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PN1' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN1', location is LC2_B6, type is buried.
PN1      = DFFE( D1,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PN2' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN2', location is LC7_B6, type is buried.
PN2      = DFFE( D2,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PN3' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN3', location is LC5_B6, type is buried.
PN3      = DFFE( D3,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PN4' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN4', location is LC1_B6, type is buried.
PN4      = DFFE( D4,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PN5' from file "sprint08.tdf" line 312, column 4
-- Equation name is 'PN5', location is LC4_B6, type is buried.
PN5      = DFFE( D5,  _LC5_B3,  /RESET,  VCC,  _LC3_B6);

-- Node name is 'PRF_CMD' from file "sprint08.tdf" line 502, column 2
-- Equation name is 'PRF_CMD', location is LC8_A6, type is buried.
PRF_CMD  = DFFE( _EQ198,  _LC6_B4,  VCC,  VCC,  VCC);
  _EQ198 =  D6 &  D7 &  _LC4_A16 &  _LC6_A6;

-- Node name is 'RAS_0' from file "sprint08.tdf" line 1617, column 6
-- Equation name is 'RAS_0', type is output 
RAS_0    =  _LC5_B8;

-- Node name is 'RAS_1' from file "sprint08.tdf" line 1617, column 6
-- Equation name is 'RAS_1', type is output 
RAS_1    =  _LC4_B8;

-- Node name is 'RA3' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA3', location is LC2_C17, type is buried.
RA3      = LCELL( _EQ199);
  _EQ199 =  AA7 & !/IO
         #  AA3 &  /IO;

-- Node name is 'RA4' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA4', location is LC4_C16, type is buried.
RA4      = LCELL( _EQ200);
  _EQ200 =  AA13 & !/IO
         #  AA4 &  /IO;

-- Node name is 'RA7' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA7', location is LC8_C23, type is buried.
RA7      = LCELL( _EQ201);
  _EQ201 =  AA7 &  /IO
         #  A14 & !/IO;

-- Node name is 'RA8' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA8', location is LC7_C20, type is buried.
RA8      = LCELL( _EQ202);
  _EQ202 =  AA8 &  /IO
         #  A15 & !/IO;

-- Node name is 'RA9' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA9', location is LC8_C24, type is buried.
RA9      = LCELL( _EQ203);
  _EQ203 =  AA9 &  /IO
         # !/IO &  /WR;

-- Node name is 'RA12' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA12', location is LC8_B17, type is buried.
RA12     = LCELL( _EQ204);
  _EQ204 =  CNF3 & !/IO
         #  AA12 &  /IO;

-- Node name is 'RA13' from file "sprint08.tdf" line 1269, column 33
-- Equation name is 'RA13', location is LC7_B14, type is buried.
RA13     = LCELL( _EQ205);
  _EQ205 =  CNF4 & !/IO
         #  AA13 &  /IO;

-- Node name is 'RXA0' from file "sprint08.tdf" line 427, column 5
-- Equation name is 'RXA0', location is LC2_C6, type is buried.
RXA0     = DFFE( _EQ206,  K_CLK,  VCC,  VCC,  VCC);
  _EQ206 = !_LC7_C3 & !RXA1;

-- Node name is 'RXA1' from file "sprint08.tdf" line 427, column 5
-- Equation name is 'RXA1', location is LC6_C6, type is buried.
RXA1     = DFFE( _EQ207,  K_CLK,  VCC,  VCC,  VCC);
  _EQ207 = !_LC7_C3 &  RXA0;

-- Node name is 'SC_LCELL' from file "sprint08.tdf" line 739, column 13
-- Equation name is 'SC_LCELL', location is LC2_B12, type is buried.
SC_LCELL = LCELL( _EQ208);
  _EQ208 = !SC1 & !SYS
         # !SC0 & !SC1;

-- Node name is 'SC_PGS' from file "sprint08.tdf" line 769, column 11
-- Equation name is 'SC_PGS', location is LC5_B10, type is buried.
SC_PGS   = LCELL( _EQ209);
  _EQ209 = !_LC1_B10 &  SC4;

-- Node name is 'SC0' from file "sprint08.tdf" line 311, column 4
-- Equation name is 'SC0', location is LC3_B16, type is buried.
SC0      = DFFE( D0,  _LC5_B3,  /RESET,  VCC, !_LC1_B16);

-- Node name is 'SC1' from file "sprint08.tdf" line 311, column 4
-- Equation name is 'SC1', location is LC4_B16, type is buried.
SC1      = DFFE( D1,  _LC5_B3,  /RESET,  VCC, !_LC1_B16);

-- Node name is 'SC4' from file "sprint08.tdf" line 311, column 4
-- Equation name is 'SC4', location is LC6_B16, type is buried.
SC4      = DFFE( D4,  _LC5_B3,  /RESET,  VCC, !_LC1_B16);

-- Node name is 'SD0~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD0~1', location is LC1_C23, type is buried.
-- synthesized logic cell 
_LC1_C23 = LCELL( _EQ210);
  _EQ210 =  DD7 &  _EC4_B & !/IO
         #  DD0 &  /IO;

-- Node name is 'SD0' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD0', location is LC6_C23, type is buried.
SD0      = LCELL( _EQ211);
  _EQ211 =  _LC1_C23
         #  AY_DD0 &  _LC6_B3
         #  _LC2_C23;

-- Node name is 'SD1~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD1~1', location is LC1_C20, type is buried.
-- synthesized logic cell 
_LC1_C20 = LCELL( _EQ212);
  _EQ212 =  DD7 &  _EC2_B & !/IO
         #  DD1 &  /IO;

-- Node name is 'SD1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD1', location is LC4_C20, type is buried.
SD1      = LCELL( _EQ213);
  _EQ213 =  _LC1_C20
         #  AY_DD1 &  _LC6_B3
         #  _LC2_C20;

-- Node name is 'SD2~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD2~1', location is LC3_C24, type is buried.
-- synthesized logic cell 
_LC3_C24 = LCELL( _EQ214);
  _EQ214 =  DD7 &  _EC6_B & !/IO
         #  DD2 &  /IO;

-- Node name is 'SD2' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD2', location is LC1_C24, type is buried.
SD2      = LCELL( _EQ215);
  _EQ215 =  _LC3_C24
         #  AY_DD2 &  _LC6_B3
         #  _LC5_C24;

-- Node name is 'SD3~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD3~1', location is LC4_B5, type is buried.
-- synthesized logic cell 
_LC4_B5  = LCELL( _EQ216);
  _EQ216 =  DD7 &  _EC7_B & !/IO
         #  DCP3 &  /IO;

-- Node name is 'SD3' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD3', location is LC3_C4, type is buried.
SD3      = LCELL( _EQ217);
  _EQ217 =  _LC4_B5
         #  AY_DD3 &  _LC6_B3
         #  _LC1_C4;

-- Node name is 'SD4~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD4~1', location is LC8_B3, type is buried.
-- synthesized logic cell 
_LC8_B3  = LCELL( _EQ218);
  _EQ218 =  KBD4 &  _LC4_B3
         #  DCP4 &  /IO;

-- Node name is 'SD4' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD4', location is LC1_A8, type is buried.
SD4      = LCELL( _EQ219);
  _EQ219 =  _LC4_A8
         #  _LC8_B3
         #  AY_DD4 &  _LC6_B3;

-- Node name is 'SD5~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD5~1', location is LC3_B3, type is buried.
-- synthesized logic cell 
_LC3_B3  = LCELL( _EQ220);
  _EQ220 =  DD7 &  _EC3_B & !/IO
         #  DCP5 &  /IO;

-- Node name is 'SD5' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD5', location is LC2_B3, type is buried.
SD5      = LCELL( _EQ221);
  _EQ221 =  _LC3_B3
         #  AY_DD5 &  _LC6_B3
         #  _LC4_B3;

-- Node name is 'SD6~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD6~1', location is LC4_B2, type is buried.
-- synthesized logic cell 
_LC4_B2  = LCELL( _EQ222);
  _EQ222 =  DD7 &  _EC8_B & !/IO
         #  DD6 &  /IO;

-- Node name is 'SD6' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD6', location is LC5_B2, type is buried.
SD6      = LCELL( _EQ223);
  _EQ223 =  _LC4_B2
         #  AY_DD6 &  _LC6_B3
         #  _LC7_B2;

-- Node name is 'SD7~1' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD7~1', location is LC8_C7, type is buried.
-- synthesized logic cell 
_LC8_C7  = LCELL( _EQ224);
  _EQ224 =  DD7 &  /IO
         #  AY_DD7 &  _LC6_B3;

-- Node name is 'SD7' from file "sprint08.tdf" line 1406, column 13
-- Equation name is 'SD7', location is LC3_C7, type is buried.
SD7      = LCELL( _EQ225);
  _EQ225 =  _LC6_C7
         #  _LC8_C7
         #  KBD5 &  _LC4_B3;

-- Node name is 'SINC' from file "sprint08.tdf" line 288, column 2
-- Equation name is 'SINC', type is output 
SINC     =  _LC8_C22;

-- Node name is 'SINC_H' from file "sprint08.tdf" line 2142, column 2
-- Equation name is 'SINC_H', type is output 
SINC_H   =  _LC1_A18;

-- Node name is 'SINC_HH' from file "sprint08.tdf" line 1722, column 12
-- Equation name is 'SINC_HH', location is LC7_C17, type is buried.
SINC_HH  = DFFE( _EQ226,  CTH1,  VCC,  VCC,  VCC);
  _EQ226 =  CTH2 & !CTH3 & !CTH4 &  CTH5;

-- Node name is 'SINC_VV' from file "sprint08.tdf" line 1726, column 12
-- Equation name is 'SINC_VV', location is LC3_C16, type is buried.
SINC_VV  = DFFE( _EQ227,  CTV5,  VCC,  VCC,  VCC);
  _EQ227 =  CTV6 &  CTV7;

-- Node name is 'SND_L0' from file "sprint08.tdf" line 3457, column 3
-- Equation name is 'SND_L0', type is output 
SND_L0   =  _LC6_A8;

-- Node name is 'SND_L1' from file "sprint08.tdf" line 3458, column 3
-- Equation name is 'SND_L1', type is output 
SND_L1   =  GND;

-- Node name is 'SND_R0' from file "sprint08.tdf" line 3460, column 3
-- Equation name is 'SND_R0', type is output 
SND_R0   =  _LC3_A8;

-- Node name is 'SND_R1' from file "sprint08.tdf" line 3461, column 3
-- Equation name is 'SND_R1', type is output 
SND_R1   =  GND;

-- Node name is 'SVA2' from file "sprint08.tdf" line 1818, column 46
-- Equation name is 'SVA2', location is LC7_C22, type is buried.
SVA2     = LCELL( _EQ228);
  _EQ228 =  CTV6 & !VCM2
         #  CTV0 &  VCM2;

-- Node name is 'SVA3' from file "sprint08.tdf" line 1818, column 46
-- Equation name is 'SVA3', location is LC3_C22, type is buried.
SVA3     = LCELL( _EQ229);
  _EQ229 =  CTV7 & !VCM2
         #  CTV1 &  VCM2;

-- Node name is 'SVA5' from file "sprint08.tdf" line 1818, column 46
-- Equation name is 'SVA5', location is LC4_C22, type is buried.
SVA5     = LCELL( _EQ230);
  _EQ230 = !VCM2
         #  CTV6;

-- Node name is 'SVA6' from file "sprint08.tdf" line 1818, column 46
-- Equation name is 'SVA6', location is LC1_B17, type is buried.
SVA6     = LCELL( _EQ231);
  _EQ231 = !VCM2
         #  CTV7;

-- Node name is 'SYS' from file "sprint08.tdf" line 313, column 2
-- Equation name is 'SYS', location is LC5_B13, type is buried.
SYS      = DFFE(!A6,  _LC5_B3,  /RESET,  VCC, !_LC2_B13);

-- Node name is 'TAPE_OUT' from file "sprint08.tdf" line 1471, column 2
-- Equation name is 'TAPE_OUT', type is output 
TAPE_OUT =  BRD3;

-- Node name is 'TB_SW' from file "sprint08.tdf" line 315, column 2
-- Equation name is 'TB_SW', location is LC8_B16, type is buried.
!TB_SW   = TB_SW~NOT;
TB_SW~NOT = DFFE(!D0,  _LC5_B3,  /RESET,  VCC,  _LC7_C15);

-- Node name is 'TSN_W3' from file "sprint08.tdf" line 329, column 2
-- Equation name is 'TSN_W3', location is LC5_B23, type is buried.
TSN_W3   = DFFE( _EQ232, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ232 =  VCM2
         #  VCM0
         #  VCM1;

-- Node name is 'TURBO' from file "sprint08.tdf" line 1516, column 12
-- Equation name is 'TURBO', location is LC6_C13, type is buried.
TURBO    = DFFE( _EQ233, GLOBAL( /M1),  VCC,  VCC,  VCC);
  _EQ233 =  _LC7_C5 &  TB_SW;

-- Node name is 'TURBO_LED' from file "sprint08.tdf" line 1448, column 2
-- Equation name is 'TURBO_LED', type is output 
TURBO_LED = !TURBO;

-- Node name is 'VA0' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA0', type is output 
VA0      =  VLA2;

-- Node name is 'VA1' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA1', type is output 
VA1      =  VLA3;

-- Node name is 'VA2' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA2', type is output 
VA2      =  VLA4;

-- Node name is 'VA3' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA3', type is output 
VA3      =  VLA5;

-- Node name is 'VA4' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA4', type is output 
VA4      =  VLA6;

-- Node name is 'VA5' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA5', type is output 
VA5      =  VLA7;

-- Node name is 'VA6' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA6', type is output 
VA6      =  VLA8;

-- Node name is 'VA7' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA7', type is output 
VA7      =  VLA9;

-- Node name is 'VA8' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA8', type is output 
VA8      =  VLA10;

-- Node name is 'VA9' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA9', type is output 
VA9      =  VLA11;

-- Node name is 'VA10' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA10', type is output 
VA10     =  VLA12;

-- Node name is 'VA11' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA11', type is output 
VA11     =  VLA13;

-- Node name is 'VA12' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA12', type is output 
VA12     =  VLA14;

-- Node name is 'VA13' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA13', type is output 
VA13     =  VLA15;

-- Node name is 'VA14' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA14', type is output 
VA14     =  VLA16;

-- Node name is 'VA15' from file "sprint08.tdf" line 2281, column 4
-- Equation name is 'VA15', type is output 
VA15     =  VLA17;

-- Node name is 'VCM0' from file "sprint08.tdf" line 330, column 5
-- Equation name is 'VCM0', location is LC6_B20, type is buried.
VCM0     = DFFE( _EQ234, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ234 = !CT0 & !CT2
         #  AY_CCC0 & !CT0;

-- Node name is 'VCM1' from file "sprint08.tdf" line 330, column 5
-- Equation name is 'VCM1', location is LC5_B20, type is buried.
VCM1     = DFFE( _EQ235, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ235 =  AY_CCC0 & !CT0 & !CT2
         # !AY_CCC0 & !CT0 &  CT2;

-- Node name is 'VCM2' from file "sprint08.tdf" line 330, column 5
-- Equation name is 'VCM2', location is LC4_B20, type is buried.
VCM2     = DFFE( _EQ236, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ236 =  AY_CCC0 & !CT0 &  CT2
         # !AY_CCC0 &  CT0 & !CT2;

-- Node name is 'V_CS0' from file "sprint08.tdf" line 332, column 6
-- Equation name is 'V_CS0', type is output 
V_CS0    =  GND;

-- Node name is 'V_CS1' from file "sprint08.tdf" line 332, column 6
-- Equation name is 'V_CS1', type is output 
V_CS1    =  VCC;

-- Node name is 'VD00' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD00', type is bidir 
VD00     = TRI(_LC3_B5, !_LC1_B23);

-- Node name is 'VD01' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD01', type is bidir 
VD01     = TRI(_LC5_A13, !_LC1_B23);

-- Node name is 'VD02' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD02', type is bidir 
VD02     = TRI(_LC7_A16, !_LC1_B23);

-- Node name is 'VD03' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD03', type is bidir 
VD03     = TRI(_LC7_C10, !_LC1_B23);

-- Node name is 'VD04' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD04', type is bidir 
VD04     = TRI(_LC8_A13, !_LC1_B23);

-- Node name is 'VD05' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD05', type is bidir 
VD05     = TRI(_LC3_A16, !_LC1_B23);

-- Node name is 'VD06' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD06', type is bidir 
VD06     = TRI(_LC5_B11, !_LC1_B23);

-- Node name is 'VD07' from file "sprint08.tdf" line 1436, column 6
-- Equation name is 'VD07', type is bidir 
VD07     = TRI(_LC4_A6, !_LC1_B23);

-- Node name is 'VD10' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD10', type is bidir 
VD10     = TRI(_LC4_C10,  GND);

-- Node name is 'VD11' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD11', type is bidir 
VD11     = TRI(_LC4_A13,  GND);

-- Node name is 'VD12' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD12', type is bidir 
VD12     = TRI(_LC8_A16,  GND);

-- Node name is 'VD13' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD13', type is bidir 
VD13     = TRI(_LC5_C10,  GND);

-- Node name is 'VD14' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD14', type is bidir 
VD14     = TRI(_LC6_A13,  GND);

-- Node name is 'VD15' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD15', type is bidir 
VD15     = TRI(_LC2_A16,  GND);

-- Node name is 'VD16' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD16', type is bidir 
VD16     = TRI(_LC2_B11,  GND);

-- Node name is 'VD17' from file "sprint08.tdf" line 1437, column 6
-- Equation name is 'VD17', type is bidir 
VD17     = TRI(_LC1_A6,  GND);

-- Node name is 'VD20' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD20', type is bidir 
VD20     = TRI(_LC8_C10,  GND);

-- Node name is 'VD21' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD21', type is bidir 
VD21     = TRI(_LC2_A13,  GND);

-- Node name is 'VD22' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD22', type is bidir 
VD22     = TRI(_LC1_A16,  GND);

-- Node name is 'VD23' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD23', type is bidir 
VD23     = TRI(_LC6_C10,  GND);

-- Node name is 'VD24' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD24', type is bidir 
VD24     = TRI(_LC3_A13,  GND);

-- Node name is 'VD25' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD25', type is bidir 
VD25     = TRI(_LC6_A16,  GND);

-- Node name is 'VD26' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD26', type is bidir 
VD26     = TRI(_LC8_B11,  GND);

-- Node name is 'VD27' from file "sprint08.tdf" line 1438, column 6
-- Equation name is 'VD27', type is bidir 
VD27     = TRI(_LC5_A6,  GND);

-- Node name is 'VD30' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD30', type is bidir 
VD30     = TRI(MXVD0,  GND);

-- Node name is 'VD31' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD31', type is bidir 
VD31     = TRI(MXVD1,  GND);

-- Node name is 'VD32' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD32', type is bidir 
VD32     = TRI(MXVD2,  GND);

-- Node name is 'VD33' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD33', type is bidir 
VD33     = TRI(MXVD3,  GND);

-- Node name is 'VD34' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD34', type is bidir 
VD34     = TRI(MXVD4,  GND);

-- Node name is 'VD35' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD35', type is bidir 
VD35     = TRI(MXVD5,  GND);

-- Node name is 'VD36' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD36', type is bidir 
VD36     = TRI(MXVD6,  GND);

-- Node name is 'VD37' from file "sprint08.tdf" line 1439, column 6
-- Equation name is 'VD37', type is bidir 
VD37     = TRI(MXVD7,  GND);

-- Node name is 'VLA2' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA2', location is LC2_C2, type is buried.
VLA2     = DFFE( _EQ237, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ237 =  SVA2 &  VCM0
         #  _LC3_C2;

-- Node name is 'VLA3' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA3', location is LC5_C19, type is buried.
VLA3     = DFFE( _EQ238, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ238 =  _LC8_C19
         #  SVA3 &  VCM0;

-- Node name is 'VLA4' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA4', location is LC4_B23, type is buried.
VLA4     = DFFE( _EQ239, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ239 =  CTV2 &  VCM0 &  VCM2
         #  _LC6_B23;

-- Node name is 'VLA5' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA5', location is LC7_C2, type is buried.
VLA5     = DFFE( _EQ240, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ240 =  SVA5 &  VCM0
         # !VCM0 & !VCM1
         #  AA11 & !VCM0;

-- Node name is 'VLA6' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA6', location is LC6_B17, type is buried.
VLA6     = DFFE( _EQ241, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ241 =  SVA6 &  VCM0
         # !VCM0 & !VCM1
         #  AA12 & !VCM0;

-- Node name is 'VLA7' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA7', location is LC6_B6, type is buried.
VLA7     = DFFE( _EQ242, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ242 = !VCM0 & !VCM1
         #  AX128 & !VCM0
         #  PN3 &  VCM0;

-- Node name is 'VLA8' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA8', location is LC8_C2, type is buried.
VLA8     = DFFE( _EQ243, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ243 = !VCM0 & !VCM1;

-- Node name is 'VLA9' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA9', location is LC6_C2, type is buried.
VLA9     = DFFE( _EQ244, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ244 = !VCM0 & !VCM1;

-- Node name is 'VLA10' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA10', location is LC5_A21, type is buried.
VLA10    = DFFE( _EQ245, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ245 =  _LC3_A18
         #  AA0 & !VCM0 &  VCM1;

-- Node name is 'VLA11' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA11', location is LC3_B19, type is buried.
VLA11    = DFFE( _EQ246, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ246 =  _LC4_B19
         #  CTH1 &  VCM0;

-- Node name is 'VLA12' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA12', location is LC5_C2, type is buried.
VLA12    = DFFE( _EQ247, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ247 =  _LC4_C2
         #  CTH2 &  VCM0;

-- Node name is 'VLA13' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA13', location is LC8_A22, type is buried.
VLA13    = DFFE( _EQ248, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ248 =  CTH3 &  VCM0
         #  _LC1_C17;

-- Node name is 'VLA14' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA14', location is LC2_B21, type is buried.
VLA14    = DFFE( _EQ249, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ249 =  CTH4 &  VCM0
         #  _LC5_B21;

-- Node name is 'VLA15' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA15', location is LC7_C21, type is buried.
VLA15    = DFFE( _EQ250, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ250 =  CTV3 &  VCM0
         #  _LC1_B14;

-- Node name is 'VLA16' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA16', location is LC5_C21, type is buried.
VLA16    = DFFE( _EQ251, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ251 =  CTV4 &  VCM0
         #  _LC6_B13;

-- Node name is 'VLA17' from file "sprint08.tdf" line 334, column 5
-- Equation name is 'VLA17', location is LC8_C21, type is buried.
VLA17    = DFFE( _EQ252, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ252 =  CTV5 &  VCM0
         #  _LC8_C17;

-- Node name is 'V_WAIT~1' from file "sprint08.tdf" line 1560, column 50
-- Equation name is 'V_WAIT~1', location is LC7_B4, type is buried.
-- synthesized logic cell 
_LC7_B4  = LCELL( _EQ253);
  _EQ253 =  _LC5_A3
         #  /MR
         #  MC_END;

-- Node name is 'V_WE' from file "sprint08.tdf" line 340, column 2
-- Equation name is 'V_WE', location is LC8_B23, type is buried.
!V_WE    = V_WE~NOT;
V_WE~NOT = DFFE( _EQ254, GLOBAL( TG42),  _LC6_B21,  VCC,  VCC);
  _EQ254 = !MXWE & !VCM0 &  VCM1;

-- Node name is 'V_WR0' from file "sprint08.tdf" line 333, column 6
-- Equation name is 'V_WR0', type is output 
V_WR0    =  _LC1_B23;

-- Node name is 'V_WR1' from file "sprint08.tdf" line 333, column 6
-- Equation name is 'V_WR1', type is output 
V_WR1    =  VCC;

-- Node name is 'V_WR2' from file "sprint08.tdf" line 333, column 6
-- Equation name is 'V_WR2', type is output 
V_WR2    =  VCC;

-- Node name is 'V_WR3' from file "sprint08.tdf" line 333, column 6
-- Equation name is 'V_WR3', type is output 
V_WR3    =  VCC;

-- Node name is 'WR_COL' from file "sprint08.tdf" line 368, column 2
-- Equation name is 'WR_COL', location is LC4_B21, type is buried.
WR_COL   = DFFE( _EQ255, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ255 =  VCM2
         # !VCM0;

-- Node name is 'WR_KBD' from file "sprint08.tdf" line 2558, column 41
-- Equation name is 'WR_KBD', location is LC1_C6, type is buried.
!WR_KBD  = WR_KBD~NOT;
WR_KBD~NOT = LCELL( _EQ256);
  _EQ256 = !K_CLK &  _LC1_C3 &  RXA0 &  RXA1;

-- Node name is 'WR_PIC' from file "sprint08.tdf" line 367, column 2
-- Equation name is 'WR_PIC', location is LC2_B23, type is buried.
WR_PIC   = DFFE( _EQ257, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ257 = !VCM2
         # !VCM0;

-- Node name is 'XACS' from file "sprint08.tdf" line 708, column 19
-- Equation name is 'XACS', type is output 
XACS     =  XC3;

-- Node name is 'XA0' from file "sprint08.tdf" line 708, column 4
-- Equation name is 'XA0', type is output 
XA0      =  XC0;

-- Node name is 'XA1' from file "sprint08.tdf" line 708, column 4
-- Equation name is 'XA1', type is output 
XA1      =  XC1;

-- Node name is 'XA2' from file "sprint08.tdf" line 708, column 4
-- Equation name is 'XA2', type is output 
XA2      =  XC2;

-- Node name is 'XC0' from file "sprint08.tdf" line 790, column 12
-- Equation name is 'XC0', location is LC3_A3, type is buried.
XC0      = LCELL( _EQ258);
  _EQ258 =  _EC1_B & !_LC8_A3;

-- Node name is 'XC1' from file "sprint08.tdf" line 790, column 12
-- Equation name is 'XC1', location is LC6_A3, type is buried.
XC1      = LCELL( _EQ259);
  _EQ259 =  _LC8_A3
         #  _EC3_B;

-- Node name is 'XC2' from file "sprint08.tdf" line 790, column 12
-- Equation name is 'XC2', location is LC4_A3, type is buried.
XC2      = LCELL( _EQ260);
  _EQ260 =  _LC8_A3
         #  _EC8_B;

-- Node name is 'XC3' from file "sprint08.tdf" line 795, column 15
-- Equation name is 'XC3', location is LC3_B7, type is buried.
XC3      = LCELL( _EQ261);
  _EQ261 =  _LC8_B7
         #  BLK_R;

-- Node name is '~GND~' 
-- Equation name is '~GND~', location is LC4_B17, type is buried.
-- synthesized logic cell 
_LC4_B17 = LCELL( GND);

-- Node name is '/INT' from file "sprint08.tdf" line 1498, column 2
-- Equation name is '/INT', type is bidir 
/INT     = OPNDRN(INTT);

-- Node name is '/IOM' from file "sprint08.tdf" line 1533, column 9
-- Equation name is '/IOM', location is LC2_B20, type is buried.
!/IOM    = /IOM~NOT;
/IOM~NOT = DFFE( /M1,  CT0, GLOBAL(!/IO),  VCC,  VCC);

-- Node name is '/IOM1' from file "sprint08.tdf" line 1534, column 10
-- Equation name is '/IOM1', location is LC5_B7, type is buried.
!/IOM1   = /IOM1~NOT;
/IOM1~NOT = DFFE( _EQ262,  CT2, GLOBAL(!/IO),  VCC,  VCC);
  _EQ262 =  MC_END &  /M1;

-- Node name is '/IOWR' from file "sprint08.tdf" line 1537, column 17
-- Equation name is '/IOWR', location is LC5_B16, type is buried.
/IOWR    = LCELL( _EQ263);
  _EQ263 =  /IOM1
         #  /WR;

-- Node name is '/NMI' from file "sprint08.tdf" line 1499, column 2
-- Equation name is '/NMI', type is bidir 
/NMI     = OPNDRN(VCC);

-- Node name is '/RESET' from file "sprint08.tdf" line 1482, column 2
-- Equation name is '/RESET', type is bidir 
/RESET   = OPNDRN(_LC4_C15);

-- Node name is '/WAIT' from file "sprint08.tdf" line 1549, column 2
-- Equation name is '/WAIT', type is bidir 
/WAIT    = OPNDRN(/WAITT);

-- Node name is '/WAITT' from file "sprint08.tdf" line 1547, column 20
-- Equation name is '/WAITT', location is LC4_B4, type is buried.
/WAITT   = LCELL( _EQ264);
  _EQ264 = !TURBO
         #  _LC2_B7 &  _LC7_B4;

-- Node name is '/WE' from file "sprint08.tdf" line 1590, column 3
-- Equation name is '/WE', type is output 
/WE      =  /WE1;

-- Node name is '/WE1' from file "sprint08.tdf" line 1588, column 34
-- Equation name is '/WE1', location is LC1_B8, type is buried.
!/WE1    = /WE1~NOT;
/WE1~NOT = LCELL( _EQ265);
  _EQ265 =  _LC1_B12 & !MC_SYCLE & !/MR & !/WR;

-- Node name is ':1921' from file "sprint08.tdf" line 746, column 28
-- Equation name is '_LC8_B10', type is buried 
_LC8_B10 = DFFE( GND,  VCC,  /RESET,  _LC2_B4,  VCC);

-- Node name is ':1922' from file "sprint08.tdf" line 748, column 8
-- Equation name is '_LC4_B10', type is buried 
_LC4_B10 = LCELL( _EQ266);
  _EQ266 =  /IO &  _LC8_B10
         #  /IO &  _LC1_B10;

-- Node name is ':1924' from file "sprint08.tdf" line 767, column 29
-- Equation name is '_LC7_B10', type is buried 
_LC7_B10 = LCELL( _EQ267);
  _EQ267 =  _EC5_B &  _EC8_B & !_LC1_B12
         #  _EC5_B &  SC_PGS;

-- Node name is ':1926' from file "sprint08.tdf" line 774, column 11
-- Equation name is '_LC1_B12', type is buried 
_LC1_B12 = LCELL( _EQ268);
  _EQ268 =  A15
         #  A14
         #  SC0 &  SYS;

-- Node name is ':1929' from file "sprint08.tdf" line 786, column 5
-- Equation name is '_LC8_A3', type is buried 
!_LC8_A3 = _LC8_A3~NOT;
_LC8_A3~NOT = DFFE( _EQ269, GLOBAL( TG42), !_LC2_C13,  VCC,  VCC);
  _EQ269 = !/IO
         # !/MR;

-- Node name is ':1930' from file "sprint08.tdf" line 795, column 18
-- Equation name is '_LC8_B7', type is buried 
_LC8_B7  = DFFE( _EQ270, !CT2, GLOBAL(!/IO),  VCC,  VCC);
  _EQ270 = !DD6 & !DD7 &  _EC5_B & !/IOM1;

-- Node name is ':1958' from file "sprint08.tdf" line 1274, column 5
-- Equation name is '_LC7_B21', type is buried 
_LC7_B21 = DFFE( AY_CCC2, GLOBAL( TG42), !_LC8_B21,  VCC,  VCC);

-- Node name is ':1962' from file "sprint08.tdf" line 1379, column 26
-- Equation name is '_LC3_B11', type is buried 
_LC3_B11 = DFFE( DOS,  AY_CCC2,  VCC,  VCC,  VCC);

-- Node name is ':1964' from file "sprint08.tdf" line 1415, column 43
-- Equation name is '_LC5_B4', type is buried 
!_LC5_B4 = _LC5_B4~NOT;
_LC5_B4~NOT = DFFE(!/RD, !_LC6_B8, GLOBAL(!/MR),  VCC,  VCC);

-- Node name is '~1966~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1966~1', location is LC1_C16, type is buried.
-- synthesized logic cell 
_LC1_C16 = LCELL( D0);

-- Node name is '~1972~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1972~1', location is LC7_A13, type is buried.
-- synthesized logic cell 
_LC7_A13 = LCELL( D1);

-- Node name is '~1978~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1978~1', location is LC7_B22, type is buried.
-- synthesized logic cell 
_LC7_B22 = LCELL( D2);

-- Node name is '~1984~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1984~1', location is LC2_C10, type is buried.
-- synthesized logic cell 
_LC2_C10 = LCELL( D3);

-- Node name is '~1990~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1990~1', location is LC2_A3, type is buried.
-- synthesized logic cell 
_LC2_A3  = LCELL( D4);

-- Node name is '~1996~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~1996~1', location is LC3_C13, type is buried.
-- synthesized logic cell 
_LC3_C13 = LCELL( D5);

-- Node name is '~2002~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~2002~1', location is LC1_B11, type is buried.
-- synthesized logic cell 
_LC1_B11 = LCELL( D6);

-- Node name is '~2008~1' from file "sprint08.tdf" line 1419, column 11
-- Equation name is '~2008~1', location is LC2_C4, type is buried.
-- synthesized logic cell 
_LC2_C4  = LCELL( D7);

-- Node name is ':2013' from file "sprint08.tdf" line 1450, column 13
-- Equation name is '_LC7_B23', type is buried 
_LC7_B23 = LCELL( TSN_W3);

-- Node name is ':2019' from file "sprint08.tdf" line 1482, column 19
-- Equation name is '_LC4_C15', type is buried 
_LC4_C15 = DFFE( VCC,  CTV0,  KB_RESET,  VCC,  VCC);

-- Node name is ':2024' from file "sprint08.tdf" line 1495, column 17
-- Equation name is '_LC5_C22', type is buried 
_LC5_C22 = DFFE( _EQ271,  CT5,  VCC,  VCC,  VCC);
  _EQ271 =  CTV6 &  CTV7 & !_LC6_C21;

-- Node name is ':2032' from file "sprint08.tdf" line 1516, column 25
-- Equation name is '_LC7_C5', type is buried 
!_LC7_C5 = _LC7_C5~NOT;
_LC7_C5~NOT = DFFE( _EQ272,  KB_F12,  /RESET,  VCC,  VCC);
  _EQ272 = !KB_CTRL &  _LC7_C5
         #  KB_CTRL & !_LC7_C5;

-- Node name is ':2034' from file "sprint08.tdf" line 1529, column 10
-- Equation name is '_LC7_B20', type is buried 
_LC7_B20 = DFFE( _EQ273, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ273 = !CT0 &  CT2 &  TURBO
         #  CT0 & !CT2 &  TURBO
         #  CT3 & !TURBO;

-- Node name is ':2040' from file "sprint08.tdf" line 1559, column 62
-- Equation name is '_LC6_B7', type is buried 
_LC6_B7  = DFFE( _EQ274,  CT2, !/IOM1,  VCC,  VCC);
  _EQ274 =  DD7
         #  DD6
         #  _LC4_B7;

-- Node name is ':2041' from file "sprint08.tdf" line 1559, column 87
-- Equation name is '_LC4_B7', type is buried 
_LC4_B7  = DFFE( _LC1_B7,  CT2, !/IOM1,  VCC,  VCC);

-- Node name is ':2042' from file "sprint08.tdf" line 1559, column 91
-- Equation name is '_LC1_B7', type is buried 
_LC1_B7  = DFFE( VCC,  CT2, !/IOM1,  VCC,  VCC);

-- Node name is ':2043' from file "sprint08.tdf" line 1563, column 4
-- Equation name is '_LC5_A3', type is buried 
_LC5_A3  = DFFE( _EQ275, GLOBAL( TG42),  BLK_R,  VCC,  VCC);
  _EQ275 =  _EC1_B &  _EC3_B &  _EC5_B &  _EC8_B;

-- Node name is ':2054' from file "sprint08.tdf" line 1630, column 8
-- Equation name is '_LC5_B9', type is buried 
_LC5_B9  = LCELL( _EQ276);
  _EQ276 =  MD4 &  MD5 &  MD6 &  MD7;

-- Node name is ':2058' from file "sprint08.tdf" line 1723, column 11
-- Equation name is '_LC1_A18', type is buried 
_LC1_A18 = DFFE( SINC_HH, !CTH1,  VCC,  VCC,  VCC);

-- Node name is ':2061' from file "sprint08.tdf" line 1729, column 9
-- Equation name is '_LC8_C22', type is buried 
_LC8_C22 = DFFE( _EQ277,  CT5,  VCC,  VCC,  VCC);
  _EQ277 = !CTV7 & !_LC1_A18
         # !CTV6 & !_LC1_A18
         # !_LC1_A18 &  _LC6_C21
         #  CTV6 &  CTV7 &  _LC1_A18 & !_LC6_C21;

-- Node name is ':2069' from file "sprint08.tdf" line 1875, column 13
-- Equation name is '_LC6_B21', type is buried 
_LC6_B21 = DFFE( V_WE, GLOBAL(!TG42),  VCC,  VCC,  VCC);

-- Node name is ':2071' from file "sprint08.tdf" line 1883, column 11
-- Equation name is '_LC1_B23', type is buried 
_LC1_B23 = LCELL( V_WE);

-- Node name is ':2140' from file "sprint08.tdf" line 2479, column 28
-- Equation name is '_LC8_C1', type is buried 
_LC8_C1  = LCELL( _EQ278);
  _EQ278 =  KB_D1 &  KB_D2 &  KB_D3 & !KB_D5;

-- Node name is ':2142' from file "sprint08.tdf" line 2501, column 7
-- Equation name is '_LC7_C3', type is buried 
_LC7_C3  = LCELL( _EQ279);
  _EQ279 =  KB_CT2 & !RXA0 & !RXA1
         # !KB_CT1 & !RXA0 & !RXA1;

-- Node name is ':2143' from file "sprint08.tdf" line 2513, column 34
-- Equation name is '_LC5_C9', type is buried 
_LC5_C9  = LCELL( _EQ280);
  _EQ280 =  KDD6 &  KDD7;

-- Node name is ':2144' from file "sprint08.tdf" line 2513, column 8
-- Equation name is '_LC4_C6', type is buried 
_LC4_C6  = LCELL( _EQ281);
  _EQ281 =  /IO & !RXA0 & !RXA1;

-- Node name is ':2149' from file "sprint08.tdf" line 2558, column 21
-- Equation name is '_LC1_C3', type is buried 
_LC1_C3  = LCELL( _EQ282);
  _EQ282 = !KB_CT0 &  KB_CT1 & !KB_CT2;

-- Node name is ':2195' from file "sprint08.tdf" line 3103, column 32
-- Equation name is '_LC2_B16', type is buried 
_LC2_B16 = LCELL( _EQ283);
  _EQ283 =  /IOM1
         #  /WR
         #  _LC1_B16
         #  _LC2_B5;

-- Node name is ':2198' from file "sprint08.tdf" line 3116, column 95
-- Equation name is '_LC5_A1', type is buried 
_LC5_A1  = LCELL( _EQ284);
  _EQ284 =  AY_D_WR
         # !AY_AAX0;

-- Node name is ':2199' from file "sprint08.tdf" line 3116, column 21
-- Equation name is '_LC3_A17', type is buried 
_LC3_A17 = DFFE( _EQ285, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ285 =  _LC2_A17
         # !AY_CCC1
         # !_EC8_A;

-- Node name is ':2200' from file "sprint08.tdf" line 3141, column 14
-- Equation name is '_LC8_A9', type is buried 
_LC8_A9  = LCELL( _EQ286);
  _EQ286 = !_EC5_A
         #  _EC2_A
         # !AY_CX &  _EC8_A;

-- Node name is ':2201' from file "sprint08.tdf" line 3157, column 15
-- Equation name is '_LC4_A9', type is buried 
_LC4_A9  = DFFE( _EQ287, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ287 =  AY_CCC1 & !_EC5_A & !_EC8_A &  _LC3_A9;

-- Node name is ':2202' from file "sprint08.tdf" line 3162, column 14
-- Equation name is '_LC1_A9', type is buried 
_LC1_A9  = DFFE( _EQ288, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ288 =  AY_CCC1 &  _EC2_A &  _EC5_A &  _EC8_A
         #  AY_CCC1 & !_EC2_A &  _EC5_A & !_EC8_A;

-- Node name is ':2203' from file "sprint08.tdf" line 3164, column 5
-- Equation name is '_LC5_A9', type is buried 
_LC5_A9  = DFFE( _EQ289, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ289 = !_EC2_A &  _EC5_A & !_EC8_A;

-- Node name is ':2204' from file "sprint08.tdf" line 3165, column 11
-- Equation name is '_LC2_A11', type is buried 
_LC2_A11 = LCELL( _EQ290);
  _EQ290 = !AY_DAT6 & !AY_DAT7 & !_LC6_A2 &  _LC8_A12;

-- Node name is ':2205' from file "sprint08.tdf" line 3167, column 11
-- Equation name is '_LC4_A23', type is buried 
_LC4_A23 = DFFE( _EQ291, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ291 = !AY_F_RES & !_EC1_A
         #  _EC1_A & !/RESET;

-- Node name is ':2206' from file "sprint08.tdf" line 3171, column 28
-- Equation name is '_LC7_A3', type is buried 
_LC7_A3  = DFFE(!AY_DAT_WR, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is ':2207' from file "sprint08.tdf" line 3173, column 49
-- Equation name is '_LC5_A10', type is buried 
_LC5_A10 = DFFE( _EQ292, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ292 =  _LC3_A10
         #  AY_C &  _LC4_A10;

-- Node name is ':2208' from file "sprint08.tdf" line 3173, column 54
-- Equation name is '_LC3_A10', type is buried 
_LC3_A10 = DFFE(!_EC2_A, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is ':2209' from file "sprint08.tdf" line 3173, column 86
-- Equation name is '_LC4_A10', type is buried 
_LC4_A10 = DFFE( _EC8_A, GLOBAL( TG42),  VCC,  VCC,  VCC);

-- Node name is ':2213' from file "sprint08.tdf" line 3203, column 21
-- Equation name is '_LC1_A5', type is buried 
_LC1_A5  = LCELL( _EQ293);
  _EQ293 =  AY_OUT1 &  AY_SH0
         #  AY_OUT1 &  AY_X_3
         #  AY_SH0 &  AY_X_0
         #  AY_X_0 &  AY_X_3;

-- Node name is ':2214' from file "sprint08.tdf" line 3205, column 18
-- Equation name is '_LC1_A7', type is buried 
_LC1_A7  = LCELL( _EQ294);
  _EQ294 =  AY_OUT2 &  AY_SH0
         #  AY_OUT2 &  AY_X_4
         #  AY_SH0 &  AY_X_1
         #  AY_X_1 &  AY_X_4;

-- Node name is ':2215' from file "sprint08.tdf" line 3207, column 18
-- Equation name is '_LC3_A12', type is buried 
_LC3_A12 = LCELL( _EQ295);
  _EQ295 =  AY_OUT3 &  AY_SH0
         #  AY_OUT3 &  AY_X_5
         #  AY_SH0 &  AY_X_2
         #  AY_X_2 &  AY_X_5;

-- Node name is ':2216' from file "sprint08.tdf" line 3211, column 17
-- Equation name is '_LC5_A24', type is buried 
_LC5_A24 = DFFE( _EQ296, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ296 = !AY_CCC5 & !AY_CCC6 & !AY_CCC7 & !AY_CCC8;

-- Node name is ':2217' from file "sprint08.tdf" line 3221, column 29
-- Equation name is '_LC7_A22', type is buried 
_LC7_A22 = DFFE( _EQ297, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ297 =  AY_CX & !_EC1_A & !_EC7_A &  _LC5_A22;

-- Node name is ':2218' from file "sprint08.tdf" line 3223, column 22
-- Equation name is '_LC1_A21', type is buried 
_LC1_A21 = LCELL( _EQ298);
  _EQ298 =  AY_SH0 &  AY_SH4 &  A0
         #  AY_SH0 & !AY_SH4 & !A0
         # !AY_SH0 &  AY_SH4 & !A0
         # !AY_SH0 & !AY_SH4 &  A0;

-- Node name is ':2219' from file "sprint08.tdf" line 3242, column 29
-- Equation name is '_LC3_A22', type is buried 
_LC3_A22 = DFFE( _EQ299, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ299 = !AY_BBLK &  _EC1_A & !_EC7_A &  _LC5_A22;

-- Node name is ':2220' from file "sprint08.tdf" line 3246, column 16
-- Equation name is '_LC2_A22', type is buried 
_LC2_A22 = DFFE( _EQ300, GLOBAL( TG42),  VCC,  VCC,  VCC);
  _EQ300 = !_EC1_A &  _EC7_A &  _LC5_A22;

-- Node name is '~2224~1' from file "sprint08.tdf" line 3273, column 11
-- Equation name is '~2224~1', location is LC3_A8, type is buried.
-- synthesized logic cell 
_LC3_A8  = DFFE( _EQ301,  AY_CCC1,  VCC,  VCC,  VCC);
  _EQ301 = !AY_XXM5 &  _LC7_A24
         #  AY_CCC7 &  _LC7_A24
         #  AY_CCC7 & !AY_XXM5;

-- Node name is ':2224' from file "sprint08.tdf" line 3273, column 11
-- Equation name is '_LC6_A8', type is buried 
_LC6_A8  = DFFE( _EQ302,  AY_CCC1,  VCC,  VCC,  VCC);
  _EQ302 = !AY_XXM5 &  _LC7_A24
         #  AY_CCC7 &  _LC7_A24
         #  AY_CCC7 & !AY_XXM5;

-- Node name is ':2292' from file "sprint08.tdf" line 734, column 3
-- Equation name is '_LC1_B10', type is buried 
!_LC1_B10 = _LC1_B10~NOT;
_LC1_B10~NOT = LCELL( _EQ303);
  _EQ303 =  A14 &  A15;

-- Node name is ':2324' from file "sprint08.tdf" line 749, column 23
-- Equation name is '_LC8_B2', type is buried 
_LC8_B2  = LCELL( _LC4_B10);

-- Node name is ':2363' from file "sprint08.tdf" line 802, column 18
-- Equation name is '_LC7_B7', type is buried 
!_LC7_B7 = _LC7_B7~NOT;
_LC7_B7~NOT = LCELL( _EQ304);
  _EQ304 =  DD6 &  DD7 & !/IOM1 & !/WR;

-- Node name is '~2463~1' from file "sprint08.tdf" line 856, column 38
-- Equation name is '~2463~1', location is LC3_A6, type is buried.
-- synthesized logic cell 
_LC3_A6  = LCELL( _EQ305);
  _EQ305 =  D0 &  D4 &  D6 &  D7;

-- Node name is '~2463~2' from file "sprint08.tdf" line 856, column 38
-- Equation name is '~2463~2', location is LC5_A15, type is buried.
-- synthesized logic cell 
_LC5_A15 = LCELL( _EQ306);
  _EQ306 =  D1 & !D2;

-- Node name is ':3452' from file "sprint08.tdf" line 1290, column 19
-- Equation name is '_LC5_B3', type is buried 
_LC5_B3  = LCELL( _EQ307);
  _EQ307 =  /IOM1
         #  /WR
         # !DCP_CX;

-- Node name is ':3466' from file "sprint08.tdf" line 1297, column 21
-- Equation name is '_LC3_B22', type is buried 
!_LC3_B22 = _LC3_B22~NOT;
_LC3_B22~NOT = LCELL( _EQ308);
  _EQ308 = !DD0 &  DD1 & !DD2;

-- Node name is ':3493' from file "sprint08.tdf" line 1303, column 39
-- Equation name is '_LC8_C15', type is buried 
_LC8_C15 = LCELL( _EQ309);
  _EQ309 = !DD0 &  DD1 &  DD2 & !D1;

-- Node name is ':3497' from file "sprint08.tdf" line 1304, column 19
-- Equation name is '_LC2_B13', type is buried 
!_LC2_B13 = _LC2_B13~NOT;
_LC2_B13~NOT = LCELL( _EQ310);
  _EQ310 = !DD0 &  DD1 &  DD2;

-- Node name is ':3505' from file "sprint08.tdf" line 1305, column 38
-- Equation name is '_LC7_C15', type is buried 
_LC7_C15 = LCELL( _EQ311);
  _EQ311 = !DD0 &  DD1 &  DD2 &  D1;

-- Node name is ':3511' from file "sprint08.tdf" line 1306, column 41
-- Equation name is '_LC7_B13', type is buried 
_LC7_B13 = LCELL( _EQ312);
  _EQ312 = !DD0 &  DD1 &  DD2 &  D2;

-- Node name is ':3513' from file "sprint08.tdf" line 1307, column 20
-- Equation name is '_LC1_B16', type is buried 
!_LC1_B16 = _LC1_B16~NOT;
_LC1_B16~NOT = LCELL( _EQ313);
  _EQ313 = !DD0 & !DD1 & !DD2;

-- Node name is ':3534' from file "sprint08.tdf" line 1308, column 50
-- Equation name is '_LC3_B6', type is buried 
_LC3_B6  = LCELL( _EQ314);
  _EQ314 =  DCP3 & !_LC6_C15
         # !_LC6_C15 & !PN5;

-- Node name is '~3551~1' from file "sprint08.tdf" line 1372, column 31
-- Equation name is '~3551~1', location is LC3_C8, type is buried.
-- synthesized logic cell 
_LC3_C8  = LCELL( _EQ315);
  _EQ315 =  A8 & !A9 &  A10 &  A11;

-- Node name is ':3551' from file "sprint08.tdf" line 1372, column 31
-- Equation name is '_LC6_C8', type is buried 
_LC6_C8  = LCELL( _EQ316);
  _EQ316 =  A12 &  A13 &  _LC3_C8 &  PN4;

-- Node name is ':3613' from file "sprint08.tdf" line 1394, column 9
-- Equation name is '_LC4_A8', type is buried 
_LC4_A8  = LCELL( _EQ317);
  _EQ317 =  DD7 &  _EC1_B & !/IO;

-- Node name is ':3622' from file "sprint08.tdf" line 1394, column 9
-- Equation name is '_LC6_C7', type is buried 
_LC6_C7  = LCELL( _EQ318);
  _EQ318 =  DD7 &  _EC5_B & !/IO;

-- Node name is ':3626' from file "sprint08.tdf" line 1399, column 5
-- Equation name is '_LC6_B3', type is buried 
_LC6_B3  = LCELL( _EQ319);
  _EQ319 =  DCP4 & !DD7 & !/IO;

-- Node name is ':3645' from file "sprint08.tdf" line 1399, column 5
-- Equation name is '_LC4_B3', type is buried 
_LC4_B3  = LCELL( _EQ320);
  _EQ320 = !DCP4 & !DD7 & !/IO;

-- Node name is ':3646' from file "sprint08.tdf" line 1406, column 13
-- Equation name is '_LC2_C23', type is buried 
_LC2_C23 = LCELL( _EQ321);
  _EQ321 =  KBD0 &  _LC4_B3;

-- Node name is ':3648' from file "sprint08.tdf" line 1406, column 13
-- Equation name is '_LC2_C20', type is buried 
_LC2_C20 = LCELL( _EQ322);
  _EQ322 =  KBD1 &  _LC4_B3;

-- Node name is ':3650' from file "sprint08.tdf" line 1406, column 13
-- Equation name is '_LC5_C24', type is buried 
_LC5_C24 = LCELL( _EQ323);
  _EQ323 =  KBD2 &  _LC4_B3;

-- Node name is ':3652' from file "sprint08.tdf" line 1406, column 13
-- Equation name is '_LC1_C4', type is buried 
_LC1_C4  = LCELL( _EQ324);
  _EQ324 =  KBD3 &  _LC4_B3;

-- Node name is ':3657' from file "sprint08.tdf" line 1406, column 13
-- Equation name is '_LC7_B2', type is buried 
_LC7_B2  = LCELL( _EQ325);
  _EQ325 = !DCP4 & !DD7 & !/IO &  TAPE_IN;

-- Node name is ':3661' from file "sprint08.tdf" line 1415, column 31
-- Equation name is '_LC5_B5', type is buried 
_LC5_B5  = LCELL( _EQ326);
  _EQ326 =  DD7
         #  DD6;

-- Node name is ':3682' from file "sprint08.tdf" line 1456, column 24
-- Equation name is '_LC5_B24', type is buried 
_LC5_B24 = LCELL( _EQ327);
  _EQ327 =  BRD4 &  CT5
         #  BRD4 &  CT4
         #  CT4 &  CT5;

-- Node name is ':3754' from file "sprint08.tdf" line 1612, column 40
-- Equation name is '_LC5_B18', type is buried 
_LC5_B18 = LCELL( _EQ328);
  _EQ328 =  AY_CCC2 &  MC_SYCLE
         #  CAS & !MC_SYCLE
         #  AY_CCC2 &  CAS
         #  E_CAS_0 & !MC_SYCLE
         #  AY_CCC2 &  E_CAS_0;

-- Node name is ':3759' from file "sprint08.tdf" line 1613, column 40
-- Equation name is '_LC4_B18', type is buried 
_LC4_B18 = LCELL( _EQ329);
  _EQ329 =  AY_CCC2 &  MC_SYCLE
         #  CAS & !MC_SYCLE
         #  AY_CCC2 &  CAS
         #  E_CAS_1 & !MC_SYCLE
         #  AY_CCC2 &  E_CAS_1;

-- Node name is ':3764' from file "sprint08.tdf" line 1614, column 40
-- Equation name is '_LC2_B8', type is buried 
_LC2_B8  = LCELL( _EQ330);
  _EQ330 =  AY_CCC2 &  MC_SYCLE
         #  CAS & !MC_SYCLE
         #  AY_CCC2 &  CAS
         #  E_CAS_2 & !MC_SYCLE
         #  AY_CCC2 &  E_CAS_2;

-- Node name is ':3769' from file "sprint08.tdf" line 1615, column 40
-- Equation name is '_LC7_B18', type is buried 
_LC7_B18 = LCELL( _EQ331);
  _EQ331 =  CAS & !MC_SYCLE
         #  E_CAS_3 & !MC_SYCLE
         #  AY_CCC2 &  MC_SYCLE
         #  AY_CCC2 &  CAS
         #  AY_CCC2 &  E_CAS_3;

-- Node name is '~3773~1' from file "sprint08.tdf" line 1617, column 29
-- Equation name is '~3773~1', location is LC4_B8, type is buried.
-- synthesized logic cell 
_LC4_B8  = LCELL( _EQ332);
  _EQ332 =  AY_CCC2 & !MC_SYCLE
         #  CAS &  MC_SYCLE
         #  AY_CCC2 &  CAS;

-- Node name is ':3773' from file "sprint08.tdf" line 1617, column 29
-- Equation name is '_LC5_B8', type is buried 
_LC5_B8  = LCELL( _EQ333);
  _EQ333 =  AY_CCC2 & !MC_SYCLE
         #  CAS &  MC_SYCLE
         #  AY_CCC2 &  CAS;

-- Node name is ':3864' from file "sprint08.tdf" line 1650, column 36
-- Equation name is '_LC4_B24', type is buried 
_LC4_B24 = LCELL( _EQ334);
  _EQ334 =  CT2 &  CT3;

-- Node name is ':4028' from file "sprint08.tdf" line 1688, column 16
-- Equation name is '_LC3_C18', type is buried 
_LC3_C18 = LCELL( _EQ335);
  _EQ335 = !CTV8
         # !_LC3_C21;

-- Node name is ':4039' from file "sprint08.tdf" line 1691, column 27
-- Equation name is '_LC3_C21', type is buried 
_LC3_C21 = LCELL( _EQ336);
  _EQ336 =  CTV3 &  CTV4 &  CTV5;

-- Node name is ':4069' from file "sprint08.tdf" line 1695, column 20
-- Equation name is '_LC3_C19', type is buried 
_LC3_C19 = LCELL( _EQ337);
  _EQ337 =  CTF0 &  CTF1;

-- Node name is '~4089~1' from file "sprint08.tdf" line 1724, column 18
-- Equation name is '~4089~1', location is LC6_C21, type is buried.
-- synthesized logic cell 
!_LC6_C21 = _LC6_C21~NOT;
_LC6_C21~NOT = LCELL( _EQ338);
  _EQ338 = !CTV3 &  CTV4 &  CTV5;

-- Node name is ':4106' from file "sprint08.tdf" line 1758, column 48
-- Equation name is '_LC7_B1', type is buried 
!_LC7_B1 = _LC7_B1~NOT;
_LC7_B1~NOT = LCELL( _EQ339);
  _EQ339 =  PN0 &  PN2 & !SC4
         # !A15;

-- Node name is '~4228~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4228~1', location is LC3_C2, type is buried.
-- synthesized logic cell 
_LC3_C2  = LCELL( _EQ340);
  _EQ340 =  AA8 & !VCM0 &  VCM1
         #  DPIC & !VCM0 & !VCM1;

-- Node name is '~4231~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4231~1', location is LC8_C19, type is buried.
-- synthesized logic cell 
_LC8_C19 = LCELL( _EQ341);
  _EQ341 =  CTF4 & !VCM0 & !VCM1
         #  AA9 & !VCM0 &  VCM1;

-- Node name is '~4234~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4234~1', location is LC6_B23, type is buried.
-- synthesized logic cell 
_LC6_B23 = LCELL( _EQ342);
  _EQ342 = !VCM0 & !VCM1
         #  AA10 & !VCM0;

-- Node name is '~4246~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4246~1', location is LC3_A18, type is buried.
-- synthesized logic cell 
_LC3_A18 = LCELL( _EQ343);
  _EQ343 =  DCOL0 & !VCM0 & !VCM1
         #  CTH0 &  VCM0;

-- Node name is '~4249~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4249~1', location is LC4_B19, type is buried.
-- synthesized logic cell 
_LC4_B19 = LCELL( _EQ344);
  _EQ344 =  DCOL1 & !VCM0 & !VCM1
         #  AA1 & !VCM0 &  VCM1;

-- Node name is '~4252~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4252~1', location is LC4_C2, type is buried.
-- synthesized logic cell 
_LC4_C2  = LCELL( _EQ345);
  _EQ345 =  DCOL2 & !VCM0 & !VCM1
         #  AA2 & !VCM0 &  VCM1;

-- Node name is '~4255~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4255~1', location is LC1_C17, type is buried.
-- synthesized logic cell 
_LC1_C17 = LCELL( _EQ346);
  _EQ346 =  DCOL3 & !VCM0 & !VCM1
         #  AA3 & !VCM0 &  VCM1;

-- Node name is '~4258~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4258~1', location is LC5_B21, type is buried.
-- synthesized logic cell 
_LC5_B21 = LCELL( _EQ347);
  _EQ347 =  DCOL4 & !VCM0 & !VCM1
         #  AA4 & !VCM0 &  VCM1;

-- Node name is '~4261~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4261~1', location is LC1_B14, type is buried.
-- synthesized logic cell 
_LC1_B14 = LCELL( _EQ348);
  _EQ348 =  DCOL5 & !VCM0 & !VCM1
         #  AA5 & !VCM0 &  VCM1;

-- Node name is '~4264~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4264~1', location is LC6_B13, type is buried.
-- synthesized logic cell 
_LC6_B13 = LCELL( _EQ349);
  _EQ349 =  DCOL6 & !VCM0 & !VCM1
         #  AA6 & !VCM0 &  VCM1;

-- Node name is '~4267~1' from file "sprint08.tdf" line 1787, column 11
-- Equation name is '~4267~1', location is LC8_C17, type is buried.
-- synthesized logic cell 
_LC8_C17 = LCELL( _EQ350);
  _EQ350 =  AA7 & !VCM0 &  VCM1
         #  DCOL7 & !VCM0 & !VCM1;

-- Node name is ':4686' from file "sprint08.tdf" line 2436, column 19
-- Equation name is '_LC4_C3', type is buried 
!_LC4_C3 = _LC4_C3~NOT;
_LC4_C3~NOT = LCELL( _EQ351);
  _EQ351 = !KB_CT0 & !KB_CT1 & !KB_CT2;

-- Node name is ':4724' from file "sprint08.tdf" line 2449, column 24
-- Equation name is '_LC2_C3', type is buried 
!_LC2_C3 = _LC2_C3~NOT;
_LC2_C3~NOT = LCELL( _EQ352);
  _EQ352 =  KB_CT0 & !KB_CT1 & !KB_CT2;

-- Node name is '~4735~1' from file "sprint08.tdf" line 2450, column 20
-- Equation name is '~4735~1', location is LC7_C1, type is buried.
-- synthesized logic cell 
_LC7_C1  = LCELL( _EQ353);
  _EQ353 = !KB_D1 & !KB_D2 &  KB_D6 &  KB_D7;

-- Node name is '~4735~2' from file "sprint08.tdf" line 2450, column 20
-- Equation name is '~4735~2', location is LC3_C1, type is buried.
-- synthesized logic cell 
_LC3_C1  = LCELL( _EQ354);
  _EQ354 = !KB_D3 & !KB_D4 &  KB_D8 &  _LC7_C1;

-- Node name is '~4777~1' from file "sprint08.tdf" line 2483, column 76
-- Equation name is '~4777~1', location is LC5_C5, type is buried.
-- synthesized logic cell 
!_LC5_C5 = _LC5_C5~NOT;
_LC5_C5~NOT = LCELL( _EQ355);
  _EQ355 = !KB_D4 & !KB_D8;

-- Node name is '~4777~2' from file "sprint08.tdf" line 2483, column 76
-- Equation name is '~4777~2', location is LC8_C5, type is buried.
-- synthesized logic cell 
_LC8_C5  = LCELL( _EQ356);
  _EQ356 =  KB_ALT &  KB_CTRL & !KB_OFF & !_LC5_C5;

-- Node name is '~6697~1' from file "sprint08.tdf" line 3108, column 23
-- Equation name is '~6697~1', location is LC6_A6, type is buried.
-- synthesized logic cell 
_LC6_A6  = LCELL( _EQ357);
  _EQ357 =  D0 &  D3;

-- Node name is ':6723' from file "sprint08.tdf" line 3125, column 14
-- Equation name is '_LC7_A4', type is buried 
_LC7_A4  = LCELL( _EQ358);
  _EQ358 = !AY_ADR3
         # !AY_ADR0
         #  AY_ADR1
         # !AY_ADR2;

-- Node name is ':6740' from file "sprint08.tdf" line 3131, column 3
-- Equation name is '_LC2_A8', type is buried 
!_LC2_A8 = _LC2_A8~NOT;
_LC2_A8~NOT = LCELL( _EQ359);
  _EQ359 = !AY_CCC0 & !AY_CCC1;

-- Node name is ':6811' from file "sprint08.tdf" line 3140, column 13
-- Equation name is '_LC6_A22', type is buried 
_LC6_A22 = LCELL( _EQ360);
  _EQ360 =  AY_CCC1 &  _EC1_A;

-- Node name is ':6813' from file "sprint08.tdf" line 3140, column 13
-- Equation name is '_LC5_A7', type is buried 
_LC5_A7  = LCELL( _EQ361);
  _EQ361 =  AY_CCC1 &  _EC7_A;

-- Node name is ':6854' from file "sprint08.tdf" line 3167, column 9
-- Equation name is '_LC7_A9', type is buried 
!_LC7_A9 = _LC7_A9~NOT;
_LC7_A9~NOT = LCELL( _EQ362);
  _EQ362 = !_LC2_A11 &  _LC5_A9
         # !AY_CX &  _LC5_A9
         # !_LC2_A11 & !_LC4_A23
         # !AY_CX & !_LC4_A23
         # !_LC4_A23 & !_LC5_A9;

-- Node name is ':6859' from file "sprint08.tdf" line 3173, column 34
-- Equation name is '_LC6_A10', type is buried 
!_LC6_A10 = _LC6_A10~NOT;
_LC6_A10~NOT = LCELL( _EQ363);
  _EQ363 = !_EC1_A &  _LC5_A10;

-- Node name is ':6875' from file "sprint08.tdf" line 3173, column 34
-- Equation name is '_LC3_A2', type is buried 
_LC3_A2  = LCELL( _EQ364);
  _EQ364 =  _EC3_A
         #  _EC7_A
         #  _LC6_A10;

-- Node name is ':6881' from file "sprint08.tdf" line 3173, column 34
-- Equation name is '_LC4_A2', type is buried 
!_LC4_A2 = _LC4_A2~NOT;
_LC4_A2~NOT = LCELL( _EQ365);
  _EQ365 = !_EC3_A & !_EC4_A & !_EC7_A & !_LC6_A10;

-- Node name is ':6891' from file "sprint08.tdf" line 3173, column 34
-- Equation name is '_LC3_A11', type is buried 
!_LC3_A11 = _LC3_A11~NOT;
_LC3_A11~NOT = LCELL( _EQ366);
  _EQ366 = !_EC2_A & !_EC6_A & !_LC4_A2;

-- Node name is ':6910' from file "sprint08.tdf" line 3178, column 28
-- Equation name is '_LC6_A2', type is buried 
!_LC6_A2 = _LC6_A2~NOT;
_LC6_A2~NOT = LCELL( _EQ367);
  _EQ367 = !AY_DAT3 & !AY_DAT4;

-- Node name is ':6943' from file "sprint08.tdf" line 3213, column 20
-- Equation name is '_LC6_A5', type is buried 
_LC6_A5  = LCELL( _EQ368);
  _EQ368 =  AY_AMP0 &  AY_XX0;

-- Node name is ':6959' from file "sprint08.tdf" line 3213, column 20
-- Equation name is '_LC2_A20', type is buried 
_LC2_A20 = LCELL( _EQ369);
  _EQ369 =  AY_AMP1 &  AY_XX1
         #  AY_AMP0 &  AY_XX0 &  AY_XX1
         #  AY_AMP0 &  AY_AMP1 &  AY_XX0;

-- Node name is ':6969' from file "sprint08.tdf" line 3213, column 20
-- Equation name is '_LC6_A20', type is buried 
_LC6_A20 = LCELL( _EQ370);
  _EQ370 =  AY_XX2 &  _LC2_A20
         #  AY_AMP2 &  _LC2_A20
         #  AY_AMP2 &  AY_XX2;

-- Node name is ':6979' from file "sprint08.tdf" line 3213, column 20
-- Equation name is '_LC7_A20', type is buried 
_LC7_A20 = LCELL( _EQ371);
  _EQ371 =  AY_XX3 &  _LC6_A20
         #  AY_AMP3 &  _LC6_A20
         #  AY_AMP3 &  AY_XX3;

-- Node name is ':6994' from file "sprint08.tdf" line 3243, column 38
-- Equation name is '_LC2_A23', type is buried 
_LC2_A23 = LCELL( _EQ372);
  _EQ372 =  AY_CX &  AY_VAR;

-- Node name is ':7008' from file "sprint08.tdf" line 3243, column 38
-- Equation name is '_LC6_A23', type is buried 
_LC6_A23 = LCELL( _EQ373);
  _EQ373 =  AY_CX &  AY_VAR &  AY_VA0 &  AY_VA1;

-- Node name is ':7357' from file "sprint08.tdf" line 3273, column 31
-- Equation name is '_LC5_A14', type is buried 
_LC5_A14 = LCELL( _EQ374);
  _EQ374 =  AY_CCC2 & !AY_XXM0 & !AY_XXM1
         #  AY_CCC2 &  AY_CCC3 & !AY_XXM0
         #  AY_CCC3 & !AY_XXM1;

-- Node name is ':7364' from file "sprint08.tdf" line 3273, column 31
-- Equation name is '_LC7_A14', type is buried 
_LC7_A14 = LCELL( _EQ375);
  _EQ375 = !AY_XXM2 &  _LC5_A14
         #  AY_CCC4 &  _LC5_A14
         #  AY_CCC4 & !AY_XXM2;

-- Node name is ':7371' from file "sprint08.tdf" line 3273, column 31
-- Equation name is '_LC2_A14', type is buried 
_LC2_A14 = LCELL( _EQ376);
  _EQ376 = !AY_XXM3 &  _LC7_A14
         #  AY_CCC5 &  _LC7_A14
         #  AY_CCC5 & !AY_XXM3;

-- Node name is ':7379' from file "sprint08.tdf" line 3273, column 31
-- Equation name is '_LC7_A24', type is buried 
_LC7_A24 = LCELL( _EQ377);
  _EQ377 = !AY_XXM4 &  _LC2_A14
         #  AY_CCC6 &  _LC2_A14
         #  AY_CCC6 & !AY_XXM4;

-- Node name is '~7404~1' from file "sprint08.tdf" line 3246, column 50
-- Equation name is '~7404~1', location is LC2_A9, type is buried.
-- synthesized logic cell 
_LC2_A9  = LCELL( _EQ378);
  _EQ378 =  _EC2_A &  _EC5_A & !_EC8_A;

-- Node name is '~7404~2' from file "sprint08.tdf" line 3246, column 50
-- Equation name is '~7404~2', location is LC5_A22, type is buried.
-- synthesized logic cell 
_LC5_A22 = LCELL( _EQ379);
  _EQ379 =  AY_CCC1 &  _EC3_A &  _LC2_A9;

-- Node name is '~7491~1' from file "sprint08.tdf" line 3165, column 26
-- Equation name is '~7491~1', location is LC8_A12, type is buried.
-- synthesized logic cell 
_LC8_A12 = LCELL( _EQ380);
  _EQ380 = !AY_DAT0 & !AY_DAT1 & !AY_DAT2 & !AY_DAT5;

-- Node name is ':7513' from file "sprint08.tdf" line 3157, column 67
-- Equation name is '_LC3_A9', type is buried 
_LC3_A9  = LCELL( _EQ381);
  _EQ381 = !_EC2_A
         #  AY_C;

-- Node name is '~7536~1' from file "sprint08.tdf" line 3116, column 73
-- Equation name is '~7536~1', location is LC2_A17, type is buried.
-- synthesized logic cell 
_LC2_A17 = LCELL( _EQ382);
  _EQ382 = !_EC5_A
         # !_EC2_A
         #  _EC1_A
         #  AY_F_RES;

-- Node name is '~7548~1' from file "sprint08.tdf" line 3114, column 25
-- Equation name is '~7548~1', location is LC2_B5, type is buried.
-- synthesized logic cell 
_LC2_B5  = LCELL( _EQ383);
  _EQ383 = !DD7
         #  DD6
         #  DCP3
         # !_LC1_B5;

-- Node name is '~7548~2' from file "sprint08.tdf" line 3114, column 25
-- Equation name is '~7548~2', location is LC6_C15, type is buried.
-- synthesized logic cell 
!_LC6_C15 = _LC6_C15~NOT;
_LC6_C15~NOT = LCELL( _EQ384);
  _EQ384 =  DD0 & !DD1 & !DD2;

-- Node name is '~7980~1' from file "sprint08.tdf" line 2526, column 6
-- Equation name is '~7980~1', location is LC7_C8, type is buried.
-- synthesized logic cell 
_LC7_C8  = LCELL( _EQ385);
  _EQ385 =  A10 & !KB_MA0 & !KB_MA2
         #  A14 & !KB_MA0 &  KB_MA2;

-- Node name is '~7980~2' from file "sprint08.tdf" line 2526, column 6
-- Equation name is '~7980~2', location is LC5_C12, type is buried.
-- synthesized logic cell 
_LC5_C12 = LCELL( _EQ386);
  _EQ386 =  A11 &  KB_MA0 & !KB_MA2
         #  A15 &  KB_MA0 &  KB_MA2;

-- Node name is '~7980~3' from file "sprint08.tdf" line 2526, column 6
-- Equation name is '~7980~3', location is LC1_C8, type is buried.
-- synthesized logic cell 
_LC1_C8  = LCELL( _EQ387);
  _EQ387 =  A8 & !KB_MA2
         #  A12 &  KB_MA2;

-- Node name is '~7980~4' from file "sprint08.tdf" line 2526, column 6
-- Equation name is '~7980~4', location is LC2_C8, type is buried.
-- synthesized logic cell 
_LC2_C8  = LCELL( _EQ388);
  _EQ388 =  A9 & !KB_MA2
         #  A13 &  KB_MA2;

-- Node name is '~7980~5' from file "sprint08.tdf" line 2526, column 6
-- Equation name is '~7980~5', location is LC8_C8, type is buried.
-- synthesized logic cell 
_LC8_C8  = LCELL( _EQ389);
  _EQ389 = !KB_MA0 &  _LC1_C8
         #  KB_MA0 &  _LC2_C8;

-- Node name is '~8352~1' from file "sprint08.tdf" line 1600, column 34
-- Equation name is '~8352~1', location is LC2_B18, type is buried.
-- synthesized logic cell 
_LC2_B18 = LCELL( _EQ390);
  _EQ390 =  AA11 &  /IO
         #  BLK_R;

-- Node name is ':8372' from file "sprint08.tdf" line 1554, column 69
-- Equation name is '_LC2_C13', type is buried 
!_LC2_C13 = _LC2_C13~NOT;
_LC2_C13~NOT = LCELL( _EQ391);
  _EQ391 = !/IO
         # !/MR;

-- Node name is ':8399' from file "sprint08.tdf" line 1495, column 50
-- Equation name is '_LC2_C22', type is buried 
_LC2_C22 = LCELL( _EQ392);
  _EQ392 =  CTH5 &  /M1
         #  CTH5 &  /IO;

-- Node name is ':8459' from file "sprint08.tdf" line 1415, column 66
-- Equation name is '_LC6_B8', type is buried 
!_LC6_B8 = _LC6_B8~NOT;
_LC6_B8~NOT = LCELL( _EQ393);
  _EQ393 = !BLK_R & !CAS & !MC_SYCLE;

-- Node name is ':8464' from file "sprint08.tdf" line 1378, column 25
-- Equation name is '_LC6_B4', type is buried 
!_LC6_B4 = _LC6_B4~NOT;
_LC6_B4~NOT = LCELL( _EQ394);
  _EQ394 = !/MR & !/M1;

-- Node name is ':8472' from file "sprint08.tdf" line 1274, column 27
-- Equation name is '_LC8_B21', type is buried 
!_LC8_B21 = _LC8_B21~NOT;
_LC8_B21~NOT = LCELL( _EQ395);
  _EQ395 = !BLK_R & !MC_END;

-- Node name is '~8621~1' from file "sprint08.tdf" line 859, column 58
-- Equation name is '~8621~1', location is LC1_B5, type is buried.
-- synthesized logic cell 
!_LC1_B5 = _LC1_B5~NOT;
_LC1_B5~NOT = LCELL( _EQ396);
  _EQ396 = !DCP4
         #  DCP5;

-- Node name is '~8621~2' from file "sprint08.tdf" line 859, column 58
-- Equation name is '~8621~2', location is LC1_C15, type is buried.
-- synthesized logic cell 
_LC1_C15 = LCELL( _EQ397);
  _EQ397 =  DD0 &  DD1 &  DD2;

-- Node name is '~8621~3' from file "sprint08.tdf" line 859, column 58
-- Equation name is '~8621~3', location is LC8_B5, type is buried.
-- synthesized logic cell 
_LC8_B5  = LCELL( _EQ398);
  _EQ398 =  DCP3 &  IN_OUT_CMD & !/MR & !/RD;

-- Node name is ':8648' from file "sprint08.tdf" line 809, column 30
-- Equation name is '_LC4_A16', type is buried 
_LC4_A16 = LCELL( _EQ399);
  _EQ399 =  D1 & !D2 & !D4 & !D5
         # !D1 &  D2 &  D4
         # !D1 &  D2 &  D5;

-- Node name is ':8687' from file "sprint08.tdf" line 746, column 52
-- Equation name is '_LC2_B4', type is buried 
_LC2_B4  = LCELL( _EQ400);
  _EQ400 =  /IO
         #  /RD;

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_0' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC4_B', type is memory 
_EC4_B   = MEMORY_SEGMENT( D0, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_1' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC2_B', type is memory 
_EC2_B   = MEMORY_SEGMENT( D1, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_2' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC6_B', type is memory 
_EC6_B   = MEMORY_SEGMENT( D2, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_3' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC7_B', type is memory 
_EC7_B   = MEMORY_SEGMENT( D3, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_4' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC1_B', type is memory 
_EC1_B   = MEMORY_SEGMENT( D4, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_5' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC3_B', type is memory 
_EC3_B   = MEMORY_SEGMENT( D5, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_6' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC8_B', type is memory 
_EC8_B   = MEMORY_SEGMENT( D6, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:195|altram:sram|segment0_7' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC5_B', type is memory 
_EC5_B   = MEMORY_SEGMENT( D7, GLOBAL(!TG42), VCC,!_LC7_B7, VCC, PGS0, PGS1, PGS2, PGS3, PGS4, PGS5, PGS6, PGS7, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_0' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC3_C', type is memory 
_EC3_C   = MEMORY_SEGMENT( KDX0, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_1' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC7_C', type is memory 
_EC7_C   = MEMORY_SEGMENT( KDX1, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_2' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC6_C', type is memory 
_EC6_C   = MEMORY_SEGMENT( KDX2, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_3' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC1_C', type is memory 
_EC1_C   = MEMORY_SEGMENT( KDX3, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_4' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC5_C', type is memory 
_EC5_C   = MEMORY_SEGMENT( KDX4, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_5' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC4_C', type is memory 
_EC4_C   = MEMORY_SEGMENT( KDX5, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_6' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC8_C', type is memory 
_EC8_C   = MEMORY_SEGMENT( VCC, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:291|altram:sram|segment0_7' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC2_C', type is memory 
_EC2_C   = MEMORY_SEGMENT( VCC, GLOBAL( TG42), VCC,!WR_KBD, VCC, KA8, KA9, KA10, KA11, KA12, KA13, KA14, KA15, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_0' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC1_A', type is memory 
_EC1_A   = MEMORY_SEGMENT( AY_DI0, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_1' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC7_A', type is memory 
_EC7_A   = MEMORY_SEGMENT( AY_DI1, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_2' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC3_A', type is memory 
_EC3_A   = MEMORY_SEGMENT( AY_DI2, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_3' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC4_A', type is memory 
_EC4_A   = MEMORY_SEGMENT( AY_DI3, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_4' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC6_A', type is memory 
_EC6_A   = MEMORY_SEGMENT( AY_DI4, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_5' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC2_A', type is memory 
_EC2_A   = MEMORY_SEGMENT( AY_DI5, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_6' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC5_A', type is memory 
_EC5_A   = MEMORY_SEGMENT( AY_DI6, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);

-- Node name is '|lpm_ram_dq:386|altram:sram|segment0_7' from file "altram.tdf" line 111, column 12
-- Equation name is '_EC8_A', type is memory 
_EC8_A   = MEMORY_SEGMENT( AY_DI7, GLOBAL( TG42), GLOBAL( TG42), AY_WR, VCC, AY_AX0, AY_AX1, AY_AX2, AY_AX3, AY_AX4, AY_AX5, _LC4_B17,!_LC2_A8, VCC, VCC, VCC,);



Project Information              c:\prj\sprinter\firmware\97\flex\sprint08.rpt

** COMPILATION SETTINGS & TIMES **

Processing Menu Commands
------------------------

Design Doctor                             = off

Logic Synthesis:

   Synthesis Type Used                    = Multi-Level

   Default Synthesis Style                = NORMAL

      Logic option settings in 'NORMAL' style for 'FLEX10K' family

      CARRY_CHAIN                         = ignore
      CARRY_CHAIN_LENGTH                  = 32
      CASCADE_CHAIN                       = ignore
      CASCADE_CHAIN_LENGTH                = 2
      DECOMPOSE_GATES                     = on
      DUPLICATE_LOGIC_EXTRACTION          = on
      MINIMIZATION                        = full
      MULTI_LEVEL_FACTORING               = on
      NOT_GATE_PUSH_BACK                  = on
      REDUCE_LOGIC                        = on
      REFACTORIZATION                     = on
      REGISTER_OPTIMIZATION               = on
      RESYNTHESIZE_NETWORK                = on
      SLOW_SLEW_RATE                      = off
      SUBFACTOR_EXTRACTION                = on
      IGNORE_SOFT_BUFFERS                 = on
      USE_LPM_FOR_AHDL_OPERATORS          = off

   Other logic synthesis settings:

      Automatic Global Clock              = on
      Automatic Global Clear              = on
      Automatic Global Preset             = on
      Automatic Global Output Enable      = on
      Automatic Fast I/O                  = off
      Automatic Register Packing          = off
      Automatic Open-Drain Pins           = on
      Automatic Implement in EAB          = off
      Optimize                            = 5

Default Timing Specifications: None

Cut All Bidir Feedback Timing Paths       = on
Cut All Clear & Preset Timing Paths       = on

Ignore Timing Assignments                 = off

Functional SNF Extractor                  = off

Linked SNF Extractor                      = off
Timing SNF Extractor                      = on
Optimize Timing SNF                       = off
Generate AHDL TDO File                    = off
Fitter Settings                           = NORMAL
Use Quartus Fitter                        = on
Smart Recompile                           = off
Total Recompile                           = off

Interfaces Menu Commands
------------------------

EDIF Netlist Writer                       = off
Verilog Netlist Writer                    = off
VHDL Netlist Writer                       = off

Compilation Times
-----------------

   Compiler Netlist Extractor             00:00:01
   Database Builder                       00:00:00
   Logic Synthesizer                      00:00:00
   Partitioner                            00:00:00
   Fitter                                 00:00:01
   Timing SNF Extractor                   00:00:01
   Assembler                              00:00:00
   --------------------------             --------
   Total Time                             00:00:03


Memory Allocated
-----------------

Peak memory allocated during compilation  = 19,110K
